|  |
| --- |
|  |
| **Title\*:** | SOL005ed451 Bug008200 Correct the typo of UploadVnfPkgFromUriRequest in table 9.4.6.3.1-2 |
|  |  |
| from **Source**\*: | DOCOMO Communications Lab. |
| Contact: | Yinan Liu, Yuya Kuno, Bertrand Souville |
|  |  |
| input for **Committee**\***:** | NFV SOL |
|  |  |
| Contribution **For\*:** | Decision | **X** |  |
|  | Discussion |  |  |
|  | Information |  |  |
|  |  |
| Submission date**\***: | 2023-06-03 |
|  |  |
| Meeting & Allocation: | **NFVSOL#248-at NFV#42** -  |
| Relevant WI(s), or deliverable(s): |  RGS/NFV-SOL005ed451 |
|  |

**Decision requested:** Please approve

**ABSTRACT:** *This contribution is to fix the bug 008200(*[*http://oldforge.etsi.org/mantis/view.php?id=8200*](http://oldforge.etsi.org/mantis/view.php?id=8200)*) to correct the typo of UploadVnfPkgFromUriRequest which should be UploadVnfPackageFromUriRequest defined in clause 9.5.2.4.*

|  |
| --- |
| **CHANGE REQUEST** |
| **NFV-SOL005** | **Version**  | **4.4.2** | **CR** | **CR(23)193**  | **rev**  | - |
|  |
| ***CR Title:*** | SOL005ed451 Bug008200 Correct the typo of UploadVnfPkgFromUriRequest in table 9.4.6.3.1-2 |
|  |
| ***Source:*** | DOCOMO Communications Lab. |
|  |
| ***Work Item Ref:*** | RGS/NFV-SOL005ed451 | ***Date:*** | 03/06/2023 |
|  |
| ***Category:*** | D | ***Release:*** | 4 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(corresponds to a correction in an earlier release)****B*** *(addition of feature)****C*** *(functional modification of feature)****D*** *(editorial modification)* |
|  |
| ***Reason for change:*** | See ETSI bug tracker [*http://oldforge.etsi.org/mantis/view.php?id=8200*](http://oldforge.etsi.org/mantis/view.php?id=8200)*.* |
|  |
| ***Summary of change:*** | Replacing UploadVnfPkgFromUriRequest by UploadVnfPackageFromUriRequest in table 9.4.6.3.1-2. |
|  |
| ***Clauses affected:*** | Clause 9.4.6.3.1 |
|  |
| ***Other deliverables*** ***affected:*** |  |
|  |
| ***Other comments:*** | \*\*\* Analysis of backward compatibility changes \*\*\** Change Type: BWC
* Change Type Code: BWC\_OTHER
 |

\*\*\* START OF CHANGES \*\*\*

|  |
| --- |
| **Change #1** |

Table 9.4.6.3.1-2: Details of the POST request/response on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Request body | Data type | Cardinality | Description |
| UploadVnfPackageFromUriRequest | 1 | The message content contains the address information based on which the NFVO can obtain the content of the VNF package. |
| Response body | Data type | Cardinality | ResponseCodes | Description |
| n/a |  | 202 Accepted | Shall be returned when the information about the VNF package has been received successfully, but the on-boarding has not been completed. It is expected to take some time for processing.The response body shall be empty. See note. |
| ProblemDetails | 1 | 409 Conflict | Shall be returned upon the following error: The operation cannot be executed currently, due to a conflict with the state of the resource.Typically, this is due to the fact that the on-boarding state of the VNF package resource is not "CREATED" or "ERROR".The response body shall contain a ProblemDetails structure, in which the "detail" attribute shall convey more information about the error. |
| ProblemDetails | See clause 6.4 of [16] | 4xx/5xx | In addition to the response codes defined above, any common error response code as defined in clause 6.4 of ETSI GS NFV-SOL 013 [16] may be returned. |
| NOTE: The API consumer can track the uploading progress by receiving the "VnfPackageOnBoardingNotification" from the NFVO or by reading the status of the individual on-boarded VNF package resource using the GET method. |

\*\*\* END OF CHANGES \*\*\*