/**
 *    @author   ETSI STF517
 *    @version  $URL$
 *              $Id$
 *    @desc     MAPEM TP functions
 *
 */

module ItsMapem_TpFunctions {
    
    // LibCommon
    import from LibCommon_BasicTypesAndValues all;
    import from LibCommon_Sync all;
    import from LibCommon_VerdictControl all;
    import from LibCommon_Time all;
    
    // LibItsCommon
    import from LibItsCommon_Functions all;
    import from LibItsCommon_TypesAndValues all;
    
    // LibIts
    import from ITS_Container language "ASN.1:1997" all;
    import from MAPEM_PDU_Descriptions language "ASN.1:1997" all;
    import from SPATEM_PDU_Descriptions language "ASN.1:1997" all;
    import from DSRC language "ASN.1:1997" all;
    
    // LibItsMapemSpatem
    import from LibItsMapemSpatem_TestSystem all;
    import from LibItsMapemSpatem_Functions all;
    import from LibItsMapemSpatem_Templates all;
    import from LibItsMapemSpatem_TypesAndValues all;
    import from LibItsMapemSpatem_Pics all;
    
    group mapeMessageDissemination { 
        
        group mapeMessageFormat { 
            
            /**
             * @desc    TP Function for TC_IS_RLT_MSGF_BV_01
             */
            function f_IS_RLT_MSGF_BV_01 () runs on ItsMapemSpatem {
                
                // Local variables
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu
                    )) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Successfully received MAPEM PDU header. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_MSGF_BV_01
            
        } // End of group mapeMessageFormat
        
        group mapeEventGeneration { 
            
            /**
             * @desc    TP Function for TC_IS_RLT_EVGN_BV_01
             */
            function f_IS_RLT_EVGN_BV_01 () runs on ItsMapemSpatem {
                
                // Local variables
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Successfully received MAPEM. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_defaultMapem
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: Received a MAPEM with incorrect information. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_EVGN_BV_01
            
            /**
             * @desc    TP Function for TC_IS_RLT_EVGN_BV_02
             */
            function f_IS_RLT_EVGN_BV_02 () runs on ItsMapemSpatem {
                
                // Local variables
                var MapemInd v_mapem;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_awaitMapeMessage(
                    mw_mapemInd(
                        mw_mapemPdu(
                            mw_defaultMapem
                    )),
                    v_mapem
                );
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                f_utTriggerEvent(m_utTriggerEvent(mapemNewContent));
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(v_mapem) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: The same MAPEM was received. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_error);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Successfully received a new MAPEM. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_defaultMapem
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: Received a MAPEM with incorrect information. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_EVGN_BV_02
            
            /**
             * @desc    TP Function for TC_IS_RLT_EVGN_BV_03
             */
            function f_IS_RLT_EVGN_BV_03 () runs on ItsMapemSpatem {
                
                // Local variables
                var MapemInd v_mapem;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_awaitMapeMessage(
                    mw_mapemInd(
                        mw_mapemPdu(
                            mw_defaultMapem
                    )),
                    v_mapem
                );
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                f_utTriggerEvent(m_utTriggerEvent(mapemNewContentWithFragmentation));
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemLayerType
                    ))) -> value v_mapem { 
                        log("*** " & testcasename() & ": INFO: Successfully received the first fragment of MAPEM. ***");
                        repeat;
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemLayerType(
                                                  v_mapem.msgIn.map_.layerID + 1
                                )
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Successfully received the last fragment of MAPEM. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_defaultMapem
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: Received a MAPEM with incorrect information. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_EVGN_BV_03
            
        } // End of group mapeEventGeneration
        
        group mapeCommunication {
            
            /**
             * @desc    TP Function for TC_IS_RLT_COMM_BV_01
             */
            function f_IS_RLT_COMM_BV_01 () runs on ItsMapemSpatem {
                
                // Local variables
                var boolean v_tlmServiceStarted := false;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_SPATEM_GENERATION or not PICS_SPATEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION and PICS_SPATEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                tc_ac.start;
                alt {
                    [v_tlmServiceStarted == false] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": INFO: Successfully received well-formed MAPEM. ***");
                        f_utTriggerEvent(m_utTriggerEvent(startTLMService));
                        v_tlmServiceStarted := true;
                        tc_ac.start;
                        repeat;
                    }
                    [] mapemSpatemPort.receive(
                        mw_spatemInd(
                            mw_spatemPdu(
                                mw_spatemWellFormatted
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Successfully received well-formed MAPEM & SPATEM. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_utTriggerEvent(m_utTriggerEvent(stopTLMService));
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_COMM_BV_01
            
            /**
             * @desc    TP Function for TC_IS_RLT_COMM_BV_02_01
             */
            function f_IS_RLT_COMM_BV_02_01 () runs on ItsMapemSpatem {
                
                // Local variables
                const UInt8 c_gnNhBtpB := 2;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                
                // Test Body
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemIndWithGnParameters(
                           mw_mapemPdu(
                               mw_mapemWellFormatted
                           ), 
                           c_gnNhBtpB
                    )) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Expected MAPEM encapsultated in BTP-B packet received. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(mw_mapemIndWithGnParameters(mw_mapemPdu(mw_mapemWellFormatted), omit)) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": INCONC: no GN NH information in MapemInd ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);  
                    }                    
                    [] mapemSpatemPort.receive(mw_mapemInd(mw_mapemPdu(mw_defaultMapem))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: Expected MAPEM received, but not encapsulated in BTP-B packet ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_error);  
                    }                    
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_COMM_BV_02_01
            
            /**
             * @desc    TP Function for TC_IS_RLT_COMM_BV_02_02
             */
            function f_IS_RLT_COMM_BV_02_02 () runs on ItsMapemSpatem {
                
                // Local variables
                const UInt16 c_gnNhBtpBPort := 2003;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                
                // Test Body
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemIndWithBtpParameters(
                           mw_mapemPdu, 
                           c_gnNhBtpBPort,
                           0
                    )) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Expected MAPEM encapsultated in BTP packet with port value 2003 received. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(mw_mapemInd(mw_mapemPdu(mw_defaultMapem))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: Expected MAPEM received, but not addressed to the correct destination port. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_error);  
                    }                    
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_COMM_BV_02_02
            
            /**
             * @desc    TP Function for TC_IS_RLT_COMM_BV_03
             */
            function f_IS_RLT_COMM_BV_03 () runs on ItsMapemSpatem {
                
                // Local variables
                const UInt8 c_gnHtGbc := 4;
                
                // Test control
                if (not PICS_RSU_ROLE or not PICS_MAPEM_GENERATION) {
                    log("*** " & testcasename() & ": PICS_RSU_ROLE and PICS_MAPEM_GENERATION required for executing the TC ***");
                    setverdict(inconc);
                    stop;
                }
                
                // Test component configuration
                f_cfUp();
                    
                // Preamble
                f_prInitialState();
                f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                    
                // Test Body
                tc_ac.start;
                alt {
                    [] mapemSpatemPort.receive(
                        mw_mapemIndWithGnParameters(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                            ),
                            -, 
                            c_gnHtGbc
                    )) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": PASS: Expected MAPEM encapsulated in GBC packet received. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemIndWithGnParameters(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                            ),
                            -, 
                            omit
                    )) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL: no GN HT information in MapemInd. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_error);
                    }
                    [] mapemSpatemPort.receive(
                        mw_mapemInd(
                            mw_mapemPdu(
                                mw_mapemWellFormatted
                    ))) { 
                        tc_ac.stop;
                        log("*** " & testcasename() & ": FAIL:  Expected MAPEM received, but not encapsulated in GBC packet. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_error);
                    }
                    [] tc_ac.timeout {
                        log("*** " & testcasename() & ": INCONC: Timeout while awaiting the reception of a message. ***");
                        f_selfOrClientSyncAndVerdict(c_tbDone, e_timeout);
                    }
                }
                
                // Postamble
                f_poDefault();
                f_cfDown();
                
            } // End of function f_IS_RLT_COMM_BV_03
            
        } // End of group mapeCommunication 
        
    } // End of group mapeMessageDissemination
    
    group mapeMessageProcessing {
        
        /**
         * @desc    TP Function for TC_IS_RLT_MSGF_BV_02
         */
        function f_IS_RLT_MSGF_BV_02 () runs on ItsMapemSpatem {
            
            // Local variables
            var MapemReq   v_mapemReq;
            var integer     i;
                
            if (PICS_RSU_ROLE or not PICS_MAPEM_RECEPTION) {
                log("*** " & testcasename() & ": not PICS_RSU_ROLE and PICS_MAPEM_RECEPTION required for executing the TC ***");
                setverdict(inconc);
                stop;
            }
                
            // Test component configuration
            f_cfUp();
                
            // Preamble
            f_prInitialState();
            f_selfOrClientSyncAndVerdictPreamble(c_prDone, e_success);
                
            // Test Body
            v_mapemReq := valueof(m_mapemReq(m_mapemPdu(m_defaultMapem)));
            mapemSpatemPort.send(v_mapemReq) ;
                
            f_sleep(PX_TAC);
            for (i := 0; i < lengthof(vc_utMapemEvents) and not match (v_mapemReq.msgOut , vc_utMapemEvents[i].mapeMsg); i := i + 1) {
                // empty on purpose 
            }
            if (i < lengthof(vc_utMapemEvents) ) {
                log("*** " & testcasename() & ": PASS: MAPEM was transmitted to upper layer ***");
                f_selfOrClientSyncAndVerdict(c_tbDone, e_success);
            } else {
                log("*** " & testcasename() & ": FAIL: MAPEM was not transmitted to upper layer ***");
                f_selfOrClientSyncAndVerdict(c_tbDone, e_error);
            }
                
            // Postamble
            f_poDefault();
            f_cfDown();
                
        } // End of function f_IS_RLT_MSGF_BV_02
        
    } // End of group mapeMessageProcessing
    
} // End of module ItsMapem_TpFunctions 