module ItsRSUsSimulator_Functions {
    
    // LibCommon
    import from LibCommon_BasicTypesAndValues all;
    import from LibCommon_DataStrings all;
    import from LibCommon_VerdictControl all;
    import from LibCommon_Sync all;
    import from LibCommon_Time all;
    
    // LibIts
    import from ITS_Container language "ASN.1:1997" all;
    import from CAM_PDU_Descriptions language "ASN.1:1997" all;
    import from DENM_PDU_Descriptions language "ASN.1:1997" all;
    import from MAPEM_PDU_Descriptions language "ASN.1:1997" all;
    import from SPATEM_PDU_Descriptions language "ASN.1:1997" all;
    import from IVIM_PDU_Descriptions language "ASN.1:1997" all;
    import from SREM_PDU_Descriptions language "ASN.1:1997" all;
    import from SSEM_PDU_Descriptions language "ASN.1:1997" all;
    import from DSRC language "ASN.1:1997" all;
    
    // LibItsCommon
    import from LibItsCommon_Functions all;
    
    // LibItsBtp
    import from LibItsBtp_TypesAndValues all;
    import from LibItsBtp_Templates all;
    
    // LibItsCam
    import from LibItsCam_Templates all;
    
    // LibItsDenm
    import from LibItsDenm_Templates all;
    
    // LibItsMapemSpatemm
    import from LibItsMapemSpatem_Templates all;
    
    // LibItsMapemSpatemm
    import from LibItsIvim_Templates all;
    
    // LibItsMapemSpatemm
    import from LibItsSremSsem_Templates all;
    
    // LibItsGeoNetworking
    import from LibItsGeoNetworking_TestSystem all;
    import from LibItsGeoNetworking_Functions all;
    import from LibItsGeoNetworking_Templates all;
    import from LibItsGeoNetworking_TypesAndValues all;
    import from LibItsGeoNetworking_Pixits all;
    
    // LibItsSecurity
    import from LibItsSecurity_TypesAndValues all;
    import from LibItsSecurity_Functions all;
    
    // AtsRSUsSimulator
    import from ItsRSUsSimulator_TypesAndValues all;
    import from ItsRSUsSimulator_TestSystem all;
    import from ItsRSUsSimulator_Templates all;
    import from ItsRSUsSimulator_Pics all;
    import from ItsRSUsSimulator_Pixits all;
    
    group externalFunctions {
        
        external function fx_computePositionFromRotation(
                                                         in Int32 p_refLatitude, 
                                                         in Int32 p_refLongitude, 
                                                         in Int32 p_cenLatitude, 
                                                         in Int32 p_cenLongitude, 
                                                         in float p_rotation, 
                                                         out Int32 p_latitude,
                                                         out Int32 p_longitude
        );
        
    } // End of group externalFunctions
    
    group rsuConfigurationFunctions {
        
        /**
         * @desc This configuration features:
         *       - one ITS node (IUT)
         *       - two ITS nodes (nodeA, nodeB)
         *       - Area1 which only includes NodeB and IUT
         *       - Area2 which only includes NodeB
         *         NodeB being close to the area center
         */
        function f_cf01Up() runs on ItsRSUsSimulator {
            
            // Local variables
            
            // Map
            map(self:acPort, system:acPort);
            map(self:cfPort, system:cfPort);
            map(self:geoNetworkingPort, system:geoNetworkingPort);
            
            // Connect
            f_connect4SelfOrClientSync();
            activate(a_cf01Down());
            
            // Initialise secured mode
            f_initialiseSecuredMode();
            
            //Initialze the Config module
            cfPort.send(CfInitialize:{});
            
            // Initialisations
            f_setup_rsu(vc_rsu_id);
             
        } // End of function f_cf01Up
        
        function f_cf01Down() runs on ItsRSUsSimulator {
            
            vc_rsuMessagesValueList := {};
            
            f_uninitialiseSecuredMode();
            
            // Unmap
            unmap(self:acPort, system:acPort);
            unmap(self:cfPort, system:cfPort);
            unmap(self:geoNetworkingPort, system:geoNetworkingPort);
            
            // Disconnect
            f_disconnect4SelfOrClientSync();
            
        } // End of function f_cf01Down
        
    } // End of group rsuConfigurationFunctions
    
    group usecase6 {
        
        function f_initialiseVehicleSimulatorComponent(
                                                       in ItsRSUsSimulator p_component,
                                                       out template (omit) CAM p_cam
        ) runs on ItsRSUsSimulator { 
            p_cam := 
                m_camMsg_vehicle(
                    f_getTsStationId(),
                    f_getCurrentTime() mod 65536,    // Shall be updated in function f_prepare_vehicle_cam
                    m_rsuPosition(
                        0,                           // Shall be computed
                        0                            // Shall be computed
                    )
            );
            map(p_component:geoNetworkingPort, system:geoNetworkingPort);
        } // End of function f_initialiseVehicleSimulatorComponent
        
        function f_uninitialiseVehicleSimulatorComponent(
                                                         in ItsRSUsSimulator p_component
        ) runs on ItsRSUsSimulator { 
            p_component.done;
            unmap(p_component:geoNetworkingPort, system:geoNetworkingPort);
        } // End of function f_uninitialiseVehicleSimulatorComponent
        
    } // End of group usecase6 
    
    function f_setup_rsu(
                         in integer p_rsu_id
    ) runs on ItsRSUsSimulator { 
        
        // Local variables
        var template (value) DenmParmContainers v_denmParmContainers;
        var template (omit) octetstring v_beacon := omit;
        var template (omit) DENMs v_denms := omit;
        var template (omit) CAM v_cam := omit;
        var template (omit) MAPEM v_mapem := omit;
        var template (omit) SPATEMs v_spatems := omit;
        var template (omit) IVIM v_ivim := omit;
        var template (omit) SSEM v_ssem := omit;
        var integer v_counter;
        
        vc_longPosVectorRsu := PICS_RSU_PARAMS[p_rsu_id].longPosVector;
        // MAPEM, only if PX_ETSI_USE_CASE_ID is set to 3
        if ((vc_mapem == true) and (PX_ETSI_USE_CASE_ID == 3) and ispresent(PICS_MAPEM_PARMS_RSUs[p_rsu_id].intersections)) {
            // Build the list of the MAPEM events
            v_mapem := 
                m_mapemParm(
                    PICS_RSU_PARAMS[vc_rsu_id].stationID,
                    m_mapem(
                        f_getMsgIssueRevision(),
                        PICS_MAPEM_PARMS_RSUs[p_rsu_id].intersections,
                        PICS_MAPEM_PARMS_RSUs[p_rsu_id].roadSegments
            ));
            // Update revision fields
            v_mapem.map_.intersections[0].revision := f_incMsgIssueRevision();
            // TODO Add more?
        } else {
            vc_mapem := false;
        }
        // SPATEM, only if PX_ETSI_USE_CASE_ID is set to 3
        if ((vc_spatem == true) and (PX_ETSI_USE_CASE_ID == 3) and (lengthof(PICS_SPATEM_PARMS_RSUs[p_rsu_id]) != 0)) {
            // Reset counter
            vc_currentPhaseStartTime := 36001;
            vc_endPhaseStartTime := 0;
            vc_spatemStatesId := 0;
            // Build the list of the SPATEM events
            for (v_counter := 0; v_counter < lengthof(PICS_SPATEM_PARMS_RSUs[p_rsu_id]); v_counter := v_counter + 1) {
                v_spatems[v_counter] := 
                    m_spatemParm(
                        PICS_RSU_PARAMS[p_rsu_id].stationID,
                        m_spatem(
                            PICS_SPATEM_PARMS_RSUs[p_rsu_id][v_counter].intersections,
                            "SignalGroupID #" & int2str(PICS_SPATEM_PARMS_RSUs[p_rsu_id][v_counter].signalGroupID)
                ));
                for (var integer v_intersection := 0; v_intersection < lengthof(v_spatems[v_counter].spat.intersections); v_intersection := v_intersection + 1) {
                    vc_states[v_counter][v_intersection] := v_spatems[v_counter].spat.intersections[v_intersection].states;
                } // End of 'for' statement
                // TODO Build SPATEM with dynamic values
            } // End of 'for' statement
            // TODO Build SPATEM with dynamic values
        } else {
            vc_spatem := false;
        }
        // IVIM, only if PX_ETSI_USE_CASE_ID is set to 5
        if ((vc_ivim == true) and (PX_ETSI_USE_CASE_ID == 5) and ispresent(PICS_IVIM_PARMS_RSUs[p_rsu_id].provider)) {
            // Build the list of the IVIM events
            v_ivim := 
                m_ivimParm(
                    PICS_RSU_PARAMS[p_rsu_id].stationID,
                    m_ivimStructure(
                        m_iviManagementContainer(
                            PICS_IVIM_PARMS_RSUs[p_rsu_id].provider,
                            PICS_IVIM_PARMS_RSUs[p_rsu_id].iviIdentificationNumber,
                            0//IviStatus_new_
                        ),
                        PICS_IVIM_PARMS_RSUs[p_rsu_id].iviContainers
            ));
            // Update ivi status
            v_ivim.ivi.mandatory.validFrom := f_getCurrentTime();
            v_ivim.ivi.mandatory.validTo := valueof(v_ivim.ivi.mandatory.validFrom) + 43200000; // 12hours
        } else {
            vc_ivim := false;
        }
        // DENM, only if PX_ETSI_USE_CASE_ID is set to 1
        if ((vc_denm == true) and (PX_ETSI_USE_CASE_ID == 1)) {
            // Build the list of the DENM events for the specified RSU (PX_RSU_ID) and the given zone (PX_ETSI_ZONE_ID)
            for (v_counter := 0; v_counter < lengthof(PICS_DENM_EVENTS_RSU[p_rsu_id][PX_ETSI_ZONE_ID - 1]); v_counter := v_counter + 1) {
                var DenmEventsParmsPerZone v_denmEventsParmsPerZone := PICS_DENM_EVENTS_RSU[p_rsu_id][PX_ETSI_ZONE_ID - 1];
                
                v_denmParmContainers := m_denmParmContainers(
                    PICS_RSU_PARAMS[p_rsu_id].stationID,
                    f_incDenmSequenceNumber(),
                    PICS_DENM_REPETITION_INTERVAL,
                    v_denmEventsParmsPerZone[v_counter].eventPosition,
                    v_denmEventsParmsPerZone[v_counter].causeCodeType,
                    v_denmEventsParmsPerZone[v_counter].eventHistory,
                    v_denmEventsParmsPerZone[v_counter].traces,
                    PICS_DENM_VALIDITY_DURATION,
                    PICS_DENM_RELEVANCE_DISTANCE,
                    PICS_DENM_RELEVANCE_TRAFFIC_DIRECTION
                );
                v_denms[v_counter] := valueof(
                    m_denmPdu_rsu(
                        PICS_RSU_PARAMS[p_rsu_id].stationID,
                        m_denm(
                               v_denmParmContainers.managementContainer, 
                               v_denmParmContainers.situationContainer,
                               v_denmParmContainers.locationContainer
                )));
                if (ispresent(v_denmEventsParmsPerZone[v_counter].roadWorksContainerExtended)) {
                    v_denms[v_counter].denm.alacarte := m_alacarte(v_denmEventsParmsPerZone[v_counter].roadWorksContainerExtended);
                }
            } // End of 'for' statement
            // Update referenceDenms field, all except the current one
            for (v_counter := 0; v_counter < lengthof(PICS_DENM_EVENTS_RSU[p_rsu_id][PX_ETSI_ZONE_ID - 1]); v_counter := v_counter + 1) {
                if (ispresent(v_denms[v_counter].denm.alacarte.roadWorks)) {
                    var integer v_referenceDenms := 0;
                    for (var integer v_counter1 := 0; v_counter1 < lengthof(PICS_DENM_EVENTS_RSU[p_rsu_id][PX_ETSI_ZONE_ID - 1]); v_counter1 := v_counter1 + 1) {
                        if (v_counter1 == v_counter) {
                            continue;
                        }
                        v_denms[v_counter].denm.alacarte.roadWorks.referenceDenms[v_referenceDenms] := v_denms[v_counter1].denm.management.actionID;
                        v_referenceDenms := v_referenceDenms + 1;
                    } // End of 'for' statement
                }
            } // End of 'for' statement
        } else {
            vc_denm := false;
        }
        // CAM
        if (vc_cam == true) {
            // Build the list of the CAM events
            if (PX_ETSI_USE_CASE_ID == 7) {
                vc_longPosVectorRsu := PICS_UC7_LPV.longPosVector;
                v_cam := 
                    m_camParm(
                        PICS_UC7_LPV.stationID,
                        PICS_UC7_LPV.stationType,
                        PICS_UC7_LPV.vehicleRole, 
                        m_rsuPosition(
                            PICS_UC7_LPV.longPosVector.latitude,
                            PICS_UC7_LPV.longPosVector.longitude
                        ), 
                        PICS_UC7_LPV.pathHistory,
                        {
                            rsuContainerHighFrequency := {
                                protectedCommunicationZonesRSU := omit
                            }
                        }
                );
            } else if (PX_ETSI_USE_CASE_ID == 9) {
                v_cam := 
                    m_camParm(
                        PICS_RSU_PARAMS[p_rsu_id].stationID,
                        -,
                        -,
                        m_rsuPosition(
                            vc_longPosVectorRsu.latitude,
                            vc_longPosVectorRsu.longitude
                        ), 
                        PICS_RSU_PARAMS[p_rsu_id].pathHistory,
                        m_highFrequencyContainer_rsuContainerHighFrequency(
                            m_rSUContainerHighFrequency(
                                PICS_USECASE9_PCZ
                )));
            } else {
                v_cam := 
                    m_camParm(
                        PICS_RSU_PARAMS[p_rsu_id].stationID,
                        -,
                        -,
                        m_rsuPosition(
                            vc_longPosVectorRsu.latitude,
                            vc_longPosVectorRsu.longitude
                        ), 
                        PICS_RSU_PARAMS[p_rsu_id].pathHistory,
                        {
                            rsuContainerHighFrequency := {
                                protectedCommunicationZonesRSU := omit
                            }
                        }
                );
            }
        } 
        if (vc_beacon == true) {
            // Build the list of the BeACON events
            v_beacon := 'AAAAAAAA'O; // TODO Use a PICS
        } 
        // Build the messages value list for this RSU
        vc_rsuMessagesValueList[p_rsu_id] := 
            m_rsuProfile(
                v_beacon,
                v_cam, 
                v_denms,
                v_mapem,
                v_spatems,
                v_ivim,
                v_ssem
        );
        if (PICS_RSU_PARAMS[p_rsu_id].geoShape == e_geoCircle) {
            vc_geoArea := {
                shape := e_geoCircle,
                area := {
                    geoAreaPosLatitude := vc_longPosVectorRsu.latitude,
                    geoAreaPosLongitude := vc_longPosVectorRsu.longitude,
                    distanceA := PICS_RSU_PARAMS[p_rsu_id].geoParms.radius,
                    distanceB := PICS_RSU_PARAMS[p_rsu_id].geoParms.radius,
                    angle := 0
                }
            }
        } else {
            log("*** " & testcasename() & ": INCONC: Wrong PICS_RSU_GEOAREA_FORM event initialisation ***");
            setverdict(inconc);
            stop;
        }
        
    } // End of function f_setup_rsu
    
    function f_process_cf_event(
                                in CfEvent p_cfEvent
    ) runs on ItsRSUsSimulator return boolean {
        var template (value) CfResult v_result := true;
        
        // Terminate simulation
        if (p_cfEvent == "stop") {
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].beacon)) {
                tc_beacon.stop;
            }
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].cam)) {
                tc_cam.stop;
            }
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].denms)) {
                tc_denm.stop;
            }
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].mapem)) {
                tc_mapem.stop;
            }
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].spatems)) {
                tc_spatem.stop;
            }
            if (ispresent(vc_rsuMessagesValueList[vc_rsu_id].ivim)) {
                tc_ivim.stop;
            }
        } else {
            v_result := false;
        }
        
        cfPort.send(v_result);
        
        return false;
    } // End of function f_process_cf_event
    
    function f_prepare_beacon(
                              out template (value) Payload p_payload
    ) runs on ItsRSUsSimulator {
        
        p_payload := valueof(
            f_adaptPayload(
                vc_rsuMessagesValueList[vc_rsu_id].beacon,
                0,
                -,
                e_any
            )
        );
    } // End of function f_prepare_beacon
    
    function f_prepare_cam(
                           out template (value) Payload p_payload
    ) runs on ItsRSUsSimulator {
        
        vc_rsuMessagesValueList[vc_rsu_id].cam.cam.generationDeltaTime := f_getCurrentTime() mod 65536; // See ETSI EN 302 637-2 V1.3.0 - Clause B.3 generationDelatTime
        p_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(
                            vc_rsuMessagesValueList[vc_rsu_id].cam
                ))),
                PICS_CAM_BTP_DESTINATION_PORT,
                PICS_CAM_BTP_SOURCE_PORT
            )
        );
    } // End of function f_prepare_cam
    
    function f_prepare_denm(
                            out template (value) Payload p_payload,
                            in boolean p_cancellation := false
    ) runs on ItsRSUsSimulator {
        
        // Update dynamic parms
        vc_rsuMessagesValueList[vc_rsu_id].denms[vc_denmEventCounter].denm.management.referenceTime  := f_getCurrentTime();
        if (p_cancellation == true) {
            vc_rsuMessagesValueList[vc_rsu_id].denms[vc_denmEventCounter].denm.management.termination := isCancellation;
        }
        p_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(vc_rsuMessagesValueList[vc_rsu_id].denms[vc_denmEventCounter]
                ))),
                PICS_DENM_BTP_DESTINATION_PORT,
                PICS_DENM_BTP_SOURCE_PORT
            )
        ); 
        vc_denmEventCounter := (vc_denmEventCounter + 1) mod lengthof(vc_rsuMessagesValueList[vc_rsu_id].denms);
    } // End of function f_prepare_denm
    
    function f_prepare_mapem(
                             out template (value) Payload p_payload
    ) runs on ItsRSUsSimulator {
        
        p_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(
                            vc_rsuMessagesValueList[vc_rsu_id].mapem
                ))),
                PICS_MAPEM_BTP_DESTINATION_PORT,
                PICS_MAPEM_BTP_SOURCE_PORT
            )
        );
    } // End of function f_prepare_mapem
    
    function f_computeEndPhaseStartTime(
                               in TimeMark p_timeMark,
                               in UInt32 p_inc
    ) return TimeMark {
        var UInt32 v_endPhaseStartTime := p_timeMark + p_inc;
        return v_endPhaseStartTime mod 36000;
    }
    
    function f_prepare_spatem(
                              in template (value) SPATEM p_spatem,
                              out template (value) Payload p_payload
    ) runs on ItsRSUsSimulator {
        var template (omit) SPATEM v_spatem := p_spatem; // Make a copy
        var TimeMark v_currentTimeMark := f_getCurrentTimeMark();
        
        if (vc_currentPhaseStartTime == 36001) {
            vc_currentPhaseStartTime := v_currentTimeMark;
            vc_endPhaseStartTime := f_computeEndPhaseStartTime(vc_currentPhaseStartTime, vc_repitition_duration[vc_spatemStatesId]);
        }
        if (v_currentTimeMark >= vc_endPhaseStartTime) {
            vc_spatemStatesId := (vc_spatemStatesId + 1) mod vc_spatemStatesNum; // Change state
            vc_currentPhaseStartTime := v_currentTimeMark;
            vc_endPhaseStartTime := f_computeEndPhaseStartTime(vc_currentPhaseStartTime, vc_repitition_duration[vc_spatemStatesId]);
        }
        log("vc_currentPhaseStartTime = ", vc_currentPhaseStartTime);
        log("vc_endPhaseStartTime = ", vc_endPhaseStartTime);
        log("v_currentTimeMark = ", v_currentTimeMark);
        log("vc_spatemStatesId = ", vc_spatemStatesId);
        log("mintime#1 = ", vc_currentPhaseStartTime + vc_repitition_duration[(vc_spatemStatesId + 1) mod vc_spatemStatesNum]);
        log("mintime#2 = ", vc_currentPhaseStartTime + vc_repitition_duration[(vc_spatemStatesId + 2) mod vc_spatemStatesNum]);
        // Rebuild SPATEM message
        for (var integer v_intersection := 0; v_intersection < lengthof(v_spatem.spat.intersections); v_intersection := v_intersection + 1) {
            var template (omit) MovementList v_states := vc_states[vc_signalGroupParmId][v_intersection];
            select (vc_spatemStatesId) {
                case (0) {
                    v_spatem.spat.intersections[v_intersection].states[0] := v_states[0];
                    v_spatem.spat.intersections[v_intersection].states[1] := v_states[1];
                    v_spatem.spat.intersections[v_intersection].states[2] := v_states[2];
                }
                case (1) {
                    v_spatem.spat.intersections[v_intersection].states[0] := v_states[1];
                    v_spatem.spat.intersections[v_intersection].states[1] := v_states[2];
                    v_spatem.spat.intersections[v_intersection].states[2] := v_states[0];
                }
                case (2) {
                    v_spatem.spat.intersections[v_intersection].states[0] := v_states[2];
                    v_spatem.spat.intersections[v_intersection].states[1] := v_states[0];
                    v_spatem.spat.intersections[v_intersection].states[2] := v_states[1];
                }
                case else {
                }
            } // End of 'select' statement
            // Update 'minEndTime' field
            v_spatem.spat.intersections[v_intersection].states[0].state_time_speed[0].timing.minEndTime := vc_currentPhaseStartTime;
            v_spatem.spat.intersections[v_intersection].states[1].state_time_speed[0].timing.minEndTime := vc_currentPhaseStartTime + vc_repitition_duration[(vc_spatemStatesId + 1) mod vc_spatemStatesNum];
            v_spatem.spat.intersections[v_intersection].states[2].state_time_speed[0].timing.minEndTime := vc_currentPhaseStartTime + vc_repitition_duration[(vc_spatemStatesId + 2) mod vc_spatemStatesNum];
            v_spatem.spat.intersections[v_intersection].timeStamp := f_getCurrentTime() mod 65536;
            v_spatem.spat.intersections[v_intersection].moy := f_getMinuteOfTheYear();
        } // End of 'for' statement
        
        p_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(
                            v_spatem
                ))),
                PICS_SPATEM_BTP_DESTINATION_PORT,
                PICS_SPATEM_BTP_SOURCE_PORT
            )
        );
        
    } // End of function f_prepare_spatem
    
    function f_prepare_ivim(
                            out template (value) Payload p_payload
    ) runs on ItsRSUsSimulator {
        
        p_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(
                            vc_rsuMessagesValueList[vc_rsu_id].ivim
                ))),
                PICS_IVIM_BTP_DESTINATION_PORT,
                PICS_IVIM_BTP_SOURCE_PORT
            )
        );
    } // End of function f_prepare_ivim
    
    function f_adaptPayload(
                            in template (value) octetstring p_finalPayload,
                            in template (value) BtpPortId  p_destPort,
                            in template (value) BtpPortId  p_srcPort := 0,
                            in NextHeader p_nextHeader := PX_GN_UPPER_LAYER
    ) return template (value) Payload {
        var template (value) Payload v_payload;
        
        if(p_nextHeader == e_any) {
            v_payload := { decodedPayload := omit, rawPayload := p_finalPayload};
            return v_payload;
        }
        
        if(p_nextHeader == e_ipv6) {
            log("*** " & testcasename() & ": INCONC: Layer IPv6 not supported ***");
            setverdict(inconc);
            stop;
        }
        
        if(p_nextHeader == e_btpA) {
            v_payload := { 
                decodedPayload := { 
                    btpPacket := m_btpAWithPorts(
                        p_destPort,
                        p_srcPort,
                        { 
                            decodedPayload := omit, 
                            rawPayload := p_finalPayload 
                        }
                    )
                },
                rawPayload := ''O
            };
            return v_payload;
        }
        
        if(p_nextHeader == e_btpB) {
            v_payload := { 
                decodedPayload := { 
                    btpPacket := m_btpBWithPorts(
                        p_destPort,
                        p_srcPort,
                        { 
                            decodedPayload := omit, 
                            rawPayload := p_finalPayload 
                        }
                    )
                }, 
                rawPayload := ''O
            };
            return v_payload;
        }
        
        return v_payload;
    } // End of function f_adaptPayload
    
    function f_mirror_and_send_vehicle_cam(
                                           in template (value) CAM p_camSimu,
                                           in CAM p_camVehicle,
                                           in ThreeDLocation p_location
    ) runs on ItsRSUsSimulator {
        // Local variables
        var ReferencePosition v_newPosition := p_camVehicle.cam.camParameters.basicContainer.referencePosition;
        var template (value) Payload v_payload;
        
        // Apply 90° rotation
        fx_computePositionFromRotation(
            p_camVehicle.cam.camParameters.basicContainer.referencePosition.latitude, 
            p_camVehicle.cam.camParameters.basicContainer.referencePosition.longitude, 
            PICS_UC6_COLLISION_POINT.latitude, 
            PICS_UC6_COLLISION_POINT.longitude, 
            -90.0, 
            v_newPosition.latitude, 
            v_newPosition.longitude);
        /*v_newPosition.latitude := ;
        v_newPosition.longitude := ;*/
        // Update CAM
        p_camSimu.cam.generationDeltaTime := f_getCurrentTime() mod 65536; // See ETSI EN 302 637-2 V1.3.0 - Clause B.3 generationDelatTime
        p_camSimu.cam.camParameters.basicContainer.referencePosition := v_newPosition;
        p_camSimu.cam.camParameters.highFrequencyContainer := p_camVehicle.cam.camParameters.highFrequencyContainer;
        v_payload := valueof(
            f_adaptPayload(
                bit2oct(
                    encvalue(
                        valueof(
                            p_camSimu
                ))),
                PICS_CAM_BTP_DESTINATION_PORT,
                PICS_CAM_BTP_SOURCE_PORT
            )
        );
        // Update GN
        vc_longPosVectorRsu := PICS_UC6_VEHICLE_TEMPLATE_POSITION;
        vc_longPosVectorRsu.latitude := valueof(p_camSimu.cam.camParameters.basicContainer.referencePosition.latitude);
        vc_longPosVectorRsu.longitude := valueof(p_camSimu.cam.camParameters.basicContainer.referencePosition.longitude);
        vc_geoArea := PICS_UC6_VEHICLE_TEMPLATE_GEOAREA;
        vc_geoArea.area.geoAreaPosLatitude := valueof(p_camSimu.cam.camParameters.basicContainer.referencePosition.latitude);
        vc_geoArea.area.geoAreaPosLongitude := valueof(p_camSimu.cam.camParameters.basicContainer.referencePosition.longitude);
        // And send it
        f_send(v_payload, PICS_CAM_ITS_AID);
    } // End of function f_send_vehicle_cam
    
    function f_send(
                    in template (value) Payload p_payload,
                    in UInt32 p_its_aid
    ) runs on ItsRSUsSimulator {
        var GeoNetworkingPdu v_geoNetworkingPdu;
        
        vc_longPosVectorRsu.timestamp_ := f_computeGnTimestamp();
        
        if (p_its_aid == 36) { // CAM 
            v_geoNetworkingPdu := valueof(m_geoNwPdu( // FIXME Use PIXIT parameter to get a fully configurable template
                m_geoNwShbPacket_payload(
                    vc_longPosVectorRsu,
                    valueof(p_payload)
                ),
                m_defaultLifetime,
                c_defaultHopLimit
            ));
        } else {
            v_geoNetworkingPdu := valueof(m_geoNwPdu( // FIXME Use PIXIT parameter to get a fully configurable template
                m_geoNwBroadcastPacket_payload( // TODO modifes 'template (value) GnNonSecuredPacket m_geoNwBroadcastPacket' to set the field
                    vc_longPosVectorRsu,
                    f_incLocalSeqNumber(),
                    f_geoArea2GeoBroadcastArea(vc_geoArea),
                    -,
                    -,
                    valueof(p_payload)
                ),
                m_defaultLifetime,
                c_hopLimit1
            ));
        }
        f_sendGeoNetMessage(valueof(m_geoNwReq_linkLayerBroadcast(v_geoNetworkingPdu, p_its_aid)));
    } // End of function f_send
    
    function f_processSrem(
                           in GeoNetworkingPdu p_geoNetworkingPdu
    ) runs on ItsRSUsSimulator {
        log("SREM=", p_geoNetworkingPdu);
        if (ispresent(p_geoNetworkingPdu.gnPacket.packet.payload.decodedPayload)) {
            if (ispresent(p_geoNetworkingPdu.gnPacket.packet.payload.decodedPayload.btpPacket.payload.decodedPayload)) {
                if (ischosen(p_geoNetworkingPdu.gnPacket.packet.payload.decodedPayload.btpPacket.payload.decodedPayload.sremPacket)) {
                    var SignalRequestMessage v_signalRequestMessage := p_geoNetworkingPdu.gnPacket.packet.payload.decodedPayload.btpPacket.payload.decodedPayload.sremPacket.srm;
                    var template (value) Payload v_payload;
                    
                    log(v_signalRequestMessage);
                    // Build response
                    // TODO v_ssem.ssm.status
                    v_payload := valueof(
                        f_adaptPayload(
                            bit2oct(
                                encvalue(
                                    valueof(
                                        m_ssem(
                                            v_signalRequestMessage
                            )))),
                            PICS_SSEM_BTP_DESTINATION_PORT,
                            PICS_SSEM_BTP_SOURCE_PORT
                        )
                    );
                    // Send SSEM 
                    f_send(v_payload, PICS_SSEM_ITS_AID);
                } // else, ignore message
            } // else, ignore message
        } // else, ignore message
    } // End of function f_processSrem
    
    function f_incLocalSeqNumber() runs on ItsRSUsSimulator return UInt16 {
        vc_localSeqNumber := (vc_localSeqNumber + 1) mod 65536;
        return vc_localSeqNumber;
    }
    
    function f_incMsgIssueRevision() runs on ItsRSUsSimulator return MsgCount {
        vc_msgIssueRevision := (vc_msgIssueRevision + 1) mod 128; // See MsgCount declaration
        return vc_msgIssueRevision;
    }
    
    function f_getMsgIssueRevision() runs on ItsRSUsSimulator return MsgCount {
        return vc_msgIssueRevision;
    }
    
    function f_incDenmSequenceNumber() runs on ItsRSUsSimulator return SequenceNumber {
        vc_sequenceNumber := (vc_sequenceNumber + 1) mod 65536; // See SequenceNumber declaration
        return vc_sequenceNumber;
    }
    
    function f_getDenmSequenceNumber() runs on ItsRSUsSimulator return SequenceNumber {
        return vc_sequenceNumber;
    }
    
} // End of module ItsRSUsSimulator_Functions