{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["GeoNetworking","CAM","DENM","_IEEE 1609.2","Geolocalisation","TD_AUTO_IOT_DENM_RWW_BV_01","TC_AUTO_IOT_DENM_RHS_BV_01","TC_AUTO_IOT_DENM_SVW_BV_01"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GeoNetworking","index":0,"n_rows":57,"n_cols":20,"rows_kept":57,"cut":false,"hidden":false,"merged":[[2,5,2,17]]}
[]
[]
[null,null,null,null,null,"Functionalities"]
[null,"Tests",null,"Expected Result","Result","Encode","Decode","device mode","automatic beaconing","manual beaconing","Location table","UpperLayer info","PCAP file","PCAP save","PCAP nic","Commsignia support","Params","Logger","acPort","utPort"]
[null,"GeoNetworking messages"]
[null,"tc_GeoNetReq_AnycastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetReq_BroadcastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetReq_UnicastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetReq_BeaconPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetReq_LsRequestPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetReq_LsReplyPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_AnycastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_BroadcastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_ShbPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_ShbPacket_1",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_UnicastPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"tc_GeoNetInd_BeaconPacket",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X"]
[null,"AC port"]
[null,"tc_GeoNet_Port_acPort_lpv",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_acPort_getLongPositionVector_1",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_acPort_getLongPositionVector_2",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_Port_acPort_beaconing_1",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_Port_acPort_beaconing_2",null,"pass","pass","X","X",null,null,null,null,null,"X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_Port_acPort_pass_beaconing_1",null,"pass","pass","X","X",null,null,"X","X","X","X","X",null,null,"X","X"]
[null,"tc_GeoNet_Port_acPort_pass_beaconing_2",null,"pass","pass","X","X",null,null,"X",null,null,"X",null,null,null,"X","X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=0\nPCAP file = test_mult_beacon"]
[null,"UT port"]
[null,"tc_GeoNet_UtGnInitialize",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnChangePosition",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoUnicast_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoUnicast_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoBroadcast_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoBroadcast_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoAnycast_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_GeoAnycast_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_Shb_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_Shb_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_Tsb_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,"tc_GeoNet_UtGnTrigger_Tsb_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=0\nPCAP file = test_mult_beacon"]
[null,"GeoNetworking port (Check with Wireshark too)"]
[null,"tc_GeoNet_Port_1"]
[null,null,"device_mode=0\nbeaconing=1\nsave_mode=1\nPCAP file = test_61_beacon","inconc","inconc","X","X",null,"X",null,"X","X","X","X",null,null,"X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=1\nPCAP file = test_61_beacon","inconc","inconc","X","X",null,"X",null,"X","X","X","X",null,null,"X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=1\nPCAP file = test_61_cam","pass","fail","X","X",null,null,null,"X","X","X","X",null,null,"X","X"]
[null,null,"device_mode=0\nbeaconing=1\nsave_mode=1\nPCAP nic","pass","fail","X","X",null,"X",null,"X","X",null,"X","X"]
[null,null,"Commsignia layer\ndevice_mode=0\nbeaconing=1\nsave_mode=1\nPCAP file = commsignia_61_beacon","inconc","inconc","X","X",null,"X",null,"X","X",null,"X","X","X"]
[null,"tc_GeoNet_Port _2"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=1\nPCAP file = test_10_beacon","pass","inconc","X","X","X","X",null,"X","X","X","X",null,null,"X","X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=1\nPCAP file = test_61_cam","pass","pass","X","X","X","X",null,"X","X","X","X",null,null,"X","X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=0\nPCAP file = commsignia_61_cam","pass","pass","X","X","X","X",null,"X","X","X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_Port _3"]
[null,null,null,"pass","pass","X","X","X","X",null,"X","X","X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_Port _4"]
[null,null,null,"pass","pass","X","X","X","X",null,"X","X","X",null,null,null,"X","X","X"]
[null,"tc_GeoNet_MultiPort"]
[null,null,"device_mode=0\nbeaconing=1\nsave_mode=1\nPCAP nic","pass",null,"X","X",null,"X",null,"X","X",null,"X","X",null,"X","X"]

{"sheet":"CAM","index":1,"n_rows":36,"n_cols":20,"rows_kept":36,"cut":false,"hidden":false,"merged":[[2,5,2,17]]}
[]
[]
[null,null,null,null,null,"Functionalities"]
[null,"Tests",null,"Expected Result","Result","Encode","Decode","GeoNet code","device mode","automatic beaconing","manual beaconing","Location table","UpperLayer info","PCAP file","PCAP save","PCAP nic","Params","Logger","acPort","utort"]
[null,"CAM messages"]
[null,"tc_CamReq",null,"pass","pass","X","X",null,null,null,null,"X","X","X","X",null,"X","X"]
[null,"tc_CamInd_1",null,"pass","pass","X","X",null,null,null,null,"X","X","X","X",null,"X","X"]
[null,"tc_CamInd_2",null,"pass","pass","X","X",null,null,null,null,"X","X","X","X",null,"X","X"]
[null,null,"device_mode=0\nbeaconing=0\nsave_mode=1\nPCAPnic"]
[]
[]
[null,"CAM port (Check with Wireshark too)"]
[null,"tc_Cam_Port"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP file = test_61_cam","pass","pass","X","X","X","X","X",null,"X","X","X","X",null,"X","X"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP nic","pass","pass","X","X","X","X","X",null,"X","X",null,null,"X","X","X"]
[null,"UT port"]
[null,"tc_Cam_UtCamInitialize",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangePosition",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangeCurvature",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangeSpeed",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetAccelerationControlStatus",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetExteriorLightsStatus_lowBeamHeadlightsOn",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetExteriorLightsStatus_leftTurnSignalOn",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetExteriorLightsStatus_daytimeRunningLightsOn",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetExteriorLightsStatus_parkingLightsOn",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangeHeading",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetDriveDirection",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangeYawRate",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamChangeYawRate_negative",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetStationType",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetVehicleRole",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetDangerousGoods",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamSetLightBarSirene",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamTriggerResult",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamEventInd_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Cam_UtCamEventInd_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,"X","X",null,"X"]

{"sheet":"DENM","index":2,"n_rows":25,"n_cols":20,"rows_kept":25,"cut":false,"hidden":false,"merged":[[2,5,2,16]]}
[]
[]
[null,null,null,null,null,"Functionalities"]
[null,"Tests",null,"Expected Result","Result","Encode","Decode","device mode","automatic beaconing","manual beaconing","Location table","UpperLayer info","PCAP file","PCAP save","PCAP nic","Params","Logger","acPort","utPort"]
[null,"GeoNetworking messages"]
[null,"tc_DenmReq"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP file = test_1_denm","pass","pass","X","X","X","X","X",null,"X","X","X","X",null,"X","X"]
[null,"tc_DenmInd"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP file = test_1_denm","pass","pass","X","X","X","X","X",null,"X","X","X","X",null,"X","X"]
[null,"DENM port  (Check with Wireshark too)"]
[null,"tc_Denm_Port"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP file = test_64_denm","pass","pass","X","X","X","X","X",null,"X","X","X",null,null,"X","X"]
[null,null,"device_mode=1\nbeaconing=1\nsave_mode=0\nPCAP nic","pass","pass","X","X","X","X","X",null,"X",null,null,"X","X","X","X"]
[null,"UT port"]
[null,"tc_Denm_UtDenmInitialize",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmChangePosition",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmChangePseudonym",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmTrigger_1",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmTrigger_2",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmUpdate_1",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmUpdate_2",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmTriggerResult",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmUpdateResult",null,"pass","pass",null,null,null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmEventInd_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,"X","X",null,"X"]
[null,"tc_Denm_UtDenmEventInd_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,null,"X","X",null,"X"]

{"sheet":"_IEEE 1609.2","index":3,"n_rows":61,"n_cols":19,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"Tests",null,"Expected Result","Result","Encode","Decode","device mode","automatic beaconing","manual beaconing","Location table","UpperLayer info","PCAP file","PCAP save","PCAP nic","Params","Logger","acPort","utPort"]
[null,"Certificates"]
[null,"tc_root_certificate_sha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_root_certificate_sha256_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_root_certificate_sha384_1",null,"pass","fail","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_at_certificate_sha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_at_certificate_sha256_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_certificate_asn1c_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"Messages"]
[null,"tc_ssp_cam_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_ssp_cam_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_ssp_denm",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_secured_message_unsecured",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_secured_message_signed_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_secured_message_signed_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"Functions"]
[null,"tc_sha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_sha384_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_generate_key_pair_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_generate_key_pair_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_generate_key_pair_3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_signWithEcdsaNistp256WithSha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaNistp256WithSha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaNistp256WithSha256_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaNistp256WithSha256_3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_signWithEcdsaBrainpoolp256WithSha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp256WithSha256_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp256WithSha256_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp256WithSha256_3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_signWithEcdsaBrainpoolp384WithSha384_1",null,"pass","fail","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp384WithSha384_1",null,"pass","fail","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp384WithSha384_2",null,"pass","fail","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_f_verifyWithEcdsaBrainpoolp384WithSha384_3",null,"pass","fail","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_load_certificates",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_read_certificate_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_read_certificate_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,".tc_read_certificate_digest",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"Chain of certificates"]
[null,"tc_full_check_certificate_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_full_check_certificate_2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"Encryption"]
[null,"tc_test_hmac_sha256_test1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_test_hmac_sha256_test2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_test_hmac_sha256_test3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_test_encrypt_aes_128_ccm_test1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_test_encrypt_aes_128_ccm_test2",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_test_encrypt_aes_128_ccm_test3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_encrypted_signed_message_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_decrypted_signed_message_1",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_decrypted_signed_message_2",null,"fail","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_decrypted_signed_message_3",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[null,"tc_decrypted_signed_message_4",null,"pass","pass","X","X",null,null,null,null,null,null,null,null,"X","X"]
[]
[]
[]
[]
[null,"tc_GeoNet_Port _3",null,null,null,"X","X",null,"X",null,"X",null,"X","X","X","X","X"]
[null,"tc_GeoNet_Port _4",null,null,null,"X","X",null,"X",null,"X",null,"X","X","X","X","X"]

{"sheet":"Geolocalisation","index":4,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["To be done"]

{"sheet":"TD_AUTO_IOT_DENM_RWW_BV_01","index":5,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["UC1"]
["File","SwarcoUC1Z0","uc1-rsu102-2016-11-14_12_49"]
["EUT1:","Swarco","04e548000001",10171,"RSU"]
["EUT2","Commsignia","70b3d5791b48",10031,"Vehicle"]

{"sheet":"TC_AUTO_IOT_DENM_RHS_BV_01","index":6,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["UC2"]
["File","plugtest2016-log-locD 007"]
["EUT1:","Kapsh","00e06a00bba1",10088,"RSU"]
["EUT2","Qfree","4c5e0c14d2ea",10143,"Vehicle"]

{"sheet":"TC_AUTO_IOT_DENM_SVW_BV_01","index":7,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["UC6"]
["File","sniff-downtown-2016-11-17__13-03"]
["EUT1:","Kapsh","b482fe4433eb",10002,"RSU"]
["EUT2","Savari","6782878c785e",10152,"Vehicle"]