ETSI ES 202 785 V1.9.1 (2022-05)

Methods for Testing and Specification (MTS);

The Testing and Test Control Notation version 3;

TTCN-3 Language Extensions: Behaviour Types

**ETSI Standard**

Reference

RES/MTS-202785v191

Keywords

conformance, testing, TTCN-3

***ETSI***

650 Route des Lucioles

F-06921 Sophia Antipolis Cedex - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Siret N° 348 623 562 00017 - APE 7112B

Association à but non lucratif enregistrée à la

Sous-Préfecture de Grasse (06) N° w061004871

***Important notice***

The present document can be downloaded from:  
<http://www.etsi.org/standards-search>

The present document may be made available in electronic versions and/or in print. The content of any electronic and/or print versions of the present document shall not be modified without the prior written authorization of ETSI. In case of any existing or perceived difference in contents between such versions and/or in print, the prevailing version of an ETSI deliverable is the one made publicly available in PDF format at [www.etsi.org/deliver](http://www.etsi.org/deliver).

Users of the present document should be aware that the document may be subject to revision or change of status. Information on the current status of this and other ETSI documents is available at <https://portal.etsi.org/TB/ETSIDeliverableStatus.aspx>

If you find errors in the present document, please send your comment to one of the following services:  
<https://portal.etsi.org/People/CommiteeSupportStaff.aspx>

If you find a security vulnerability in the present document, please report it through our

Coordinated Vulnerability Disclosure Program:

<https://www.etsi.org/standards/coordinated-vulnerability-disclosure>

***Notice of disclaimer & limitation of liability***

The information provided in the present deliverable is directed solely to professionals who have the appropriate degree of experience to understand and interpret its content in accordance with generally accepted engineering or

other professional standard and applicable regulations.

No recommendation as to products and services or vendors is made or should be implied.

No representation or warranty is made that this deliverable is technically accurate or sufficient or conforms to any law and/or governmental rule and/or regulation and further, no representation or warranty is made of merchantability or fitness for any particular purpose or against infringement of intellectual property rights.

In no event shall ETSI be held liable for loss of profits or any other incidental or consequential damages.

Any software contained in this deliverable is provided "AS IS" with no warranties, express or implied, including but not limited to, the warranties of merchantability, fitness for a particular purpose and non-infringement of intellectual property rights and ETSI shall not be held liable in any event for any damages whatsoever (including, without limitation, damages for loss of profits, business interruption, loss of information, or any other pecuniary loss) arising out of or related to the use of or inability to use the software.

***Copyright Notification***

No part may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm except as authorized by written permission of ETSI.  
The content of the PDF version shall not be modified without the written authorization of ETSI.  
The copyright and the foregoing restriction extend to reproduction in all media.

© ETSI 2022.

All rights reserved.

Contents

Intellectual Property Rights 4

Foreword 4

Modal verbs terminology 4

1 Scope 5

2 References 5

2.1 Normative references 5

2.2 Informative references 6

3 Definition of terms, symbols and abbreviations 6

3.1 Terms 6

3.2 Symbols 6

3.3 Abbreviations 6

4 Package conformance and compatibility 6

5 Package concepts for the core language 7

5.1 Extension to ETSI ES 201 873-1, clause 5 (Basic language elements) 7

5.2 Extension to ETSI ES 201 873-1, clause 6 (Types and values) 8

5.3 Extension to ETSI ES 201 873-1, clause 7 (Expressions) 14

5.4 Extension to ETSI ES 201 873-1, clause 8 (Modules) 14

5.5 Extension to ETSI ES 201 873-1, clause 10 (Declaring constants) 15

5.6 Extension to ETSI ES 201 873-1, clause 11 (Declaring variables) 15

5.7 Extension to ETSI ES 201 873-1, clause 15 (Declaring templates) 15

5.8 Extension to ETSI ES 201 873-1, clause 16 (Functions, altsteps and test cases) 16

5.9 Extension to ETSI ES 201 873-1, clause 19 (Basic program statements) 16

5.10 Extension to ETSI ES 201 873-1, clause 20 (Statement and operations for alternative behaviours) 17

5.11 Extension to ETSI ES 201 873-1, clause 21 (Configuration Operations) 17

5.12 Extension to ETSI ES 201 873-1, clause 26 (Module control) 18

5.13 Extension to ETSI ES 201 873-1, annex A (BNF and static semantics) 19

5.13.0 New keywords and TTCN-3 syntax BNF productions 19

5.13.1 Changes to ETSI ES 201 873-1, clause A.1.6 (TTCN-3 syntax BNF productions) 19

6 Package semantics 20

6.1 Replacements 20

6.2 Activate statement 20

6.3 Replacements in Execute statement's operational semantics 21

6.3.0 Execute statement 21

6.3.1 Flow graph segment <execute-without-timeout> 22

6.4 Replacements in Function call's operational semantics 23

6.4.0 Function call 23

6.4.1 Flow graph segment <user-def-func-call> 25

6.4.2 Flow graph segment <predef-ext-func-call> 25

6.5 Start component operation 25

7 TRI extensions for the package 28

8 TCI extensions for the package 28

8.1 Extensions to ETSI ES 201 873-6, clause 7 (TTCN-3 control interface and operations) 28

8.2 Extensions to ETSI ES 201 873-6, clause 8 (Java language mapping) 29

8.3 Extensions to ETSI ES 201 873-6, clause 9 (ANSI C language mapping) 30

8.4 Extensions to ETSI ES 201 873-6, clause 10 (C++ language mapping) 30

8.5 Extensions to ETSI ES 201 873-6, clause 11 (W3C XML mapping) 32

9 Extensions to TTCN-3 documentation comment specification for the package 42

9.1 Extensions to ETSI ES 201 873-10, annex A (where Tags can be used) 42

History 44

# Intellectual Property Rights

Essential patents

IPRs essential or potentially essential to normative deliverables may have been declared to ETSI. The declarations pertaining to these essential IPRs, if any, are publicly available for **ETSI members and non-members**, and can be found in ETSI SR 000 314: *"Intellectual Property Rights (IPRs); Essential, or potentially Essential, IPRs notified to ETSI in respect of ETSI standards"*, which is available from the ETSI Secretariat. Latest updates are available on the ETSI Web server (<https://ipr.etsi.org/>).

Pursuant to the ETSI Directives including the ETSI IPR Policy, no investigation regarding the essentiality of IPRs, including IPR searches, has been carried out by ETSI. No guarantee can be given as to the existence of other IPRs not referenced in ETSI SR 000 314 (or the updates on the ETSI Web server) which are, or may be, or may become, essential to the present document.

Trademarks

The present document may include trademarks and/or tradenames which are asserted and/or registered by their owners. ETSI claims no ownership of these except for any which are indicated as being the property of ETSI, and conveys no right to use or reproduce any trademark and/or tradename. Mention of those trademarks in the present document does not constitute an endorsement by ETSI of products, services or organizations associated with those trademarks.

**DECT™**, **PLUGTESTS™**, **UMTS™** and the ETSI logo are trademarks of ETSI registered for the benefit of its Members. **3GPP™**and **LTE™** are trademarks of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners. **oneM2M™** logo is a trademark of ETSI registered for the benefit of its Members and of the oneM2M Partners. **GSM**® and the GSM logo are trademarks registered and owned by the GSM Association.

# Foreword

This ETSI Standard (ES) has been produced by ETSI Technical Committee Methods for Testing and Specification (MTS).

**The use of underline (additional text) highlights the differences between base document and extended documents.**

The present document relates to the multi-part standard ETSI ES 201 873 covering the Testing and Test Control Notation version 3, as identified in ETSI ES 201 873-1 [1].

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the [ETSI Drafting Rules](https://portal.etsi.org/Services/editHelp!/Howtostart/ETSIDraftingRules.aspx) (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in ETSI deliverables except when used in direct citation.

# 1 Scope

The present document defines the Behaviour Types package of TTCN‑3. TTCN‑3 can be used for the specification of all types of reactive system tests over a variety of communication ports. Typical areas of application are protocol testing (including mobile and Internet protocols), service testing (including supplementary services), module testing, testing of APIs, etc. TTCN‑3 is not restricted to conformance testing and can be used for many other kinds of testing including interoperability, robustness, regression, system and integration testing. The specification of test suites for physical layer protocols is outside the scope of the present document.

TTCN‑3 packages are intended to define additional TTCN-3 concepts, which are not mandatory as concepts in the TTCN-3 core language, but which are optional as part of a package which is suited for dedicated applications and/or usages of TTCN-3.

This package defines types for behaviour definitions in TTCN-3.

While the design of TTCN‑3 package has taken into account the consistency of a combined usage of the core language with a number of packages, the concrete usages and guidelines for this package in combination with other packages is outside the scope of the present document.

# 2 References

## 2.1 Normative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

Referenced documents which are not found to be publicly available in the expected location might be found at <https://docbox.etsi.org/Reference/>.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are necessary for the application of the present document.

[1] ETSI ES 201 873-1: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN-3 Core Language".

[2] ETSI ES 201 873-4: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 4: TTCN-3 Operational Semantics".

[3] ETSI ES 201 873-5: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 5: TTCN-3 Runtime Interface (TRI)".

[4] ETSI ES 201 873-6: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 6: TTCN-3 Control Interface (TCI)".

[5] ISO/IEC 9646-1: "Information technology -- Open Systems Interconnection -- Conformance testing methodology and framework; Part 1: General concepts".

[6] ETSI ES 202 784: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Advanced Parameterization".

[7] ETSI ES 201 873-10: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 10: TTCN-3 Documentation Comment Specification".

## 2.2 Informative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.

[i.1] ETSI ES 201 873-7: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 7: Using ASN.1 with TTCN-3".

[i.2] ETSI ES 201 873-8: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 8: The IDL to TTCN-3 Mapping".

[i.3] ETSI ES 201 873-9: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 9: Using XML schema with TTCN-3".

# 3 Definition of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in ETSI ES 201 873-1 [1], ETSI ES 201 873‑4 [2], ETSI ES 201 873-5 [3], ETSI ES 201 873-6 [4], ISO/IEC 9646-1 [5] and the following apply:

**behaviour definition:** definition of an altstep, function, or testcase that can be called explicitly

NOTE: A control part is not considered a behaviour definition, because it cannot be called explicitly.

**behaviour type:** type of behaviour definitions

NOTE: Behaviour types are of kind altstep, function, or testcase.

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in ETSI ES 201 873-1 [1], ETSI ES 201 873‑4 [2], ETSI ES 201 873‑5 [3], ETSI ES 201 873-6 [4] and ISO/IEC 9646-1 [5] apply.

# 4 Package conformance and compatibility

The package presented in the present document is identified by the package tag:

"TTCN‑3:2009 Behaviour Types" *- to be used with modules complying with the present document*

For an implementation claiming to conform to this package version, all features specified in the present document shall be implemented consistently with the requirements given in the present document; in ETSI ES 201 873‑1 [1] and ETSI ES 201 873‑4 [2]. All features marked [AdvancedParameterization] have to be implemented only in case that this package is used together with the Advanced Parameterization package [6].

The package presented in the present document is compatible with:

* ETSI ES 201 873-1 [1] (V4.5.1).
* ETSI ES 201 873-4 [2] (V4.4.1).
* ETSI ES 201 873-5 [3] (V4.5.1).
* ETSI ES 201 873-6 [4] (V4.5.1).
* ETSI ES 201 873-7 [i.1] (V4.5.1).
* ETSI ES 201 873-8 [i.2] (V4.5.1).
* ETSI ES 201 873-9 [i.3] (V4.5.1).
* ETSI ES 201 873-10 [7] (V4.5.1).

If later versions of those parts are available and should be used instead, the compatibility to the package presented in the present document has to be checked individually.

The package presented in the present document is also compatible with:

* ETSI ES 202 784 [6] Package Advanced Parameterization (V1.3.1);

and can be used together with this package.

If later versions of those packages are available and should be used instead, the compatibility to the package presented in the present document has to be checked individually.

# 5 Package concepts for the core language

## 5.1 Extension to ETSI ES 201 873-1, clause 5 (Basic language elements)

Clause 5.4 Parameterization

Values of behaviour types can be passed as parameters as indicated in table 2.

Table 2: Overview of parameterizable TTCN‑3 objects

|  |  |  |  |
| --- | --- | --- | --- |
| Keyword | Allowed kind of Parameterization | Allowed form of Parameterization | Allowed types in formal parameter lists |
| module | Value parameterization | Static at start of run-time | all basic types, all user-defined types and **address** type. |
| type (see note) | Value parameterization | Static at compile-time | all basic types, all user-defined types and **address** type. |
| template | Value and template parameterization | Dynamic at run-time | all basic types, all user-defined types, **address** type, **template**, andbehaviour types. |
| function | Value, template, port and timer parameterization | Dynamic at run-time | all basic types, all user-defined types, **address** type, **component** type, **port** type, **default**, behaviour types, **template** and **timer**. |
| altstep | Value, template, port and timer parameterization | Dynamic at run-time | all basic types, all user-defined types, **address** type, **component** type, **port** type, **default**, behaviour types, **template** and **timer**. |
| testcase | Value, template, port and timer parameterization | Dynamic at run-time | all basic types and of all user-defined types, **address** type, **template**, andbehaviour types. |
| signature | Value and template parameterization | Dynamic at run-time | all basic types, all user-defined types and **address** type, **component** type, andbehaviour types. |
| NOTE: Record of, set of, enumerated, port, component and sub-type definitions do not allow parameterization. | | | |

Clause 5.4.1.1 Formal parameters of kind value

Also, values of behaviour types can be passed as value parameters.

## 5.2 Extension to ETSI ES 201 873-1, clause 6 (Types and values)

Behaviour types such as **altstep**, **function**, and **testcase** may be used to define flexible behaviour of TTCN‑3 libraries.

No subtyping is defined for behaviour types.

Clause 6.2 Structured Types and Values

Extend clause 6.2 Structured types and values by the following clause 6.2.13.

6.2.13 Behaviour Types

6.2.13.1 Behaviour Type Definitions

Behaviour types are the set of identifiers of altstep, function, and testcase definitions with a specific parameter list, runs on, system, mtc and return clauses. They denote those altsteps, functions, and testcases, respectively, defined in the test suite that have a compatible parameter list and compatible **runs on** or **system** clauses.

***Syntactical Structure***

**type**  **function** *BehaviourTypeIdentifier*[ "<" { *FormalTypePar* [","] } ">" ] NOTE 1

"(" [ { ( *FormalValuePar* | *FormalTimerPar* | *FormalTemplatePar* | *FormalPortPar* ) [","] } ] ")"

[ **runs** **on** ( *ComponentType |* **self**] NOTE 2

[ **mtc** *ComponentType* ]

[ **system** *ComponentType* ]

[ **return** [ **template** ] *Type* ]

**type altstep** *BehaviourTypeIdentifier*[ "<" { *FormalTypePar* [","] } ">" ] NOTE 1

"(" [ { ( *FormalValuePar* | *FormalTimerPar* | *FormalTemplatePar* | *FormalPortPar* ) [","] } ] ")"

[ **runs** **on** ( *ComponentType |* **self**] NOTE 2

[ **mtc** *ComponentType* ]

[ **system** *ComponentType* ]

**type testcase** *BehaviourTypeIdentifier*[ "<" { *FormalTypePar* [","] } ">" ] NOTE 1

"(" [ { ( *FormalValuePar* | *FormalTemplatePar* ) [","] } ] ")"

**runs** **on** *ComponentType*

[ **system** *ComponentType* ]

***Semantic Description***

Behaviour types define prototypes of altsteps, functions, and testcases.

NOTE 1: [AdvancedParameterization] If the advanced parameterization package [6] is also supported, behaviour types can have type parameters.

NOTE 2: **runs on self** indicates a specific compatibility check, see extension of clause 6.3.

***Restrictions***

1. The rules for formal parameter lists shall be followed as defined in the TTCN-3 Core Language [1] clause 5.4 and extended in clause 5.1 of the present document.
2. Behaviour types of kind **altstep** may have a **runs on**, **system** or **mtc** clause, behaviour types of type **function** may have a **runs on**, **system**, **mtc** or **return** clause, behaviour types of kind **testcase** shall have a **runs on** clause and may have a **system** clause.
3. **runs on self** shall not be used for test cases.

***Examples***

EXAMPLE 1: Function type with one parameter and a return value.

**type function** MyFunc1 ( **in integer** p1 ) **return** **boolean**;

EXAMPLE 2: Function type with one parameter, a **runs on** clause and a return value.

**type function** MyFunc2 ( **in integer** p1 ) **runs** **on** MyCompType **return** **boolean**;

EXAMPLE 3: Altstep type with a type parameter and a **runs on** clause.

**type altstep** MyAltstep1<**type** T> ( **in** T p1 ) **runs on** MyCompType;

EXAMPLE 4: Testcase type without parameter, with a **runs on** clause and a **system** clause.

**type testcase** MyTestcase1 ( ) **runs on** MyCompType **system** MySysType;

6.2.13.2 Behaviour Values

The values of a behaviour type are the identifiers of altsteps, functions, and testcases with compatible parameters and **runs on,** **system**, **mtc** and **return** clauses. Both predefined and user-defined, including external, functions can be used as values. Type compatibility of behaviour types is defined in the extension to clause 6.3.5 within the present document.

***Syntactical Structure***

*VariableRef | FunctionInstance | FunctionRef | AltstepRef | TestcaseRef |* null

***Semantic Description***

The literal behaviour values are the identifiers of the predefined and user-defined altsteps, (external) functions, and testcases and the special value **null**. The special value **null** is available to indicate an undefined behaviour value, e.g. for the initialization of variables. Behaviour values can be passed around as parameters and behaviour values can be stored. Behaviour values can be used, together with a corresponding list of actual parameters, to invoke the behaviours in statements and expressions. Behaviour values can also be used, again together with a corresponding list of actual parameters, in **activate**, **start**, and **execute** statements, respectively.

The only operators (see clause 7.1 of the TTCN-3 core language [1]) on behaviour values that are defined are the check for equality and inequality.

***Restrictions***

1. Values of a behaviour type with a **runs on self** clause shall not be sent to another test component.
2. Values of a behaviour type with a **runs on self** clause shall not be used in a start test component operation.
3. The special value **null** shall not be used to invoke a behaviour.

***Examples***

**type function** MyFunc3 ( **in integer** p1 ) **return** **charstring**;

**function** blanks (**in** **integer** p1) **return** **charstring** {

// return a charstring of p1 blank characters

}

**var** MyFunc3 myVar1 := blanks;

**var** MyFunc3 myVar1 := int2char;

6.2.13.3 Deferred Behaviour Type Definitions

Deferred behaviour types are the set of altstep, function, and testcase behaviours with possible runs on, system and mtc clauses paired with their actual parameter list which can be passed to the **activate**, **start** and **execute** operations, respectively. They denote those instantiations of altsteps, functions, and testcases defined in the test suite that have compatible **runs on**, **system** or **mtc** clauses.

***Syntactical Structure***

**type**  **function** BehaviourTypeIdentifier

[ **runs** **on** ComponentType ]

[ **mtc** ComponentType ]

[ **system** ComponentType ]

**type altstep** BehaviourTypeIdentifier

[ **runs** **on** ComponentType ]

[ **mtc** ComponentType ]

[ **system** ComponentType ]

**type testcase** BehaviourTypeIdentifier

**runs** **on** ComponentType

[ **system** ComponentType ]

***Semantic Description***

Deferred behaviour types define references to executable behaviours. Deferred function behaviour types define the set of behaviours that can be started on a ptc. Deferred altstep behaviour types define the set of behaviours that can be activated as default alternatives. Deferred testcase behaviour types define the set of behaviours that can be executed from the control part.

The actual parameters of a deferred behaviour value are evaluated when creating the value.

***Restrictions***

1. The same restrictions apply for the start, activate and execute operations that apply for functions, altsteps and testcases used directly in these statements in a non-deferred way.

***Examples***

EXAMPLE 1: Deferred function type with.

**type function** MyFunc1;

EXAMPLE 2: Deferred function type with a **runs on** clause.

**type function** MyFunc2 **runs** **on** MyCompType;

EXAMPLE 3: Deferred altstep type with a **runs on** clause.

**type altstep** MyAltstep1 **runs on** MyCompType;

EXAMPLE 4: Deferred testcase type with a **runs on** clause and a **system** clause.

**type testcase** MyTestcase1 **runs on** MyCompType **system** MySysType;

6.2.13.4 Deferred Behaviour Values

The values of a deferred behaviour type are the un-executed instantiations of altsteps, functions, and testcases together with their compatible actual parameters which have compatible runs on, system and mtc clauses to those in the behaviour type. Type compatibility of deferred behaviour types is defined in the extension to clause 6.3.5 within the present document.

***Syntactical Structure***

*VariableRef | FunctionInstance*

***Semantic Description***

The literal deferred behaviour values are the function instance expressions of the user-defined altsteps, (external) functions, and testcases. Deferred behaviour values can be passed around as actual parameters or stored in a variable. Deferred altstep, function or testcase behaviour values can be used in **activate**, **start**, and **execute** statements, respectively.

The only operators (see clause 7.1 of the TTCN-3 core language [1]) on deferred behaviour values that are defined are the check for equality and inequality.

***Restrictions***

1. Only in functions, altsteps and testcases without inout or out parameters shall be used as deferred behaviour values.
2. For the actual parameters of a function behaviour value instance, restrictions from clause 21.3.2 of the core language specification shall apply.
3. For the actual parameters of an alstep behaviour value instance, restrictions from clause 20.5.2 of the core language specification shall apply.
4. For the actual parameters of a testcase behaviour value instance, restriction from clause 26.1 of the core language specification shall apply.

***Examples***

EXAMPLE 1:

**type function** MyFunctionBehaviour;

**function** MyFunction (**in** **integer** p1) {

// …

}

**var** MyFunctionBehaviour v\_myBehaviour := MyFunction(4); // does not invoke MyFunction(4)

var PtcType ptc := PtcType.create;

ptc.start(myBehaviour); // starts MyFunction(4) on component ptc

EXAMPLE 2:

type altstep MyAltstepType runs on PtcType;

altstep MyAltstep(integer i) runs on PtcType {

[] …

}

var MyAltstepType v\_myAltstep := MyAltstep(3);

activate(v\_myAltstep);

EXAMPLE 3:

type testcase MyTestcaseBehaviour runs on PtcType;

testcase MyTestcase(integer i) runs on PtcType { … }

function runTestCase(MyTestcaseBehaviour p\_myTestcase) {

execute(p\_myTestcase, 1.0);

}

control {

var MyTestcaseBehaviour v\_myTestcase := MyTestcase(3);

runTestCase(v\_myTestcase);

runTestCase(MyTestcase(4)); // execution is deferred to runTestCase

}

Clause 6.3 Type compatibility

Clause 6.3 Type compatibility is extended by:

6.3.5 Type compatibility of behaviour types

Altsteps are only compatible to **altstep** behaviour types, functions are only compatible to **function** behaviour types, testcases are only compatible to **testcase** behaviour types. A behaviour object (an altstep, function or testcase) is a value of a given behaviour type, if the parameter lists are compatible, if the return clause is compatible, if the **runs** **on**, **mtc** and **system** clauses are compatible, provided they exist, and if modifiers (optionally) declared for the behaviour object and the given behaviour type are identical.

The parameter list of an object is compatible with the parameter list of a type if the order of the parameters is identical, as well as direction, kind, type, name of the parameters, optional modifiers and whether a default exists. If the parameter is of kind **template**, then also potential template restrictions have to be identical. Compatibility of parameter lists applies to the type parameter list, if exists (i.e. when the advanced parameterization package [6] is also supported and a type parameter list is defined), and the value parameter list separately.

The return clause of a function is compatible with the return clause of a function type if it is either absent in case the function type does not have a return clause, or it is of identical kind and type if the function type has a return clause. In case the return clause is of kind **template**, then potential template restrictions have to be identical, too.

The **runs** **on** clause of an object is compatible with the **runs** **on** clause of a behaviour type, if it is either absent in the object or, if the **runs** **on** clause exists, the component type in the **runs** **on** clause of the object is runs on compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, section 2)) with the type specified in the **runs on** clause of the behaviour type. According to the first condition, an object without a **runs** **on** clause is compatible with a behaviour type that has a **runs** **on** clause.

The **system** clause of a **testcase** object is compatible with the **system** clause of a **testcase** type, if the component type in the **system** clause of the **testcase** object is system compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, section 4)) with the type specified in the **system** clause of the **testcase** type. If the **testcase** object or the **testcase** behaviour type does not have a **system** clause, then the component type of the **runs** **on** clause is used instead (see ETSI ES 201 873‑1 [1], clause 9.2).

The **system** clause of a function or altstep object is compatible with the **system** clause of a function or altstep behaviour type, if it is either absent in the function or altstep object or, if the **system** clause exists, the component type in the **system** clause of the function or altstep object is system compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, section 4)) with the type specified in the **system** clause of the function or altstep behaviour. According to the first condition, a function or altstep object without a **system** clause is compatible with a function or altstep behaviour type that has a **system** clause.

The **mtc** clause of an object is compatible with the **mtc** clause of a behaviour type, if it is either absent in the object or, if the **mtc** clause exists, the component type in the **mtc** clause of the object is mtc compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, section 3)) with the type specified in the **mtc** clause of the behaviour type. According to the first condition, an object without an **mtc** clause is compatible with a behaviour type that has an **mtc** clause.

For functions it does not matter whether the function is an external function. If the parameter lists are compatible, then an external function is also compatible with the function behaviour type.

EXAMPLE:

// Given

**type** **component** MyCompType0 { };

**type** **component** MyCompType1 { **integer** a };

**type** **component** MyCompType2 { **integer** a;   
 **float** b };

**type function** MyFunc( **in integer** p1 ) **runs on** MyCompType1 **return boolean;**

**type function** MyFuncNoRunsOn( **in integer** p1 ) **return boolean;**

//compatible with MyFunc, identical parameterlist, runs on clause, return type

**function** f1 (**in** **integer** p1) **runs** **on** MyCompType1 **return** **boolean** { /\*…\*/ };

//compatible with MyFunc, component type in type extends the one of the function

**function** f2 (**in** **integer** p1) **runs** **on** MyCompType0 **return** **boolean** { /\* … \*/ }

//compatible with MyFunc, function does not have runs on clause

**function** f3 (**in** **integer** p1) **return** **boolean** { /\* … \*/ }

//incompatible with MyFunc, additional parameter without default value

**function** g1 (in **integer** p1, **in** **boolean** p2) **runs** **on** MyCompType1 **return** **boolean** { /\*…\*/ };

//incompatible with MyFunc, missing return clause

**function** g2 (in **integer** p1) **runs** **on** MyCompType1 { /\*…\*/ };

//incompatible with MyFunc, different kind of parameter

**function** g3 (in **template** **integer** p1) **runs** **on** MyCompType1 **return** **boolean** { /\*…\*/ };

//incompatible with MyFunc, component type of function is an extension of the function type

**function** g4 (**in** **integer** p1) **runs** **on** MyCompType2 **return** **boolean** { /\* … \*/ }

//incompatible with MyFuncNoRunsOn, function has runs on clause, type does not have one

**function** g5 (**in** **integer** p1) **runs** **on** MyCompType1 **return** **boolean** { /\* … \*/ }

6.3.6 Type compatibility of behaviour types with runs on self

Function and altstep types can be defined with a **runs on self** clause. If a specific value is assigned to a variable or parameter of such a behaviour type, then the **runs on** clause of the enclosing definition is used in the compatibility check.

A value of a behaviour type with a **runs** **on** **self** clause can always be used in a function or altstep invocation.

***Restriction***

1. Behaviour type definitions of module parameters and global constants shall have no **runs on** **self** clause.

NOTE: The compatibility check is not possible for module parameters and global constants defined in the module definitions because the module definitions part has no **runs on** clause.

EXAMPLE:

// Given

**type** **component** MyCompType0 { };

**type** **component** MyCompType1 { **integer** a };

**type** **component** MyCompType2 { **integer** a;   
 **float**  b };

**type function** MyFuncType( **in integer** p1 ) **runs on self;**

**function** MyFunc1( **in integer** p1 ) **runs on** MyCompType1 { /\* … \*/ }**;  
function** MyFunc2 () **runs on** MyCompType2 { **var** MyFuncType func;  
 func := MyFunc1; // correct,   
 // MyCompType1 of MyFunc1 is compared against MyCompType2 of MyFunc2  
:  
}

6.3.7 Type compatibility of deferred behaviour types

Deferred altstep behaviour values are only compatible to deferred **altstep** behaviour types, deferred function behaviour values are only compatible to deferred **function** behaviour types, deferred testcase behaviour values are only compatible to deferred **testcase** behaviour types. A behaviour object (an altstep, function or testcase) is a value of a given behaviour type, if the **runs** **on**, **system** and mtc clauses are compatible, provided they exist.

The **runs** **on** clause of a deferred object is compatible with the **runs** **on** clause of a deferred behaviour type, if it is either absent in the object or, if the **runs** **on** clause exists, the component type in the **runs** **on** clause of the object is runs on compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, condition 2)) with the type specified in the **runs on** clause of the deferred behaviour. According to the first condition, an object without a **runs** **on** clause is compatible with a deferred behaviour type that has a **runs** **on** clause.

The **system** clause of a deferred **testcase** behaviour object is compatible with the **system** clause of a deferred **testcase** behaviour type, if the component type in the **system** clause of the **testcase** object is system compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, condition 4)) with the type specified in the **system** clause of the deferred **testcase** behaviour type. If the **testcase** object or the deferred **testcase** behaviour type does not have a **system** clause, then the component type of the **runs** **on** clause is used instead (see ETSI ES 201 873‑1 [1], clause 9.2).

The **system** clause of a deferred function or altstep object is compatible with the **system** clause of a deferred function or altstep behaviour type, if it is either absent in the function or altstep object or, if the **system** clause exists, the component type in the **system** clause of the function or altstep object is system compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, condition 4)) with the type specified in the **system** clause of the deferred function or altstep behaviour type. According to the first condition, a function or altstep object without a **system** clause is compatible with a deferred function or altstep behaviour type that has a **system** clause.

The **mtc** clause of a deferred object is compatible with the **mtc** clause of a deferred behaviour type, if it is either absent in the object or, if the **mtc** clause exists, the component type in the **mtc** clause of the object is mtc compatible (see ETSI ES 201 873‑1 [1], clause 6.3.3, condition 3)) with the type specified in the **mtc** clause of the deferred behaviour type. According to the first condition, an object without an **mtc** clause is compatible with a deferred behaviour type that has an **mtc** clause.

EXAMPLE:

// Given

**type** **component** MyCompType0 { };

**type** **component** MyCompType1 { **integer** a };

**type** **component** MyCompType2 { **integer** a;   
 **float** b };

**type function** MyFunc **runs on** MyCompType1**;**

**type function** MyFuncNoRunsOn**;**

// instantiations of f1 are compatible with MyFunc runs on clause

**function** f1 (**in** **integer** p1) **runs** **on** MyCompType1 **return** **boolean** { /\*…\*/ };

// instantiations of f2 are compatible with MyFunc, component type in type

// extends the one of the function

**function** f2 (**in** **integer** p1) **runs** **on** MyCompType0 **return** **boolean** { /\* … \*/ }

// instantiations of f3 compatible with MyFunc, function does not have runs on clause

**function** f3 (**in** **integer** p1) **return** **boolean** { /\* … \*/ }

//incompatible with MyFunc, component type of function is an extension of the function type

**function** g4 (**in** **integer** p1) **runs** **on** MyCompType2 **return** **boolean** { /\* … \*/ }

//incompatible with MyFuncNoRunsOn, function has runs on clause, type does not have one

**function** g5 (**in** **integer** p1) **runs** **on** MyCompType1 **return** **boolean** { /\* … \*/ }

## 5.3 Extension to ETSI ES 201 873-1, clause 7 (Expressions)

Values of behaviour types can be passed around as parameters, stored in variables, exchanged among components, compared against each other, and applied to parameter lists. No other operation is defined on values of behaviour types.

Values of deferred behaviour types can be passed around as parameters, stored in variables, exchanged among components, compared against each other, and used in the component start, activate and execute operations, dependant on their behaviour kind. No other operation is defined on values of behaviour types.

Clause 7.1.3 Relational operators

The operators of equality and non-equality can be applied to values of the same behaviour type. Each behaviour value can be compared with **null**. No other value is equal to **null**.

The operators of equality and non-equality can be applied to values of the same deferred behaviour type.

## 5.4 Extension to ETSI ES 201 873-1, clause 8 (Modules)

Clause 8.2.1 Module parameters

Module parameters of behaviour types can be declared.

Module parameters of deferred behaviour types can be declared.

## 5.5 Extension to ETSI ES 201 873-1, clause 10 (Declaring constants)

Constants of behaviour types can be declared.

Constants of deferred behaviour types can be declared.

## 5.6 Extension to ETSI ES 201 873-1, clause 11 (Declaring variables)

Variables of behaviour types can be declared.

Variables of deferred behaviour types can be declared.

## 5.7 Extension to ETSI ES 201 873-1, clause 15 (Declaring templates)

Clause 15.7 Template matching mechanisms

Template matching mechanisms can be used for behaviour types and deferred behaviour types as indicated in the following extension of table 11 TTCN-3 matching mechanisms.

| Used with values of | Value | | Instead of values | | | | | | | | Inside values | | | Attributes | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | S  p  e  c  i  f  i  c  V  a  l  u  e | O  m  i  t  V  a  l  u  e | C  o  m  p  l  e  m  e  n  t  e  d  L  i  s  t | V  a  l  u  e  L  i  s  t | A  n  y  V  a  l  u  e  (?) | A  n  y  V  a  l  u  e  O  r  n  o  n  e  (s  e  e  n  o  t  e) | R  a  n  g  e | S  u  p  e  r  s  e  t | S  u  b  s  e  t | P  a  t  t  e  r  n | A  n  y  e  l  e  m  e  n  t  (?) | A  n  y  E  l  e  m  e  n  t  s  O  r  n  o  n  e  (s  e  e  n  o  t  e) | P  e  r  mu  t  a  t  i  o  n | L  e  n  g  t  h  R  e  s  t  r  i  c  t  i  o  n | I  f  P  r  e  s  e  n  t |
| **altstep** | Yes | Yes | Yes | Yes | Yes | Yes (see note 3) |  |  |  |  |  |  |  |  | Yes (see note 3) |
| **function** | Yes | Yes | Yes | Yes | Yes | Yes (see note 3) |  |  |  |  |  |  |  |  | Yes (see note 3) |
| **testcase** | Yes | Yes | Yes | Yes | Yes | Yes (see note 3) |  |  |  |  |  |  |  |  | Yes (see note 3) |
| ...  NOTE 3: When used, shall be applied to optional fields of record and set types only (without restriction on the type of that field). | | | | | | | | | | | | | | | |

## 5.8 Extension to ETSI ES 201 873-1, clause 16 (Functions, altsteps and test cases)

Clause 16.1.1 Invoking functions

A function can also be invoked by the **apply** operation by referring to an expression of a behaviour type of kind function and to a parameter list.

***Syntactical Structure***

**apply** *"*(*" Value "*(*"* [ { ( *TimerRef* | *TemplateInstance* |   
 *Port* | *ComponentRef* | "-" ) [","] } ] *"*)*" "*)*"*

NOTE: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

g) The value in an **apply** operation shall be an expression of a function type but it shall not be the literal name of a function.

***Examples***

**var** MyFuncType v\_func := …;

**apply**(v\_func(MyVar2)); // the function stored in v\_func is applied to MyVar2

Clause 16.2.1 Invoking altsteps

An altstep can be invoked by referring to a value of a behaviour type of kind altstep.

***Syntactical Structure***

**apply** *"*(*" Value "*(*"* [ { ( *TimerRef* | *TemplateInstance* |   
 *Port* | *ComponentRef* | "-" ) [","] } ] *"*)*" "*)*"*

NOTE: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

1. The value in an **apply** operation shall be an expression of an altstep type but it shall not be the literal name of an altstep.

## 5.9 Extension to ETSI ES 201 873-1, clause 19 (Basic program statements)

Clause 19.11 The log statement

Values of behaviour types shall be logged as indicated in the following extension of table 18 TTCN-3 language elements that can be logged.

| Used in a log statement | What is logged | Comment |
| --- | --- | --- |
| behaviour type variable identifier | actual value or "UNINITIALIZED" | See notes 4 and 9. |
| formal parameter identifier | see comment column | In case of behaviour type parameters the actual value shall be logged (see notes 4 and 9). |
| NOTE 4: The string "UNINITIALIZED" is logged only if the log item is unbound (uninitialized).  NOTE 9: For values of behaviour types the name of the definition qualified with the module of its definition shall be logged. For predefined functions the function name only shall be logged. | | |

Values of deferred behaviour types shall be logged as indicated in the following extension of table 18 TTCN-3 language elements that can be logged.

| Used in a log statement | What is logged | Comment |
| --- | --- | --- |
| Deferred behaviour type variable identifier | actual value or "UNINITIALIZED" | See notes 4 and 10. |
| formal parameter identifier | see comment column | In case of deferred behaviour type parameters the actual value shall be logged (see notes 4 and 10). |
| NOTE 4: The string "UNINITIALIZED" is logged only if the log item is unbound (uninitialized).  NOTE 10: For values of deferred behaviour types the name of the definition qualified with the module of its definition shall be logged. For predefined functions the function name only shall be logged. In both cases, additionally, the actual parameter lists of the behaviour value are logged. | | |

## 5.10 Extension to ETSI ES 201 873-1, clause 20 (Statement and operations for alternative behaviours)

Clause 20.5.2 The activate operation

Altsteps can also be activated by referring to a value of an altstep type.

***Syntactical Structure***

**activate** "(" **apply** *"(" Value* "(" [ { ( *TimerRef* | *TemplateInstance* |

*Port* | *ComponentRef* | "-" ) [","] } ] ")" ")" ")"

NOTE 1: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

a) The value in the **apply** operation shall be an expression of an altstep type but it shall not be the literal name of an altstep.

Altsteps can also be activated by referring to a deferred altstep behaviour value.

***Syntactical Structure***

**activate** "(" *VariableRef*")"

NOTE 2: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

a) VariableRef shall refer to a deferred altstep behaviour.

## 5.11 Extension to ETSI ES 201 873-1, clause 21 (Configuration Operations)

Clause 21.2.2 The start test component operation

Functions can also be started on other components by referring to a value of a function type.

***Syntactical Structure***

( *VariableRef* | *FunctionInstance* ) "." **start** "(" **apply** *"(" Value* "("  
 [ { ( *TimerRef* | *TemplateInstance* | *Port* | *ComponentRef* | "-" ) [","] } ]  
 ")" ")"")"

NOTE 1: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

1. The value in the **apply** operation shall be an expression of a function type but it shall not be the literal name of a function.

***Examples***

**function** MyFirstBehaviour() **runs on** MyComponentType { … }

**type** **function** MyBehaviourType () **runs** **on** MyComponentType

:

**var** MyComponentType MyNewPTC;

**var** MyComponentType MyAlivePTC;

**var** MyBehaviourType MyFunction := MyFirstBehaviour;

:

MyNewPTC := MyComponentType.**create**; // Creation of a new non-alive test component.

MyAlivePTC := MyComponentType.**create alive**; // Creation of a new alive-type test component

:

MyAlivePTC.**start**(**apply**(MyFunction())); // Start function indicated by variable MyFunction

Functions can also be started on other components by referring to a deferred function behaviour value.

***Syntactical Structure***

( VariableRef | FunctionInstance ) "." **start** "(" VariableRef")"

NOTE 2: This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option.

***Restrictions***

1. The *VariableRef* given as parameter to the start operation shall refer to a deferred function behaviour.

***Examples***

**function** MyFirstBehaviour() **runs on** MyComponentType { … }

**type** **function** MyBehaviourType **runs** **on** MyComponentType

:

**var** MyComponentType MyNewPTC;

**var** MyComponentType MyAlivePTC;

**var** MyBehaviourType MyFunction := MyFirstBehaviour();

:

MyNewPTC := MyComponentType.**create**; // Creation of a new non-alive test component.

MyAlivePTC := MyComponentType.**create alive**; // Creation of a new alive-type test component

:

MyAlivePTC.**start**(MyFunction); // Start function indicated by variable MyFunction

## 5.12 Extension to ETSI ES 201 873-1, clause 26 (Module control)

Clause 26.1 The execute statement

A testcase can also be executed by referring to a value of a testcase type.

***Syntactical Structure***

This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option:

**execute** "(" **apply** *"*(*" Value* "(" [ { ( *TemplateInstance |* "-" ) [","] } ] ")"

[ "," *TimerValue* ] ")" ")"

***Restrictions***

1. The value in the **apply** operation shall be an expression of a testcase type but it shall not be the literal name of a testcase.

A testcase can also be executed by referring to a deferred testcase behaviour value.

***Syntactical Structure***

This syntactical structure supplements the syntactical structure in ETSI ES 201 873-1 [1] with an alternative option:

**execute** "(" *VariableRef*

[ "," *TimerValue* ] ")" ")"

***Restrictions***

1. The *VariableRef* given as parameter to the **execute** operation shall refer to a deferred testcase behaviour.

## 5.13 Extension to ETSI ES 201 873-1, annex A (BNF and static semantics)

### 5.13.0 New keywords and TTCN-3 syntax BNF productions

New TTCN-3 Keywords

The list of keywords is extended by the following keywords:

**apply**

New TTCN-3 syntax BNF productions

The BNF is extended with the following productions.

NOTE: [AdvancedParameterization] FormalTypeParList is applicable only when the advanced parameterization package [6] is also supported.

785001. BehaviourDef ::= ( AltstepKeyword TypeReference [FormalTypeParList]

[ "("[FunctionFormalParList] ")" ] [RunsOnSpec] [MtcSpec] [SystemSpec] ) |

( FunctionKeyword TypeReference [FormalTypeParList]

[ "("[FunctionFormalParList] ")" ] [RunsOnSpec] [MtcSpec] [SystemSpec]

[ReturnType] ) |

( TestcaseKeyword TypeReference [FormalTypeParList]

[ "("[TemplateOrValueFormalParList] ")"] ConfigSpec StatementBlock)

785002. NestedBehaviourDef ::= ( AltstepKeyword "("[FunctionFormalParList] ")" [RunsOnSpec] [MtcSpec] [SystemSpec] ) |

( FunctionKeyword "("[FunctionFormalParList] ")" [RunsOnSpec] [ReturnType] [MtcSpec] [SystemSpec] ) |

( TestcaseKeyword "("[TemplateOrValueFormalParList] ")"

ConfigSpec StatementBlock)

785003. BehaviourValue ::= ExtendedIdentifier /\*AltstepRef, FunctionRef or TestcaseRef \*/ | "null"

785004. ApplyKeyword ::= "apply"

### 5.13.1 Changes to ETSI ES 201 873-1, clause A.1.6 (TTCN-3 syntax BNF productions)

The following productions from [1] TTCN-3 Core Language clause A.1.6 are modified.

12. StructuredTypeDef ::= RecordDef | UnionDef | SetDef | RecordOfDef | SetOfDef | EnumDef |

PortDef | ComponentDef | MapDef | BehaviourDef

18. NestedTypeDef ::= NestedRecordDef | NestedUnionDef | NestedSetDef |

NestedRecordOfDef | NestedSetOfDef | NestedEnumDef | NestedBehaviourDef

167. RunsOnSpec ::= RunsKeyword OnKeyword ( ComponentType | SelfOp )  
178. FunctionInstance ::= ( FunctionRef ~~[~~ "(" [ActualParList] ")" ~~]~~ ) |  
 ( ApplyKeyword "(" Primary "(" [ActualParList] ")" ")" ) |

( ExtendedIdentifier )

/\* STATIC SEMANTICS – the part is only optional if the *FunctionRef* uses the *ControlKeyword* and the referenced control function has no formal parameters \*/

193. TestcaseInstance ::= ExecuteKeyword "(" ( ExtendedIdentifier ["(" [ActualParList] ")"] ) |  
 ( ApplyKeyword "(" Primary "(" [TestcaseActualParList] ")" ")" )  
 [","(Expression | Minus) ["," SingleExpression]] ")"  
424. PredefinedValue ::= Bstring |

BooleanValue |

CharStringValue |

Number |  /\* IntegerValue \*/

Ostring |

Hstring |

VerdictTypeValue |

FloatValue |

AddressValue |

OmitKeyword |

BehaviourValue

# 6 Package semantics

## 6.1 Replacements

The following clauses shall replace the following clauses in ETSI ES 201 873-4 [2] (V4.4.1):

* Clause 6.2 replaces clause 9.2 Activate statement in ETSI ES 201 873-4 [2] (V4.4.1).
* Clause 6.3.0 replaces the main text part of clause 9.17 Execute statement in ETSI ES 201 873-4 [2] (V4.4.1).
* Clause 6.3.1 replaces clause 9.17.1 Flow graph segment <execute-without-timeout> in ETSI ES 201 873‑4 [2] (V4.4.1).
* Clause 6.4.0 replaces the main text part of clause 9.24 Function call in ETSI ES 201 873-4 [2] (V4.4.1).
* Clause 6.4.1 replaces clause 9.24.4 Flow graph segment <user-def-func-call> in ETSI ES 201 873-4 [2] (V4.4.1).
* Clause 6.4.2 replaces clause 9.24.5 Flow graph segment <predef-ext-func-call> in ETSI ES 201 873-4 [2] (V4.4.1).
* Clause 6.5 replaces clause 9.46 Start component operation in ETSI ES 201 873-4 [2] (V4.4.1).

In the clauses 6.2 to 6.5 all figure numbers, figure references and clause references are related to the clauses and figures in ETSI ES 201 873-4 [2] (V4.4.1) and not to any clause or figure in the present document.

## 6.2 Activate statement

The syntactical structure of the **activate** statement is:

**activate**(<altstep-name>([<act-par-desc1>, … , <act-par-descn>])) |  
 **activate**(**apply**(<altstep-expr>([<act-par-desc1>, … , <act-par-descn>]))) |

**activate**(<deferred-altstep-behaviour>)

The <altstep-name> and the <altstep-expr> denote the identifier of the altstep that is activated as default behaviour, and <act‑par‑descr1>, … , <act-par-descrn> describe the actual parameter values of the altstep at the time of its activation. The <deferred-altstep-behaviour> denotes a reference to a deferred altstep behaviour. The operational semantics assumes that <altstep-name> is a literal name of the altstep type and can be handled like the <altstep-expr>, i.e. as an expression that evaluates to a value of the altstep behaviour type. Furthermore, it is assumed that for each <act-par-desc1> the corresponding formal parameter identifier <f‑par-Id1> is known, i.e. the syntactical structure above can be extended to:

**activate**(<altstep-name>((<f-par-Id1>,<act-par-desc1>), … , (<f-par-Idn>,<act‑par-descn>))) |

**activate**(**apply**(<altstep-expr> ((<f-par-Id1>,<act-par-desc1>), … , (<f-par-Idn>,<act‑par-descn>))))

The flow graph segment <activate-stmt> in figure 37 defines the execution of the **activate** statement. The execution is structured into four steps. In the first step, the identifier of the altstep to be activated is determined. The identifier may directly be given by an altstep name or be given in form of an expression that evaluates to the altstep identifier. In the second step, a call record for the altstep is created. In the third step the values of the actual parameter are calculated and assigned to the corresponding field in the call record. In the fourth step, the call record is put as first element in the *DEFAULT-LIST* of the entity that activates the default.

NOTE: For altsteps that are activated as default behaviour, only value parameters are allowed. In figure 37, the handling of the value parameters is described by the flow graph segment <value-par-calculation>, which is defined in clause 9.24.1.



Figure 37: Flow graph segment <activate-stmt>

## 6.3 Replacements in Execute statement's operational semantics

### 6.3.0 Execute statement

The syntactical structure of the **execute** statement is:

**execute**(<testCaseId>([<act-par1>, … , <act-parn>)]) [, <float-expression>]) |

**execute**(**apply**(<testCase-expr>([<act-par1>, … , <act-parn>)]) [, <float-expression>])) |

**execute**(<deferred-testCase-behaviour> [, <float-expression>])

The **execute** statement describes the execution of a test case that is identified by a <testCaseId> or a <testCase-expr> with the (optional) actual parameters <act-par1>, … , <act-parn> or a <deferred-testcase-behaviour> which denotes a reference to a deferred testcase behaviour. Optionally the execute statement may be guarded by a duration provided in form of an expression that evaluates to a **float**. If within the specified duration the test case does not return a verdict, a timeout exception occurs, the test case is stopped and an **error** verdict is returned.

NOTE: The operational semantics models the stopping of the test case by a stop of the MTC. In reality, other mechanisms may be more appropriate.

If no timeout exception occurs, the MTC is created, the control instance (representing the control part of the TTCN‑3 module) is blocked until the test case terminates, and for the further test case execution the flow of control is given to the MTC. The flow of control is given back to the control instance when the MTC terminates.

The flow graph segment <execute-stmt> in figure 67 defines the execution of an **execute** statement.



Figure 67: Flow graph segment <execute-stmt>

### 6.3.1 Flow graph segment <execute-without-timeout>

The execution of a test case starts with the creation of the **mtc**. Then the mtc is started with the behaviour defined in the test case definition. Afterwards, the module control waits until the test case terminates. The creation and the start of the MTC can be described by using **create** and **start** statements:

**var** MtcType myMTC := MtcType.**create**;

myMTC.**start**(TestCaseName(P1…Pn));

or, if the testcase is identified by a behaviour expression:

**var** MtcType myMTC := MtcType.**create**;

myMTC.**start**(**apply**(myTestCaseVar (P1…Pn)));

NOTE 1: For the replacements sketched above, the operational semantics assumes that all referenced definitions (e.g. MtcType, TestCaseName, myTestCaseVar) exist and that all definitions which are needed for the referenced definitions also exist (e.g. a testcase behaviour type definition for myTestCaseVar).

NOTE 2: For the case where the test case is identified by a behaviour expression, the operational semantics assumes for the replacement sketched above that the type of the MTC MtcType is referenced in the **runs on** clause of the behaviour type definition of variable myTestCaseVar.

The flow graph segment <execute-without-timeout> in figure 68 defines the execution of an **execute** statement without the occurrence of a timeout exception by using the flow graph segments of the operations **create** and the **start**.



Figure 68: Flow graph segment <execute-without-timeout>

## 6.4 Replacements in Function call's operational semantics

### 6.4.0 Function call

The syntactical structure of a function call is:

<function-name>([<act-par-desc1>, … , <act-par-descn>]) |

**apply**(<function-expr>([<act-par-desc1>, … , <act-par-descn>])

The <function-name> and the <function-expr> denote to the identifier of the function that is invoked. The operational semantics assumes that <function-name> is a literal value of the function behaviour type. <act‑par-descr1>, … , <act-par-descrn> describe the actual parameter values of the function call.

NOTE 1: A function call and an altstep call are handled in the same manner. Therefore, the altstep call (see clause 9.4 in ETSI ES 201 873-4 [2]) refers to this clause.

Furthermore, it is assumed that for each <act-par-desc1> the corresponding formal parameter identifier   
<f-par-Id1> is known, i.e. the syntactical structure above can be extended to:

<function-name>((<f-par-Id1>,<act-par-desc1>), … , (<f-par-Idn>,<act‑par-descn>)) |

**apply**(<function-expr>((<f-par-Id1>,<act-par-desc1>), … , (<f-par-Idn>,<act‑par-descn>)))

The flow graph segment <function-call> in figure 80 defines the execution of a function call. The execution is structured into three steps. In the first step, the identifier of the function to be called is determined. The identifier may directly be given by the function name or be given in form of an expression that evaluates to the function identifier. In the second step, a call record for the function is created. In the third step the values of the actual parameter are calculated and assigned to the corresponding fields in the call record. In the fourth step, the parameters called by reference are handled. In the fifth step, two situations have to be distinguished: the called function is a user-defined function (<user‑def‑func‑call>), i.e. there exists a flow graph representation for the function, or the called function is a pre-defined or external function (<predef-ext-func-call>). In case of a user-defined function call, the control is given to the called function. In case of a pre-defined or external function, it is assumed that the call record can be used to execute the function in one step. The correct handling of reference parameters and return value (has to be pushed onto the value stack) is in the responsibility of the called function, i.e. is outside the scope of this operational semantics.

NOTE 2: If the function call models an altstep call, only the <user-def-func-call> branch will be chosen, because there exists a flow graph representation of the called altstep.

NOTE 3: The <function call> segment is also used to describe the start of the MTC in an **execute** statement. In this case, a call record for the test case is constructed and only the <user‑def‑func‑call> branch will be chosen.



Figure 80: Flow graph segment <function-call>

### 6.4.1 Flow graph segment <user-def-func-call>

The flow graph-segment <user-def-func-call> (figure 84) describes the transfer of control to a called user‑defined function.



Figure 84: Flow graph segment <user-def-func-call>

### 6.4.2 Flow graph segment <predef-ext-func-call>

The flow graph-segment <predef-ext-func-call> (figure 85) describes the call of a pre-defined or external function.

NOTE: In figure 85, it is assumed that the call record can be used to execute the pre-defined or external function in one step.



Figure 85: Flow graph segment <predef-ext-func-call>

## 6.5 Start component operation

The syntactical structure of the **start** component operation is:

<component-expression>**.start**(<function-name>(<act-par-desc1>,…, <act-par-descn>)) |

<component-expression>**.start**(**apply**(<function-expr>(<act-par-desc1>,…, <act-par-descn>))) |

<component-expression>**.start**(<deferred-function-behaviour>)

The **start** component operation starts a component. Using a component reference identifies the component to be started. The reference may be stored in a variable or be returned by a function, i.e. it is an expression that evaluates to a component reference.

The <function-name> and the <function-expr> denote the identifier of the function that defines the behaviour of the new component. <deferred-function-behaviour> denotes a reference to a deferred function behaviour. The operational semantics assumes that <function-name> is a literal name of a function and can be handled like the <function-expr>, i.e. as an expression that evaluates to a value of the function behaviour type. <act-par-descr1>, …, <act-par-descrn> provide the description of the actual parameter values of the function. The descriptions of the actual parameters are provided in form of expressions that have to be evaluated before the call can be executed. The handling of formal and actual value parameters is similar to their handling in function calls (see clause 9.24 in ETSI ES 201 873-4 [2]).

The flow graph segment <start-component-op> in figure 120 defines the execution of the **start** component operation. The start component operation is executed in five steps. In the first step, the identifier of the function to be started is determined. In the second step, a call record is created. In the third step the actual parameter values are calculated. In the fourth step the reference of the component to be started is retrieved, and, in the fifth step, control and call record are given to the new component.

NOTE: The flow graph segment in figure 120 includes the handling of reference parameters (<ref‑var‑par‑calc>). Reference parameters are needed to explain reference parameters of test cases. The operational semantics assumes that these parameters are handled by the MTC.



Figure 120: Flow graph segment <start-component-op>

# 7 TRI extensions for the package

This package does not have an effect on TRI.

# 8 TCI extensions for the package

## 8.1 Extensions to ETSI ES 201 873-6, clause 7 (TTCN-3 control interface and operations)

Clause 7.2.2.1 Abstract TTCN-3 data types

Three additional type classes are used to distinguish the three kinds of behaviours: ALTSTEP, FUNCTION and TESTCASE They are also used for deferred altstep, function and testcase behaviour values, respectively.

TciTypeClassType getTypeClass() Returns the type class of the respective type. A value of TciTypeClassType can have one of the following constants: ADDRESS, ALTSTEP, ANYTYPE, BITSTRING, BOOLEAN, CHARSTRING, COMPONENT, ENUMERATED, FLOAT, FUNCTION, HEXSTRING, INTEGER, OBJID, OCTETSTRING, RECORD, RECORD\_OF, SET, SET\_OF, TESTCASE, UNION, UNIVERSAL\_CHARSTRING, VERDICT.

Clause 7.2.2.2 Abstract TTCN-3 values

Clause 7.2.2.2 Abstract TTCN-3 values is extended by figure 4.



Figure 4: Hierarchy of abstract values

7.2.2.2.16 The abstract data type BehaviourValue

The following operations are defined on the base abstract data type BehaviourValue, which is used to represent both behaviour values and deferred behaviour values. The concrete representations of these operations are defined in the respective language mapping sections:

Value getName() Returns the name of the behaviour.

TciModuleIdType getDefiningModule() Returns the module identifier of the module in which the behaviour is defined. Returns the distinct value null if the behaviour is a predefined function.

## 8.2 Extensions to ETSI ES 201 873-6, clause 8 (Java language mapping)

Clause 8.3.2.4 TciTypeClassType

Clause 8.3.2.4 TciTypeClassType shall be extended as follows:

**TciTypeClassType** is mapped to the following interface:

// TCI IDL TciTypeClassType

package org.etsi.ttcn.tci;

public interface TciTypeClass {

public final static int ADDRESS = 0 ;

public final static int ANYTYPE = 1 ;

public final static int BITSTRING = 2 ;

public final static int BOOLEAN = 3 ;

public final static int CHARSTRING = 5 ;

public final static int COMPONENT = 6 ;

public final static int ENUMERATED = 7 ;

public final static int FLOAT = 8 ;

public final static int HEXSTRING = 9 ;

public final static int INTEGER = 10 ;

public final static int OBJID = 11 ;

public final static int OCTETSTRING = 12 ;

public final static int RECORD = 13 ;

public final static int RECORD\_OF = 14 ;

public final static int SET = 15 ;

public final static int SET\_OF = 16 ;

public final static int UNION = 17 ;

public final static int UNIVERSAL\_CHARSTRING = 19 ;

public final static int VERDICT = 20 ;

public final static int ALTSTEP = 21 ;

public final static int FUNCTION = 22 ;

public final static int TESTCASE = 23 ;

}

Clause 8.3.4 Abstract value mapping

Clause 8.3.4 Abstract value mapping shall be extended by:

8.3.4.16 BehaviourValue

**BehaviourValue** is mapped to the following interface:

// TCI IDL Type

package org.etsi.ttcn.tci;

public interface BehaviourValue {

public String getName ();

public TciModuleId getDefiningModule ();

}

**Methods:**

* getName() Returns the name of the behaviour as defined in the TTCN‑3 module.
* getDefiningModule() Returns the module identifier of the module the behaviour has been defined in.

## 8.3 Extensions to ETSI ES 201 873-6, clause 9 (ANSI C language mapping)

Clause 9.2 Value Interfaces

Clause 9.2 Value Interfaces shall be extended by:

| TCI IDL Interface | ANSI C representation | Notes and comments |
| --- | --- | --- |
| BehaviourValue | | |
| Value getName() | Value tciName(Value inst) | Returns the name of the behaviour as a CharstringValue. |
| TciModuleIdType getDefiningModule() | TciModuleIdType tciDefiningModule  (Value inst) | Returns the module identifier of the module in which the behaviour is defined. The module identifier will be empty in case the behaviour is a predefined function. |

Clause 9.5 Data

Clause 9.5 Data shall be extended by:

| TCI IDL ADT | ANSI C representation (Type definition) | Notes and comments |
| --- | --- | --- |
| TciTypeClassType | typedef enum  {  TCI\_ADDRESS\_TYPE,  TCI\_ANYTYPE\_TYPE,  TCI\_BITSTRING\_TYPE,  TCI\_BOOLEAN\_TYPE,  TCI\_CHAR\_TYPE,  TCI\_CHARSTRING\_TYPE,  TCI\_COMPONENT\_TYPE,  TCI\_ENUMERATED\_TYPE,  TCI\_FLOAT\_TYPE,  TCI\_HEXSTRING\_TYPE,  TCI\_INTEGER\_TYPE,  TCI\_OBJID\_TYPE,  TCI\_OCTETSTRING\_TYPE,  TCI\_RECORD\_TYPE,  TCI\_RECORD\_OF\_TYPE,  TCI\_SET\_TYPE,  TCI\_SET\_OF\_TYPE,  TCI\_UNION\_TYPE,  TCI\_UNIVERSAL\_CHAR\_TYPE,  TCI\_UNIVERSAL\_CHARSTRING\_TYPE,  TCI\_VERDICT\_TYPE,  TCI\_ALTSTEP\_TYPE,  TCI\_FUNCTION\_TYPE,  TCI\_TESTCASE\_TYPE  } TciTypeClassType; | TCI\_ALTSTEP\_TYPE, TCI\_FUNCTION\_TYPE, and TCI\_TESTCASE\_TYPE added. |

## 8.4 Extensions to ETSI ES 201 873-6, clause 10 (C++ language mapping)

Clause 10.5.2.14 TciTypeClass

Clause 10.5.2.14 TciTypeClass shall be extended by the three behaviour type classes as follows:

Defines the different type classes in TTCN-3 (i.e. boolean, float, etc.). It is mapped to the following pure virtual class:

class TciTypeClass {

public:

static const TciTypeClass TCI\_ADDRESS

static const TciTypeClass TCI\_ANYTYPE

static const TciTypeClass TCI\_BITSTRING

static const TciTypeClass TCI\_BOOLEAN

static const TciTypeClass TCI\_CHARSTRING

static const TciTypeClass TCI\_COMPONENT

static const TciTypeClass TCI\_ENUMERATED

static const TciTypeClass TCI\_FLOAT

static const TciTypeClass TCI\_HEXSTRING

static const TciTypeClass TCI\_INTEGER

static const TciTypeClass TCI\_OCTETSTRING

static const TciTypeClass TCI\_RECORD

static const TciTypeClass TCI\_RECORD\_OF

static const TciTypeClass TCI\_ARRAY

static const TciTypeClass TCI\_SET

static const TciTypeClass TCI\_SET\_OF

static const TciTypeClass TCI\_UNION

static const TciTypeClass TCI\_UNIVERSAL\_CHARSTRING

static const TciTypeClass TCI\_VERDICT

static const TciTypeClass TCI\_ALTSTEP

static const TciTypeClass TCI\_FUNCTION

static const TciTypeClass TCI\_TESTCASE

~TciTypeClass ()

Tboolean equals (const TciTypeClass &p\_other) const

Tstring toString () const

Tinteger getTypeClass() const

}

Clause 10.5.3 Abstract TTCN-3 data types and values

Clause 10.5.3 Abstract TTCN-3 data types and valuesshall be extended by:

10.5.3.18 BehaviourValue

A value of BehaviourValue represents an altstep, function or testcase in a TTCN-3 module. It is mapped to the following pure virtual class:

class BehaviourValue {

public:

virtual ~BehaviourValue ();

virtual const TciModuleId & getDefiningModule () const =0;

virtual const Tstring & getName () const =0;

virtual Tboolean equals (const BehaviourValue &behVal) const =0;

virtual BehaviourValue \* cloneBehaviourValue () const =0;

virtual Tboolean operator< (const BehaviourValue &behVal) const =0;

}

10.5.3.18.1 Methods

* ~TciType ()

Destructor.

* getDefiningModule ()

Return the defining module as defined in the TTCN-3 ATS.

* getName ()

Return behaviour name as defined in the ATS.

* equals (const BehaviourValue &behVal)

Return true if the behaviours are equal.

* cloneType ()

Return a copy of the BehaviourValue.

* operator< (const BehaviourValue &behVal)

Operator < overload.

## 8.5 Extensions to ETSI ES 201 873-6, clause 11 (W3C XML mapping)

Clause 11.3.3.1 Value

Clause 11.3.3.1 Value shall be extended by:

**Value** is mapped to the following complex type:

<xsd:complexType name="Value" mixed="true">

<xsd:choice>

<xsd:element name="integer" type="Values:IntegerValue"/>

<xsd:element name="float" type="Values:FloatValue"/>

<xsd:element name="boolean" type="Values:BooleanValue"/>

<xsd:element name="verdicttype" type="Values:VerdictValue"/>

<xsd:element name="bitstring" type="Values:BitstringValue"/>

<xsd:element name="hexstring" type="Values:HexstringValue"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"/>

<xsd:element name="charstring" type="Values:CharstringValue"/>

<xsd:element name="universal\_charstring" type="Values:UniversalCharstringValue"/>

<xsd:element name="record" type="Values:RecordValue"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"/>

<xsd:element name="array" type="Values:ArrayValue"/>

<xsd:element name="set" type="Values:SetValue"/>

<xsd:element name="set\_of" type="Values:SetOfValue"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"/>

<xsd:element name="union" type="Values:UnionValue"/>

<xsd:element name="anytype" type="Values:AnytypeValue"/>

<xsd:element name="address" type="Values:AddressValue"/>

<xsd:element name="behaviour" type="Values:BehaviourValue"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

<xsd:attributeGroup name="ValueAtts">

<xsd:attribute name="name" type="SimpleTypes:TString" use="optional"/>

<xsd:attribute name="type" type="SimpleTypes:TString" use="optional"/>

<xsd:attribute name="module" type="SimpleTypes:TString" use="optional"/>

<xsd:attribute name="annotation" type="SimpleTypes:TString" use="optional"/> </xsd:attributeGroup>

**Choice of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.

**Attributes:**

* name The name of the value, if known.
* type The type of the value, if known.
* module The module of the value, if known.
* annotation A helper attribute to provide additional matching/mismatching information, etc.

11.3.3.24b BehaviourValue

**BehaviourValue** is mapped to the following complex type:

<xsd:complexType name="BehaviourValue">

<xsd:sequence>

<xsd:element name="name" type="Types:QualifiedName"/>

</xsd:sequence>

</xsd:complexType>

**Elements:**

* name The qualified name of the behaviour.

**Attributes:**

* none.

Clause 11.3.3.12 RecordValue

All clauses for structured values are to be extended with an element for a BehaviourValue.

11.3.3.12 RecordValue

**RecordValue** is mapped to the following complex type:

<xsd:complexType name="RecordValue">

<xsd:choice>

<xsd:choice minOccurs="0" maxOccurs="unbounded">

<xsd:element name="integer" type="Values:IntegerValue"/>

<xsd:element name="float" type="Values:FloatValue"/>

<xsd:element name="boolean" type="Values:BooleanValue"/>

<xsd:element name="verdicttype" type="Values:VerdictValue"/>

<xsd:element name="bitstring" type="Values:BitstringValue"/>

<xsd:element name="hexstring" type="Values:HexstringValue"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"/>

<xsd:element name="charstring" type="Values:CharstringValue"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue"/>

<xsd:element name="record" type="Values:RecordValue"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"/>

<xsd:element name="array" type="Values:ArrayValue"/>

<xsd:element name="set" type="Values:SetValue"/>

<xsd:element name="set\_of" type="Values:SetOfValue"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"/>

<xsd:element name="union" type="Values:UnionValue"/>

<xsd:element name="anytype" type="Values:AnytypeValue"/>

<xsd:element name="address" type="Values:AddressValue"/>

<xsd:element name="behaviour" type="Values:BehaviourValue"/>

</xsd:choice>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd: choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Sequence of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.
* null If no field is given.
* omit If the field is omitted.

**Attributes:**

* The same attributes as those of Value.

11.3.3.13 RecordOfValue

**RecordOfValue** is mapped to the following complex type:

<xsd:complexType name="RecordOfValue">

<xsd:choice>

<xsd:element name="integer" type="Values:IntegerValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="float" type="Values:FloatValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="boolean" type="Values:BooleanValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="verdicttype" type="Values:VerdictValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="bitstring" type="Values:BitstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="hexstring" type="Values:HexstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="charstring" type="Values:CharstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record" type="Values:RecordValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="array" type="Values:ArrayValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="set" type="Values:SetValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="set\_of" type="Values:SetOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="union" type="Values:UnionValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="anytype" type="Values:AnytypeValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="address" type="Values:AddressValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="behaviour" type="Values:BehaviourValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Choice of Sequence of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.
* null If no field is given.
* omit If the field is omitted.

**Attributes:**

* The same attributes as those of Value.

11.3.3.14 ArrayValue

**ArrayValue** is mapped to the following complex type:

<xsd:complexType name="ArrayValue">

<xsd:choice>

<xsd:element name="integer" type="Values:IntegerValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="float" type="Values:FloatValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="boolean" type="Values:BooleanValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="verdicttype" type="Values:VerdictValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="bitstring" type="Values:BitstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="hexstring" type="Values:HexstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="charstring" type="Values:CharstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record" type="Values:RecordValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="array" type="Values:ArrayValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="set" type="Values:SetValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="set\_of" type="Values:SetOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="union" type="Values:UnionValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="anytype" type="Values:AnytypeValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="address" type="Values:AddressValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="behaviour" type="Values:BehaviourValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Choice of Sequence of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.
* null If no field is given.
* omit If the field is omitted.

**Attributes:**

* The same attributes as those of Value.

11.3.3.15 SetValue

**SetValue** is mapped to the following complex type:

<xsd:complexType name="SetValue">

<xsd:choice>

<xsd:choice minOccurs="0" maxOccurs="unbounded">

<xsd:element name="integer" type="Values:IntegerValue"/>

<xsd:element name="float" type="Values:FloatValue"/>

<xsd:element name="boolean" type="Values:BooleanValue"/>

<xsd:element name="verdicttype" type="Values:VerdictValue"/>

<xsd:element name="bitstring" type="Values:BitstringValue"/>

<xsd:element name="hexstring" type="Values:HexstringValue"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"/>

<xsd:element name="charstring" type="Values:CharstringValue"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue"/>

<xsd:element name="record" type="Values:RecordValue"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"/>

<xsd:element name="array" type="Values:ArrayValue"/>

<xsd:element name="set" type="Values:SetValue"/>

<xsd:element name="set\_of" type="Values:SetOfValue"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"/>

<xsd:element name="union" type="Values:UnionValue"/>

<xsd:element name="anytype" type="Values:AnytypeValue"/>

<xsd:element name="address" type="Values:AddressValue"/>

<xsd:element name="behaviour" type="Values:BehaviourValue"/>

</xsd:choice>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Sequence of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.
* null If no field is given.
* omit If the field is omitted.

**Attributes:**

* The same attributes as those of Value.

11.3.3.16 SetOfValue

**SetOfValue** is mapped to the following complex type:

<xsd:complexType name="SetOfValue">

<xsd:choice>

<xsd:element name="integer" type="Values:IntegerValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="float" type="Values:FloatValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="boolean" type="Values:BooleanValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="verdicttype" type="Values:VerdictValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="bitstring" type="Values:BitstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="hexstring" type="Values:HexstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="charstring" type="Values:CharstringValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record" type="Values:RecordValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="array" type="Values:ArrayValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="set" type="Values:SetValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="set\_of" type="Values:SetOfValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"

minOccurs="0" maxOccurs="unbounded"/>

<xsd:element name="union" type="Values:UnionValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="anytype" type="Values:AnytypeValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="address" type="Values:AddressValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="behaviour" type="Values:BehaviourValue" minOccurs="0"

maxOccurs="unbounded"/>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/> </xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Choice of Sequence of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.
* null If no field is given.
* omit If the field is omitted.

**Attributes:**

* The same attributes as those of Value.

11.3.3.18 UnionValue

**UnionValue** is mapped to the following complex type:

<xsd:complexType name="UnionValue">

<xsd:choice>

<xsd:element name="integer" type="Values:IntegerValue"/>

<xsd:element name="float" type="Values:FloatValue"/>

<xsd:element name="boolean" type="Values:BooleanValue"/>

<xsd:element name="verdicttype" type="Values:VerdictValue"/>

<xsd:element name="bitstring" type="Values:BitstringValue"/>

<xsd:element name="hexstring" type="Values:HexstringValue"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"/>

<xsd:element name="charstring" type="Values:CharstringValue"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue"/>

<xsd:element name="record" type="Values:RecordValue"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"/>

<xsd:element name="array" type="Values:ArrayValue"/>

<xsd:element name="set" type="Values:SetValue"/>

<xsd:element name="set\_of" type="Values:SetOfValue"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"/>

<xsd:element name="union" type="Values:UnionValue"/>

<xsd:element name="anytype" type="Values:AnytypeValue"/>

<xsd:element name="address" type="Values:AddressValue"/>

<xsd:element name="behaviour" type="Values:BehaviourValue"/>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Choice of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* anytype An anytype value.
* address An address value.
* behaviour A behaviour value.

**Attributes:**

* The same attributes as those of Value.

11.3.3.19 AnytypeValue

**AnytypeValue** is mapped to the following complex type:

<xsd:complexType name="AnytypeValue">

<xsd:choice minOccurs="0" maxOccurs="unbounded">

<xsd:element name="integer" type="Values:IntegerValue"/>

<xsd:element name="float" type="Values:FloatValue"/>

<xsd:element name="boolean" type="Values:BooleanValue"/>

<xsd:element name="verdicttype" type="Values:VerdictValue"/>

<xsd:element name="bitstring" type="Values:BitstringValue"/>

<xsd:element name="hexstring" type="Values:HexstringValue"/>

<xsd:element name="octetstring" type="Values:OctetstringValue"/>

<xsd:element name="charstring" type="Values:OctetstringValue"/>

<xsd:element name="universal\_charstring"

type="Values:UniversalCharstringValue"/>

<xsd:element name="record" type="Values:RecordValue"/>

<xsd:element name="record\_of" type="Values:RecordOfValue"/>

<xsd:element name="array" type="Values:ArrayValue"/>

<xsd:element name="set" type="Values:SetValue"/>

<xsd:element name="set\_of" type="Values:SetOfValue"/>

<xsd:element name="enumerated" type="Values:EnumeratedValue"/>

<xsd:element name="union" type="Values:UnionValue"/>

<xsd:element name="address" type="Values:AddressValue"/>

<xsd:element name="behaviour" type="Values:BehaviourValue"/>

<xsd:element name="null" type="Templates:null"/>

<xsd:element name="omit" type="Templates:omit"/>

</xsd:choice>

<xsd:attributeGroup ref="Values:ValueAtts"/>

</xsd:complexType>

**Choice of Elements:**

* integer An integer value.
* float A float value.
* boolean A boolean value.
* verdicttype A verdicttype value.
* bitstring A bitstring value.
* hexstring An hexstring value.
* octetstring An octetstring value.
* charstring A charstring value.
* universal\_charstring A universal charstring value.
* record A record value.
* record\_of A record of value.
* array An array value.
* set A set value.
* set\_of A set of value.
* enumerated An enumerated value.
* union A union value.
* address An address value.
* behaviour A behaviour value.

**Attributes:**

* The same attributes as those of Value.

# 9 Extensions to TTCN-3 documentation comment specification for the package

## 9.1 Extensions to ETSI ES 201 873-10, annex A (where Tags can be used)

Add ", function behaviour types" to the cell "Functions (TTCN‑3 and external)", ", altstep behaviour types" to the cell "Altsteps" and ", test case behaviour types" to the cell "Test cases" in the header of table A.1 of [7].

Table A.1 shows an example for the extended table A.1. Note that other packages may also extend the same table. Underlined character shows the insertions by this package.

Table A.: Relation of documentation tags and TTCN-3

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Simple Data Types | Structured Data Types | Component Types | Port Types | Modulepars | Constants | Templates | Signatures | Functions (TTCN‑3 and external) , function behaviour types | Altsteps, altstep behaviour types | Test Cases, test case behaviour types | Modules | Groups | Control Parts | Component local definitions | Used in implicit form (see clause 7) | Embedded in other tags | |
| @author | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| @config |  |  |  |  |  |  |  |  |  |  | X |  |  |  |  |  |  | |
| @desc | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| @exception |  |  |  |  |  |  |  | X |  |  |  |  |  |  |  | X |  | |
| @member |  | X1 | X | X | X1 | X1 | X1 |  |  |  |  |  |  |  |  | X |  | |
| @param |  |  |  |  |  |  | X | X | X | X | X |  |  |  |  | X |  | |
| @priority |  |  |  |  |  |  |  |  |  |  | X |  |  |  |  |  |  | |
| @purpose |  |  |  |  |  |  |  |  |  |  | X | X |  |  |  |  |  | |
| @remark | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| @reference | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| **@**requirement |  |  |  |  |  |  |  |  | X | X | X | X |  |  |  |  |  | |
| @return |  |  |  |  |  |  |  | X | X |  |  |  |  |  |  | X |  | |
| @see | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  | X | |
| @since | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| @status | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| @url | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  | X | |
| @verdict |  |  |  |  |  |  |  |  | X | X | X | X |  |  |  |  |  | |
| @version | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X |  |  | |
| NOTE: 1 Preceding language elements of record, set, union or enumerated types only. | | | | | | | | | | | | | | | | | |

# History

|  |  |  |
| --- | --- | --- |
| **Document history** | | |
| V1.1.1 | January 2010 | Publication |
| V1.2.1 | May 2011 | Publication |
| V1.3.1 | April 2013 | Publication |
| V1.4.1 | June 2015 | Publication |
| V1.5.1 | August 2017 | Publication |
| V1.6.1 | May 2018 | Publication |
| V1.7.1 | May 2020 | Publication |
| V1.8.1 | June 2021 | Publication |
| V1.9.1 | February 2022 | Membership Approval Procedure MV 20220429: 2022-02-28 to 2022-04-29 |
| V1.9.1 | May 2022 | Publication |