ETSI ES 201 873-5 V4.8.2 (2021-12)

Methods for Testing and Specification (MTS);

The Testing and Test Control Notation version 3;

Part 5: TTCN-3 Runtime Interface (TRI)

**ETSI Standard**

Reference

RES/MTS-201873-5 T3ed481TRI

Keywords

interface, methodology, runtime, testing, TRI, TTCN-3

***ETSI***

650 Route des Lucioles

F-06921 Sophia Antipolis Cedex - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Siret N° 348 623 562 00017 - NAF 742 C

Association à but non lucratif enregistrée à la

Sous-Préfecture de Grasse (06) N° 7803/88

***Important notice***

The present document can be downloaded from:  
<http://www.etsi.org/standards-search>

The present document may be made available in electronic versions and/or in print. The content of any electronic and/or print versions of the present document shall not be modified without the prior written authorization of ETSI. In case of any existing or perceived difference in contents between such versions and/or in print, the only prevailing document is the print of the Portable Document Format (PDF) version kept on a specific network drive within ETSI Secretariat.

Users of the present document should be aware that the document may be subject to revision or change of status. Information on the current status of this and other ETSI documents is available at <https://portal.etsi.org/TB/ETSIDeliverableStatus.aspx>

If you find errors in the present document, please send your comment to one of the following services:  
<https://portal.etsi.org/People/CommiteeSupportStaff.aspx>

***Copyright Notification***

No part may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm except as authorized by written permission of ETSI.  
The content of the PDF version shall not be modified without the written authorization of ETSI.  
The copyright and the foregoing restriction extend to reproduction in all media.

© European Telecommunications Standards Institute 2017.

All rights reserved.

**DECT**TM, **PLUGTESTS**TM, **UMTS**TM and the ETSI logo are Trade Marks of ETSI registered for the benefit of its Members.  
**3GPP**TM and **LTE**™ are Trade Marks of ETSI registered for the benefit of its Members and  
of the 3GPP Organizational Partners.  
**oneM2M** logo is protected for the benefit of its Members  
**GSM**® and the GSM logo are Trade Marks registered and owned by the GSM Association.

Contents

Intellectual Property Rights 8

Foreword 8

Modal verbs terminology 8

Introduction 8

1 Scope 9

1.1 Scope of the present document 9

1.2 Compliance 9

2 References 9

2.1 Normative references 9

2.2 Informative references 10

3 Definitions and abbreviations 10

3.1 Definitions 10

3.2 Abbreviations 11

4 General Structure of a TTCN‑3 Test System 12

4.1 Entities in a TTCN‑3 test system 12

4.1.0 Types of entities 12

4.1.1 Test Management and Control (TMC) 12

4.1.1.0 Test Management and Control Entities 12

4.1.1.1 Test Management (TM) 13

4.1.1.2 Test Logging (TL) 13

4.1.1.3 Coding and Decoding (CD) 13

4.1.1.4 Component Handling (CH) 13

4.1.2 TTCN‑3 Executable (TE) 13

4.1.2.0 TTCN-3 Executable Entity 13

4.1.2.1 Executable Test Suite (ETS) 13

4.1.2.2 TTCN‑3 RunTime System (T3RTS) 13

4.1.2.3 Encoding/Decoding System (EDS) 14

4.1.2.4 Timers in the TTCN‑3 Executable 14

4.1.3 SUT Adaptor (SA) 14

4.1.4 Platform Adaptor (PA) 14

4.2 Interfaces in a TTCN‑3 Test System 15

4.3 Execution requirements for a TTCN‑3 test system 15

5 TTCN‑3 Runtime Interface and operations 15

5.1 Overview of the TRI 15

5.1.0 Sub-interfaces 15

5.1.1 The triCommunication Interface 16

5.1.2 The triPlatform Interface 16

5.1.3 Correlation between TTCN‑3 and TRI Operation Invocations 16

5.2 Error handling 17

5.2.0 Basic rules 17

5.2.1 triSAErrorReq (SA → TE) 18

5.2.2 triPAErrorReq (PA → TE) 18

5.3 Data interface 18

5.3.0 Basic rules 18

5.3.1 Connection 18

5.3.2 Communication 19

5.3.3 Timer 20

5.3.4 Miscellaneous 20

5.4 Operation descriptions 20

5.5 Communication interface operations 20

5.5.1 triSAReset (TE → SA) 20

5.5.2 Connection handling operations 21

5.5.2.1 triExecuteTestCase (TE → SA) 21

5.5.2.2 triMap (TE → SA) 21

5.5.2.3 triMapParam (TE → SA) 21

5.5.2.4 triUnmap (TE → SA) 22

5.5.2.5 triUnmapParam (TE → SA) 22

5.5.2.6 triEndTestCase (TE → SA) 22

5.5.3 Message based communication operations 23

5.5.3.1 triSend (TE → SA) 23

5.5.3.2 triSendBC (TE → SA) 23

5.5.3.3 triSendMC (TE → SA) 24

5.5.3.4 triEnqueueMsg (SA → TE) 24

5.5.4 Procedure based communication operations 25

5.5.4.1 triCall (TE → SA) 25

5.5.4.2 triCallBC (TE → SA) 26

5.5.4.3 triCallMC (TE → SA) 27

5.5.4.4 triReply (TE → SA) 28

5.5.4.5 triReplyBC (TE → SA) 29

5.5.4.6 triReplyMC (TE → SA) 30

5.5.4.7 triRaise (TE → SA) 30

5.5.4.8 triRaiseBC (TE → SA) 31

5.5.4.9 triRaiseMC (TE → SA) 31

5.5.4.10 triEnqueueCall (SA → TE) 32

5.5.4.11 triEnqueueReply (SA → TE) 32

5.5.4.12 triEnqueueException (SA → TE) 33

5.5.5 Miscellaneous operations 33

5.5.5.1 triSUTActionInformal (TE → SA) 33

5.5.5.2 triSUTActionParam (TE → SA) 33

5.6 Platform interface operations 34

5.6.1 triPAReset (TE → PA) 34

5.6.2 Timer operations 34

5.6.2.1 triStartTimer (TE → PA) 34

5.6.2.2 triStopTimer (TE → PA) 34

5.6.2.3 triReadTimer (TE → PA) 35

5.6.2.4 triTimerRunning (TE → PA) 35

5.6.2.5 triTimeout (PA → TE) 35

5.6.3 Miscellaneous operations 36

5.6.3.1 triExternalFunction (TE → PA) 36

5.6.3.2 triSelf (PA → TE) 36

5.6.3.3 triRnd (PA → TE) 36

6 JavaTM language mapping 37

6.1 Introduction 37

6.2 Names and scopes 37

6.2.1 Names 37

6.2.2 Scopes 37

6.3 Type mapping 37

6.3.1 Basic type mapping 37

6.3.1.0 IDL type mapping 37

6.3.1.1 Boolean 38

6.3.1.2 String 38

6.3.2 Structured type mapping 38

6.3.2.0 Mapping rules 38

6.3.2.1 TriPortIdType 38

6.3.2.2 TriPortIdListType 39

6.3.2.3 TriComponentIdType 39

6.3.2.4 TriComponentIdListType 40

6.3.2.5 TriMessageType 40

6.3.2.6 TriAddressType 41

6.3.2.7 TriAddressListType 41

6.3.2.8 TriSignatureIdType 42

6.3.2.9 TriParameterType 42

6.3.2.10 TriParameterPassingModeType 43

6.3.2.11 TriParameterListType 43

6.3.2.12 TriExceptionType 44

6.3.2.13 TriTimerIdType 44

6.3.2.14 TriTimerDurationType 44

6.3.2.15 TriFunctionIdType 45

6.3.2.16 TriTestCaseIdType 45

6.3.2.17 TriActionTemplateType 45

6.3.2.18 TriStatusType 46

6.4 Constants 46

6.5 Mapping of interfaces 47

6.5.0 Basic rules 47

6.5.1 Out and InOut Parameter Passing Mode 47

6.5.2 triCommunication - Interface 47

6.5.2.0 Introduction 47

6.5.2.1 triCommunicationSA 47

6.5.2.2 triCommunicationTE 48

6.5.3 triPlatform - Interface 49

6.5.3.0 Introduction 49

6.5.3.1 TriPlatformPA 49

6.5.3.2 TriPlatformTE 50

6.6 Optional parameters 50

6.7 TRI initialization 50

7 ANSI C language mapping 50

7.1 Introduction 50

7.2 Names and scopes 50

7.2.0 Naming rules 50

7.2.1 Abstract type mapping 51

7.2.2 ANSI C type definitions 52

7.2.3 IDL type mapping 52

7.2.4 TRI operation mapping 52

7.3 Memory management 55

8 C++ language mapping 55

8.1 Introduction 55

8.2 Names and scopes 55

8.3 Memory management 55

8.4 Void 55

8.5 Type mapping 55

8.5.0 Basic rules 55

8.5.1 Encapsulated C++ types 55

8.5.2 Abstract data types 56

8.5.2.1 QualifiedName 56

8.5.2.2 TriAddress 56

8.5.2.3 TriAddressList 57

8.5.2.4 TriComponentId 58

8.5.2.5 TriComponentIdList 58

8.5.2.6 TriException 59

8.5.2.7 TriFunctionId 60

8.5.2.8 TriMessage 60

8.5.2.9 TriParameter 61

8.5.2.10 TriParameterList 61

8.5.2.11 TriParameterPassingMode 62

8.5.2.12 TriPortId 62

8.5.2.13 TriPortIdList 63

8.5.2.14 TriSignatureId 64

8.5.2.15 TriStatus 64

8.5.2.16 TriTestCaseId 64

8.5.2.17 TriTimerDuration 65

8.5.2.18 TriTimerId 65

8.6 Mapping of interfaces 66

8.6.1 TriCommunicationSA 66

8.6.2 TriCommunicationTE 67

8.6.3 TriPlatformPA 68

8.6.4 TriPlatformTE 68

9 C# language mapping 69

9.1 Introduction 69

9.2 Names and scopes 69

9.2.1 Names 69

9.2.2 Scopes 69

9.3 Null value mapping 69

9.4 Type mapping 69

9.4.1 Basic type mapping 69

9.4.1.0 IDL type mapping 69

9.4.1.1 Boolean 70

9.4.1.2 String 70

9.4.2 Structured type mapping 70

9.4.2.0 Mapping rules 70

9.4.2.1 IQualifiedName 70

9.4.2.2 TriPortIdType 70

9.4.2.3 TriPortIdListType 71

9.4.2.4 TriComponentIdType 71

9.4.2.5 TriComponentIdListType 72

9.4.2.6 TriMessageType 72

9.4.2.7 TriAddressType 73

9.4.2.8 TriAddressListType 73

9.4.2.9 TriSignatureIdType 74

9.4.2.10 TriParameterPassingModeType 74

9.4.2.11 TriParameterType 74

9.4.2.12 TriParameterListType 74

9.4.2.13 TriExceptionType 75

9.4.2.14 TriTimerIdType 75

9.4.2.15 TriTimerDurationType 76

9.4.2.16 TriFunctionIdType 76

9.4.2.17 TriTestCaseIdType 76

9.4.2.18 TriStatusType 76

9.5 Mapping of interfaces 76

9.5.0 Basic rules 76

9.5.1 Out and inout parameter passing mode 77

9.5.2 triCommunication interface 77

9.5.2.0 Introduction 77

9.5.2.1 ITriCommunicationSA 77

9.5.2.2 ITriCommunicationTE 78

9.5.2.3 ITriPlatformPA 79

9.5.2.4 ITriPlatformTE 79

9.6 Optional parameters 79

Annex A (normative): IDL Summary 80

Annex B (informative): Use scenarios 84

B.0 Introduction 84

B.1 First scenario 85

B.1.0 Use case 85

B.1.1 TTCN‑3 fragment 85

B.1.2 Message sequence chart 86

B.2 Second scenario 87

B.2.0 Use case 87

B.2.1 TTCN‑3 fragment 87

B.2.2 Message sequence chart 88

B.3 Third scenario 89

B.3.0 Use case 89

B.3.1 TTCN‑3 fragment 89

B.3.2 Message sequence chart 90

Annex C (informative): Bibliography 91

History 92

# Intellectual Property Rights

IPRs essential or potentially essential to the present document may have been declared to ETSI. The information pertaining to these essential IPRs, if any, is publicly available for **ETSI members and non-members**, and can be found in ETSI SR 000 314: *"Intellectual Property Rights (IPRs); Essential, or potentially Essential, IPRs notified to ETSI in respect of ETSI standards"*, which is available from the ETSI Secretariat. Latest updates are available on the ETSI Web server (<https://ipr.etsi.org/>).

Pursuant to the ETSI IPR Policy, no investigation, including IPR searches, has been carried out by ETSI. No guarantee can be given as to the existence of other IPRs not referenced in ETSI SR 000 314 (or the updates on the ETSI Web server) which are, or may be, or may become, essential to the present document.

# Foreword

This ETSI Standard (ES) has been produced by ETSI Technical Committee Methods for Testing and Specification (MTS).

The present document is part 5 of a multi-part deliverable. Full details of the entire series can be found in part 1 [2].

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the [ETSI Drafting Rules](https://portal.etsi.org/Services/editHelp!/Howtostart/ETSIDraftingRules.aspx) (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in ETSI deliverables except when used in direct citation.

# Introduction

The present document consists of two distinct parts, the first part describing the structure of a TTCN‑3 test system implementation and the second part presenting the TTCN‑3 Runtime Interface specification.

The first part introduces the decomposition of a TTCN‑3 test system into four main entities: Test Management (TM), TTCN‑3 Executable (TE), SUT Adaptor (SA), and Platform Adaptor (PA). In addition, the interaction between these entities, i.e. the corresponding interfaces, is defined.

The second part of the present document specifies the TTCN‑3 Runtime Interface (TRI). The interface is defined in terms of operations, which are implemented as part of one entity and called by other entities of the test system. For each operation, the interface specification defines associated data structures, the intended effect on the test system and any constraints on the usage of the operation. Note that this interface specification only defines interactions between the TSI and the SUT as well as timer operations.

# 1 Scope

## 1.1 Scope of the present document

The present document provides the specification of the runtime interface for TTCN‑3 test system implementations. The TTCN‑3 Runtime Interface provides a standardized adaptation for timing and communication of a test system to a particular processing platform and the system under test, respectively. The present document defines the interface as a set of operations independent of target language.

The interface is defined to be compatible with the TTCN‑3 standard (see ETSI ES 201 873-1 [2]). The present document uses the CORBA Interface Definition Language (IDL) to specify the TRI completely. Clauses 6, 7 and 8 present language mappings for this abstract specification to the target languages JavaTM, ANSI C, and C++. A summary of the IDL based interface specification is provided in annex A.

NOTE: JavaTM is the trade name of a programming language developed by Oracle Corporation. This information is given for the convenience of users of the present document and does not constitute an endorsement by ETSI of the programming language named. Equivalent programming languages may be used if they can be shown to lead to the same results.

## 1.2 Compliance

The requirement for a TTCN‑3 test system to be TRI compliant is to adhere to the interface specification stated in the present document as well as to one of the target language mappings included.

EXAMPLE: If a vendor supports JavaTM, the TRI operation calls and implementations, which are part of the TTCN‑3 executable, have to comply with the IDL to JavaTM mapping specified in the present document.

# 2 References

## 2.1 Normative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

Referenced documents which are not found to be publicly available in the expected location might be found at <https://docbox.etsi.org/Reference/>.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are necessary for the application of the present document.

[1] Recommendation ITU-T X.290: "OSI conformance testing methodology and framework for protocol Recommendations for ITU-T applications - General concepts".

NOTE: The corresponding ISO/IEC standard is ISO/IEC 9646-1: "Information technology -- Open Systems Interconnection -- Conformance testing methodology and framework; Part 1: General concepts".

[2] ETSI ES 201 873-1: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN-3 Core Language".

[3] ETSI ES 201 873-4: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 4: TTCN-3 Operational Semantics".

[4] CORBA 3.0: "The Common Object Request Broker: Architecture and Specification", OMG Formal Document (specifies IDL).

[5] Sun Microsystems: "Java™ Language Specification".

NOTE: See at <http://java.sun.com/docs/books/jls/third_edition/html/j3TOC.html>.

[6] ISO/IEC 9899: "Information technology -- Programming Languages -- C".

[7] ISO/IEC 14882: "Information technology -- Programming Languages -- C++".

[8] ECMA-334: "C# Language Specification".

NOTE: See at <http://www.ecma-international.org/publications/standards/Ecma-334.htm>.

## 2.2 Informative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.

Not applicable.

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in ETSI ES 201 873‑1 [2] and the following apply:

**Abstract Test Suite (ATS):** See Recommendation ITU-T X.290 [1].

**communication port:** abstract mechanism facilitating communication between test components

NOTE: A communication port is modelled as a FIFO queue in the receiving direction. Ports can be message‑based, procedure‑based or a mixture of the two.

**Executable Test Suite (ETS):** See Recommendation ITU-T X.290 [1].

**explicit timer:** timer that is declared in a TTCN‑3 ATS and that can be accessed through TTCN‑3 timer operations

**implementation extra information for testing (IXIT):** See Recommendation ITU-T X.290 [1].

**implicit timer:** system timer that is created by the TTCN‑3 Executable to guard a TTCN‑3 call or execute operation

NOTE: Implicit timers are not accessible to the TTCN‑3 user.

**Platform Adaptor (PA):** entity that adapts the TTCN‑3 Executable to a particular execution platform

NOTE: The Platform Adaptor creates a single notion of time for a TTCN‑3 test system, and implements external functions as well as explicit and implicit timers.

**SUT Adaptor (SA):** entity that adapts the TTCN‑3 communication operations with the SUT based on an abstract test system interface and implements the real test system interface

**system under test (SUT):** See Recommendation ITU-T X.290 [1].

NOTE: All types are known at compile time, i.e. are statically bound.

**test case:** See Recommendation ITU-T X.290 [1].

**test event:** either sent or received test data (message or procedure call) on a communication port that is part of the test system interface

**Test Management (TM):** entity that provides a user interface and administers the TTCN‑3 test system

**test system:** See Recommendation ITU-T X.290 [1].

**Test System Interface (TSI):** test component that provides a mapping of the ports available in the (abstract) TTCN‑3 test system to those offered by a real test system

**Timer IDentification (TID):** unique identification for explicit or implicit timer instances that is generated by the TTCN‑3 Executable

**TTCN‑3 Control Interface (TCI):** four interfaces that define the interaction of the TTCN‑3 Executable with the test management, the coding and decoding, the test component handling, and the logging in a test system

**TTCN‑3 Executable (TE):** part of a test system that deals with interpretation or execution of a TTCN‑3 ETS

**TTCN‑3 Runtime Interface (TRI):** two interfaces that define the interaction of the TTCN‑3 Executable between the SUT and the Platform Adapter (PA) and the System Adapter (SA) in a test system

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

ADT Abstract Data Type

ANSI American National Standards Institute

ASN.1 Abstract Syntax Notation One

ATS Abstract Test Suite

CD (External) Coding/Decoding

CH Component Handling

CORBA Common Object Request Broker Architecture

EDS (Internal) Encoding/Decoding System

ETS Executable Test Suite

FIFO First-In-First-Out (Scheduling Discipline)

IDL Interface Definition Language

IXIT Implementation eXtra Information for Testing

MSC Message Sequence Chart

MTC Main Test Component

OMG Object Management Group

PA Platform Adaptor

SA SUT Adaptor

STL Standard Template Library of C++

SUT System Under Test

T3RTS TTCN‑3 RunTime System

TCI TTCN‑3 Control Interface

TE TTCN‑3 Executable

TID Timer IDentification

TL Test Logging

TM Test Management

TMC Test Management and Control

TRI TTCN‑3 Runtime Interface

TSI Test System Interface

TTCN Testing and Test Control Notation

TTCN‑3 Tree and Tabular Combined Notation version 3

# 4 General Structure of a TTCN‑3 Test System

## 4.1 Entities in a TTCN‑3 test system

### 4.1.0 Types of entities

A TTCN‑3 test system can be thought of conceptually as a set of interacting entities where each entity corresponds to a particular aspect of functionality in a test system implementation. These entities manage test execution, interpreting or executing compiled TTCN‑3 code, realize proper communication with the SUT, implement external functions, and handle timer operations.



Figure 1: General Structure of a TTCN‑3 Test System

The structure of a TTCN‑3 test system implementation is illustrated in figure 1. It should be noted that the further refinement of TM into smaller entities, as shown in figure 1 and used in the following clauses of the present document, is purely an aid to define TTCN‑3 test system interfaces.

The part of the test system that deals with interpretation and execution of TTCN‑3 modules, i.e. the Executable Test Suite (ETS), is part of the TTCN‑3 Executable (TE). This corresponds either to the executable code produced by a TTCN‑3 compiler or a TTCN‑3 interpreter in a test system implementation. It is assumed that a test system implementation includes the ETS as derived from a TTCN‑3 ATS.

The remaining part of the TTCN‑3 test system, which deals with any aspects that cannot be concluded from information being present in the original ATS alone, can be decomposed into Test Management (TM), SUT Adaptor (SA), and Platform Adaptor (PA) entities. In general, these entities cover a test system user interface, test execution control, test event logging, as well as communication with the SUT and timer implementation.

### 4.1.1 Test Management and Control (TMC)

#### 4.1.1.0 Test Management and Control Entities

The TMC entity includes functionality related to management of:

* test execution;
* components;
* encoding and decoding; and
* logging.

#### 4.1.1.1 Test Management (TM)

The TM entity is responsible for overall management of the test system. After the test system has been initialized, test execution starts within the TM entity. The entity is responsible for the proper invocation of TTCN‑3 modules, i.e. propagating module parameters and/or IXIT information to the TE if necessary. Typically, this entity would also implement a test system user interface.

#### 4.1.1.2 Test Logging (TL)

The TL entity is responsible for maintaining the test log. It is explicitly notified to log test events by the TE. The TL entity has a unidirectional interface where any entity part of the TE may post a logging request to the TL entity. A TM internal interface may also be used to record test management information generated by the TE.

#### 4.1.1.3 Coding and Decoding (CD)

The CD entity is optionally responsible for the external encoding and decoding data associated with message based or procedure based communication within the TE. The external codecs can be used in parallel with, or instead of, the built‑in codecs associated with the TE. Unlike the built-in codecs the external codecs have a standardized interface which makes them portable between different TTCN‑3 systems and tools.

#### 4.1.1.4 Component Handling (CH)

The CH entity is responsible for distributing parallel test components. This distribution might be across one or many physical systems. The CH entity allows the test management to create and control distributed test systems in a manner which is transparent and independent from the TE.

### 4.1.2 TTCN‑3 Executable (TE)

#### 4.1.2.0 TTCN-3 Executable Entity

The TE entity is responsible for the interpretation or execution of the TTCN‑3 ATS. Conceptually, the TE can be decomposed into three interacting entities: an ETS, TTCN‑3 RunTime System (T3RTS), and an optional internal Encoding/Decoding System (EDS) entity. Note that this refinement of the TE into smaller entities is purely a conceptual aid to define TTCN‑3 test system interfaces ‑ there is no requirement for this distinction to be reflected in TRI implementations.

The following clauses define the responsibilities of each entity and also discuss the handling of timers in the TRI.

#### 4.1.2.1 Executable Test Suite (ETS)

The ETS entity handles the execution or interpretation of test cases, the sequencing and matching of test events, as defined in the corresponding TTCN‑3 modules ETSI ES 201 873‑1 [2]. It interacts with the T3RTS entity to send, attempt to receive (or match), and log test events during test case execution, to create and remove TTCN‑3 test components, as well as to handle external function calls, action operations, and timers. Note that the ETS entity does not directly interact with the SA via the TRI.

#### 4.1.2.2 TTCN‑3 RunTime System (T3RTS)

The T3RTS entity interacts with the TM, SA and PA entities via TCI and TRI, and manages ETS and EDS entities. The T3RTS initializes adaptors as well as ETS and EDS entities. This entity performs all the actions necessary to properly start the execution of a test case or function with parameters in the ETS entity. It queries the TM entity for module parameter values required by the ETS and sends logging information to it. It also collects and resolves associated verdicts returned by the ETS entity as defined in ETSI ES 201 873‑1 [2].

The T3RTS entity implements the creation and removal of TTCN‑3 test components, as well as the TTCN‑3 semantics of message and procedure based communication, external function calls, action operations and timers. This includes notifying the SUT Adaptor (SA) which message or procedure call is to be sent to the SUT, or the Platform Adaptor (PA) which external function is to be executed or which timers are to be started, stopped, queried, or read. Similarly, the T3RTS notifies the ETS entity of incoming messages or procedure calls from the SUT as well as timeout events.

Prior to sending or receiving messages and procedure calls to or from the SA, or handling function calls and action operations in the PA for the ETS entity, the T3RTS invokes the EDS entity for their encoding or decoding. The T3RTS entity should implement all message and procedure based communication operations between test components, but only the TTCN‑3 semantics of procedure based communication with the SUT, i.e. the possible blocking and unblocking of test component execution, guarding with implicit timers, and handling of timeout exceptions as a result of such communication operations. All procedure based communication operations with the SUT are to be realized and identified (in the case of a receiving operation) in the SA as they are most efficiently implemented in a platform specific manner. Note that the timing of any procedure call operation, i.e. implicit timers, is implemented in the Platform Adaptor (PA).

The TTCN‑3 Executable is required to maintain its own port queues (distinct from those which may be available in the SA or PA) for input test events to perform snapshots for receiving operations as defined in ETSI ES 201 873‑1 [2]. Timeout events, which are generated by TTCN‑3 timer, call timer, or test case timer implementations, are to be kept in a timeout list as defined in ETSI ES 201 873‑1 [2]. In figure B.1, all of this functionality has been assigned to the T3RTS entity. It is responsible to store events that the SA or PA has notified the TE entity of, but which have yet to be processed.

#### 4.1.2.3 Encoding/Decoding System (EDS)

The EDS entity is responsible for the internal encoding and decoding of test data, which includes data used in communication operations with the SUT, as specified in the executing TTCN‑3 module. If no encoding has been specified for a TTCN‑3 module the encoding of data values is tool specific. This entity is invoked by and returns to the T3RTS entity. Note that the EDS entity does not directly interact with the SA via the TRI.

#### 4.1.2.4 Timers in the TTCN‑3 Executable

Timers that have been declared and named in the TTCN‑3 ATS can be conceptually classified as explicit in the TE. Timers that are created by the TE for guarding TTCN‑3 procedure calls or execute operations are known in the TE as implicit timers. Explicit as well as implicit timers are both created within the TE but implemented by the Platform Adaptor (PA). This is achieved by generating a unique Timer IDentification (TID) for any timer created in the TE. This unique TID should enable the TE to differentiate between different timers. The TID is to be used by the TE to interact with corresponding timer implementation in the PA.

Note that it is the responsibility of the TE to implement the different TTCN‑3 semantics for explicit and implicit timers correctly as defined in ETSI ES 201 873‑1 [2], e.g. the use of keywords any and all with timers only applies to explicit timers. In the PA all timers, i.e. implicit and explicit, are treated in the same manner.

### 4.1.3 SUT Adaptor (SA)

The SA adapts message and procedure based communication of the TTCN‑3 test system with the SUT to the particular execution platform of the test system. It is aware of the mapping of the TTCN‑3 test component communication ports to test system interface ports and implements the real test system interface as defined in ETSI ES 201 873‑1 [2]. It is responsible to propagate send requests and SUT action operations from the TTCN‑3 Executable (TE) to the SUT, and to notify the TE of any received test events by appending them to the port queues of the TE.

Procedure based communication operations with the SUT are implemented in the SA. The SA is responsible for distinguishing between the different messages within procedure‑based communication (i.e. call, reply, and exception) and to propagate them in the appropriate manner either to the SUT or the TE. TTCN‑3 procedure based communication semantics, i.e. the effect of such operation on TTCN‑3 test component execution, are to be handled in the TE.

The SA has an interface with the TE, which is used to send SUT messages (issued in TTCN‑3 SUT action operations) to the SA and to exchange encoded test data between the two entities in communication operations with the SUT.

### 4.1.4 Platform Adaptor (PA)

The PA implements TTCN‑3 external functions and provides a TTCN‑3 test system with a single notion of time. In this entity, external functions are to be implemented as well as all timers. Notice that timer instances are created in the TE. A timer in the PA can only be distinguished by its Timer IDentification (TID). Therefore, the PA treats both explicit and implicit timers in the same manner.

The interface with the TE enables the invocation of external functions and the starting, reading, and stopping of timers as well as the inquiring of the status of timers using their timer ID. The PA notifies the TE of expired timers.

## 4.2 Interfaces in a TTCN‑3 Test System

As previously depicted in figure 1, a TTCN‑3 test system has two interface sets, the TTCN‑3 Control Interface (TCI) and the TTCN‑3 Runtime Interface (TRI), which specify the interface between Test Management (TM), Test Logging (TL), Component Handling (CH), Encoding/Decoding (CD) and TTCN‑3 Executable (TE) entities, and the TE, SUT Adaptor (SA) and Platform Adaptor (PA) entities, respectively.

The present document defines the TRI. The interaction of the TE with SA and PA are defined in terms of TRI operations.

## 4.3 Execution requirements for a TTCN‑3 test system

Each TRI operation call shall be treated as an atomic operation in the calling entity. The called entity, which implements a TRI operation, shall return control to the calling entity as soon as its intended effect has been accomplished or if the operation cannot be completed successfully. The called entity shall not block in the implementation of procedure‑based communication. Nevertheless, the called entity shall block after the invocation of an external function implementation and wait for its return value. Notice that depending on the test system implementation failure to return from an external function implementation may result in the infinite blocking of test component execution, the TTCN‑3 executable, the Platform Adaptor, or even of the entire test system.

The execution requirements stated above can be realized in a tightly integrated test system implementation. Here, the entire TTCN‑3 test system is implemented in a single executable or process where each test system entity is assigned at least one thread of execution. TRI operations can be implemented here as procedure calls.

Note that a looser integration of a test system implementation is still possible, e.g. an implementation of a TTCN‑3 test system with multiple SUT Adaptors in a distributed computing environment. In this case only a small part of the SUT Adaptor is tightly integrated with the remainder of the TTCN‑3 test system whereas actual SA Adaptors may be realized in separate processes. That small part of SA may then only implement a routing of information provided by TRI operations to the desired SUT Adaptor processes, possibly being executed on remote hosts, and vice versa.

# 5 TTCN‑3 Runtime Interface and operations

## 5.1 Overview of the TRI

### 5.1.0 Sub-interfaces

The subclauses in the clause 5 define TRI operations in terms of when they are to be used and what their effect is intended to be in a TTCN‑3 test system implementation. Also a set of abstract data types is defined which is then used for the definition of TRI operations. The definitions also include a more detailed description of the input parameters required for each TRI operation call and its return value.

The TRI defines the interaction between the TTCN‑3 Executable (TE), SUT Adaptor (SA), and Platform Adaptor (PA) entities within a TTCN‑3 test system implementation. Conceptually, it provides a means for the TE to send test data to the SUT or manipulate timers, and similarly to notify the TE of received test data and timeouts.

The TRI can be considered to consist of two sub‑interfaces, a triCommunication and a triPlatform interface. The triCommunication interface addresses the communication of a TTCN‑3 ETS with the SUT, which is implemented in the SA. The triPlatform interface represents a set of operations, which adapt an ETS to a particular execution platform.

Table 1: Interface Overview

|  |  |  |
| --- | --- | --- |
| Interface | Direction (calling entity → called entity) | |
| Name | TE → SA or PA | SA or PA → TE |
| triCommunication | TE → SA | SA → TE |
| triPlatform | TE → PA | PA → TE |

Both interfaces are bi‑directional so that calling and called parts reside in the TE, SA, and PA entities of the test system. Table 1 shows in more detail the caller/callee relationship between the respective entities. Notice that this table only shows interactions visible at the TRI. Internal communication between parts of the same entity is not reflected as the internal structure of the TE, SA, or PA may differ in a TTCN‑3 test system implementation.

### 5.1.1 The triCommunication Interface

This interface consists of operations that are necessary to implement the communication of the TTCN‑3 ETS with the SUT. It includes operations to initialize the Test System Interface (TSI), establish connections to the SUT, and handle message and procedure based communication with the SUT. In addition, the triCommunication interface offers an operation to reset the SUT Adaptor (SA).

### 5.1.2 The triPlatform Interface

This interface includes all operations necessary to adapt the TTCN‑3 Executable to a particular execution platform. The triPlatform interface offers means to start, stop, read a timer, enquire its status and to add timeout events to the expired timer list. In addition, it offers operations to call TTCN‑3 external functions and to reset the Platform Adaptor (PA). Notice that there is no differentiation between explicit and implicit timers required at the triPlatform Interface. Instead each timer shall be addressed uniformly with its Timer IDentifier (TID).

### 5.1.3 Correlation between TTCN‑3 and TRI Operation Invocations

For some TTCN‑3 operation invocations there exists a direct correlation to one TRI operation invocation (or possibly two in the case of TTCN‑3 execute and call operations), which is shown in table 2. For all other TRI operation invocations there may be no direct correlation.

The shown correlation for TTCN‑3 communication operations (i.e. send, call, reply, and raise) only holds if these operations are invoked on a test component port, which is mapped to a TSI port. Nevertheless, this correlation holds for all such operation invocations if no system component has been specified for a test case, i.e. only the MTC test component is created for a test case and no other test components.

Table 2: Correlation between TTCN‑3 and TRI Operation Invocations (\* = if applicable)

|  |  |  |
| --- | --- | --- |
| TTCN‑3 Operation Name | TRI Operation Name | TRI Interface Name |
| execute | triExecuteTestCase  triStartTimer  triEndTestCase | TriCommunication  TriPlatform  TriCommunication |
| map | triMap (see note 1) | TriCommunication |
| triMapParam (see note 2) |
| unmap | triUnmap (see note 1) | TriCommunication |
| triUnmapParam (see note 2) |
| send | triSend (see note 3) | TriCommunication |
| triSendBC (see note 4) |
| triSendMC (see note 5) |
| call | triCall (see note 3) | TriCommunication |
| triCallBC (see note 4) |
| triCallMC (see note 5) |
| triStartTimer\* | TriPlatform |
| reply | triReply (see note 3) | TriCommunication |
| triReplyBC (see note 4) |
| triReplyMC (see note 5) |
| raise | triRaise (see note 3) | TriCommunication |
| triRaiseBC (see note 4) |
| triRaiseMC (see note 5) |
| action | triSUTactionInformal | TriCommunication |
| start (timer) | triStartTimer | TriPlatform |
| stop (timer) | triStopTimer | TriPlatform |
| read (timer) | triReadTimer | TriPlatform |
| running (timer) | triTimerRunning | TriPlatform |
| TTCN‑3 external function | triExternalFunction | TriPlatform |
| self | triSelf | TriPlatform |
| rnd | triRnd | TriPlatform |
| NOTE 1: For statement without configuration parameter.  note 2: For statement with configuration parameter.  Note 3: For unicast communication.  Note 4: For broadcast communication.  Note 5: For multicast communication. | | |

Note that all of the TRI operations listed in table 2 are used by the TE and that the TE may implement the invocation of these operations differently when evaluating a TTCN snapshot within the TTCN‑3 ETS.

## 5.2 Error handling

### 5.2.0 Basic rules

Error handling is specified for TRI operations called by the TTCN‑3 Executable (TE): The SA or PA reports the status of a TRI operation in the return value of a TRI operation. The status value can either indicate the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the TRI operation. Therefore, the TE may react to an error that occurred either within the SA or PA and issue, e.g. a test case error.

The SA or PA can in addition provide notifications about unrecoverable error situations by use of the operations triSAErrorReq and triPAErrorReq, respectively.

For TRI operations called by the SA or PA no explicit error handling is required since these operations are implemented in the TE. Here, the TE is in control over the test execution in the case that an error occurs in such a TRI operation.

Notice that specific error codes as well as the detection and handling of errors in any of the test system entities are beyond the scope of the present document.

### 5.2.1 triSAErrorReq (SA → TE)

|  |  |
| --- | --- |
| **Signature** | void triSAErrorReq(in string message) |
| **In Parameters** | message A string value, i.e. the error phrase describing the problem. |
| **Return Value** | void |
| **Constraint** | Shall be called whenever an error situation has occurred in the SA with the exception of errors occurring when processing SA calls initiated by the TE. These errors are reported in the operation return. |
| **Effect** | The TE will be notified about an unrecoverable error situation within the SA and may forward the error indication to the test management. |

### 5.2.2 triPAErrorReq (PA → TE)

|  |  |
| --- | --- |
| **Signature** | void triPAErrorReq(in string message) |
| **In Parameters** | message A string value, i.e. the error phrase describing the problem. |
| **Return Value** | void |
| **Constraint** | Shall be called whenever an error situation has occurred in the PA with the exception of errors occurring when processing PA calls initiated by the TE. These errors are reported in the operation return. |
| **Effect** | The TE will be notified about an unrecoverable error situation within the PA and may forward the error indication to the test management. |

## 5.3 Data interface

### 5.3.0 Basic rules

In the TRI operations only encoded test data shall be passed. The TTCN‑3 Executable (TE) is responsible for encoding test data to be sent and decoding received test data in the respective TRI operations since encoding rules can be specified for or within a TTCN‑3 module. Notice that the TE is required to encode test data even if no encoding information has been provided in a TTCN‑3 ATS. In this case the tool vendor has to define an encoding.

Instead of defining an explicit data interface for TTCN‑3 and ASN.1 data types, the TRI standard defines a set of abstract data types. These data types are used in the following definition of TRI operations to indicate which information is to be passed from the calling to the called entity, and vice versa. The concrete representation of these abstract data types as well as the definition of basic data types are defined in the respective language mappings in clauses 6, 7 and 8.

Notice that the values for any identifier data type shall be unique in the test system implementation where uniqueness is defined as being globally distinct at any point in time.

The following abstract data types are defined and used for the definition of TRI operations.

### 5.3.1 Connection

TriComponentIdType A value of type TriComponentIdType includes an identifier, a name and the component type. The distinct value of the latter is the component type name as specified in the TTCN‑3 ATS. This abstract type is mainly used to resolve TRI communication operations on TSI ports that have mappings to many test component ports. It is also used to resolve TCI component handling.

NOTE 1: For the handling of TCI operations on any or all components, the component type name can also be set to "ANY" or "ALL". In that case, both the identifier and the component name are to be ignored.

TriComponentIdListType A value of type TriComponentIdListType is a list of TriComponentIdType. This abstract type is used for multicast communication in TCI.

TriPortIdType A value of type TriPortIdType includes a value of type TriComponentIdType to represent the component to which the port belongs, a port index (if present), and the port and port type name as specified in the TTCN‑3 ATS. The TriPortIdType type is mainly required to pass information about the TSI and connections to the TSI from the TE to the SA.

NOTE 2: If the port is in an n-dimensional port array of the form "**port** MyPortType myPort[d1]...[dn]", the port index ind of the port p[i1]...[in] is computed by the following formula:

ind = ( ∑k=1..n-1 ik\*∏ l=k+1..ndl ) + in

EXAMPLE:

For a four-dimensional port-array with dimensions [10][10][10][10], the port index ind1 of the port at index [2][3][4][5] is ind1= 2\*(10\*10\*10) + 3\*(10\*10) + 4\*10 + 5 = 2345.

For a three-dimensional port-array with dimensions [2][3][4], the port index ind2 of the port at index [1][2][2] is ind2= 1\*(3\*4) + 2\*4 + 2 = 22.

TriPortIdListType A value of type TriPortIdListType is a list of TriPortIdType. This abstract type is used for initialization purposes after the invocation of a TTCN‑3 test case.

### 5.3.2 Communication

TriMessageType A value of type TriMessageType is encoded test data that either is to be sent to the SUT or has been received from the SUT. The order of bits in a value of type TriMessagetype corresponds to the order of bits according to the encoding. If the encoded message consists of the bits b0 .. b9, where b0 is the first bit, then the value of type triMessageType contains "b0 b1 b2 b3 b4 b5 b6 b7 b8 b9" in this order. If padding bits are needed then these are added to the right.

TriAddressType A value of type TriAddressType indicates a source or destination address within the SUT. This abstract type can be used in TRI communication operations and is an open type, which is opaque to the TE.

TriAddressListType A value of type TriAddressListType is a list of TriAddressType. This abstract type is used for multicast communication in TRI.

TriSignatureIdType A value of type TriSignatureIdType is the name of a procedure signature as specified in the TTCN‑3 ATS. This abstract type is used in procedure based TRI communication operations.

TriParameterType A value of type TriParameterType includes an encoded parameter and a value of TriParameterPassingModeType to represent the passing mode specified for the parameter in the TTCN‑3 ATS.

TriParameterPassingModeType A value of type TriParameterPassingModeType is either *in*, *inout*, or *out*. This abstract type is used in procedure based TRI communication operations and for external function calls.

TriParameterListType A value of type TriParameterListType is a list of TriParameterType. This abstract type is used in procedure based TRI communication operations and for external function calls.

TriExceptionType A value of type TriExceptionType is an encoded type and value of an exception that either is to be sent to the SUT or has been received from the SUT. This abstract type is used in procedure based TRI communication operations.

### 5.3.3 Timer

TriTimerIdType A value of type TriTimerIdType specifies an identifier for a timer. This abstract type is required for all TRI timer operations.

TriTimerDurationType A value of type TriTimerDurationType specifies the duration for a timer in seconds.

### 5.3.4 Miscellaneous

TriTestCaseIdType A value of type TriTestCaseIdType is the name of a test case as specified in the TTCN‑3 ATS.

TriFunctionIdType A value of type TriFunctionIdType is the name of an external function as specified in the TTCN‑3 ATS.

TriStatusType A value of type TriStatusType is either ***TRI\_OK*** or ***TRI\_Error*** indicating the success or failure of a TRI operation.

## 5.4 Operation descriptions

All operation definitions are defined using the Interface Definition Language (IDL). Concrete language mappings are defined in clauses 6, 7 and 8.

For every TRI operation call all *in*, *inout*, and *out* parameters listed in the particular operation definition are mandatory. The value of an *in* parameter is specified by the calling entity. Similarly, the value of an *out* parameter is specified by the called entity. In the case of an *inout* parameter, a value is first specified by the calling entity but may be replaced with a new value by the called entity. Note that although TTCN‑3 also uses *in*, *inout*,and *out* for signature definitions the denotations used in TRI IDL specification are not related to those in a TTCN‑3 specification.

Operation calls should use a reserved value to indicate the absence of parameters that are defined as optional in the corresponding TRI parameter description. The reserved values for these types are defined in each language mapping and will be subsequently referred to as the null value.

All functions in the interface are described using the following template:

|  |  |
| --- | --- |
| **F.n.m** | **Operation Name** calling entity → called entity |
| **Signature** | IDL‑Signature |
| **In Parameters** | Description of data passed as parameters to the operation from the calling entity to the called entity |
| **Out Parameters** | Description of data passed as parameters to the operation from the called entity to the calling entity |
| **InOutParameters** | Description of data passed as parameters to the operation from the calling entity to the called entity and from the called entity back to the calling entity |
| **Return Value** | Description of data returned from the operation to the calling entity |
| **Constraints** | Description of any constraints that apply to calling the operation |
| **Effect** | Behaviour required of the called entity before the operation may return |

## 5.5 Communication interface operations

### 5.5.1 triSAReset (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSAReset() |
| **In Parameters** | n.a. |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSAReset operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation can be called by the TE at any time to reset the SA. |
| **Effect** | The SA shall reset all communication means that it is maintaining, e.g. reset static connections to the SUT, close dynamic connections to the SUT, discard any pending messages or procedure calls. The triResetSA operation returns ***TRI\_OK*** in case the operation has been successfully performed, ***TRI\_Error*** otherwise. |

### 5.5.2 Connection handling operations

#### 5.5.2.1 triExecuteTestCase (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triExecuteTestCase( in TriTestCaseIdType testCaseId,  in TriPortIdListType tsiPortList) |
| **In Parameters** | testCaseId identifier of the test case that is going to be executed tsiPortList a list of test system interface ports defined for the test system |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triExecuteTestCase operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error*)** of the operation. |
| **Constraints** | This operation is called by the TE immediately before the execution of any test case. The test case that is going to be executed is indicated by the testCaseId. tsiPortList contains all ports that have been declared in the definition of the system component for the test case, i.e. the TSI ports. If a system component has not been explicitly defined for the test case in the TTCN‑3 ATS then the tsiPortList contains all communication ports of the MTC test component. The ports in tsiPortList are ordered as they appear in the respective TTCN‑3 component declaration. |
| **Effect** | The SA can set up any static connections to the SUT and initialize any communication means for TSI ports.  The triExecuteTestCase operation returns ***TRI\_OK*** in case the operation has been successfully performed, ***TRI\_Error*** otherwise. |

#### 5.5.2.2 triMap (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triMap(in TriPortIdType compPortId,  in TriPortIdType tsiPortId) |
| **In Parameters** | compPortId identifier of the test component port to be mapped tsiPortId identifier of the test system interface port to be mapped |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triMap operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 map operation. |
| **Effect** | The SA can establish a dynamic connection to the SUT for the referenced TSI port.  The triMap operation returns ***TRI\_Error*** in case a connection could not be established successfully, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connection needs to be established by the test system. |

#### 5.5.2.3 triMapParam (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triMapParam(in TriPortIdType compPortId,  in TriPortIdType tsiPortId,  in TriParameterListType paramList) |
| **In Parameters** | compPortId identifier of the test component port to be mapped tsiPortId identifier of the test system interface port to be mapped paramList configuration parameter list |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triMapParam operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 map operation including parameters. |
| **Effect** | The SA can establish a dynamic connection to the SUT for the referenced TSI port.  The triMapParam operation returns ***TRI\_Error*** in case a connection could not be established successfully, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connection needs to be established by the test system. The configuration parameter paramList can be used for setting connection establishment specific parameters. |

#### 5.5.2.4 triUnmap (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triUnmap(in TriPortIdType compPortId,  in TriPortIdType tsiPortId) |
| **In Parameters** | compPortId identifier of the test component port to be unmapped tsiPortId identifier of the test system interface port to be unmapped |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triUnmap operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes any TTCN‑3 unmap operation. |
| **Effect** | The SA shall close a dynamic connection to the SUT for the referenced TSI port.  The triUnmap operation returns ***TRI\_Error*** in case a connection could not be closed successfully or no such connection has been established previously, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connections have to be closed by the test system.  In case the TTCN-3 unmap operation contains a single parameter or all port notation, the triUnmap operation is called once for each affected pair of mapped ports (and might not be called at all if there are no ports to unmap). |

#### 5.5.2.5 triUnmapParam (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triUnmapParam(in TriPortIdType compPortId,  in TriPortIdType tsiPortId,  in TriParameterListType paramList) |
| **In Parameters** | compPortId identifier of the test component port to be unmapped tsiPortId identifier of the test system interface port to be unmapped paramList configuration parameter list |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triUnmapParam operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes any TTCN‑3 unmap operation including parameters. |
| **Effect** | The SA shall close a dynamic connection to the SUT for the referenced TSI port.  The triUnmapParam operation returns ***TRI\_Error*** in case a connection could not be closed successfully or no such connection has been established previously, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connections have to be established by the test system. The configuration parameter paramList can be used for setting connection teardown specific parameters.  In case the TTCN-3 unmap operation contains a single parameter, the triUnmapParam operation is called once for each existing mapping of the referenced system port. The inout parameter values changed during a single call of the triUnmapParam operation are re-used in the subsequent triUnmapParam calls. The final value of the out parameters is the value obtained during the last triUnmapParam call. |

#### 5.5.2.6 triEndTestCase (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triEndTestCase() |
| **In Parameters** | n.a. |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triEndTestCase operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error*)** of the operation. |
| **Constraints** | This operation is called by the TE immediately after the execution of any test case. |
| **Effect** | The SA can free resources, cease communication at system ports and to test components.  The triEndTestCase operation returns ***TRI\_OK*** in case the operation has been successfully performed, ***TRI\_Error*** otherwise. |

### 5.5.3 Message based communication operations

#### 5.5.3.1 triSend (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSend(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,   in TriAddressType SUTaddress,   in TriMessageType sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  sendMessage the encoded message to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSend operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of sendMessage has to be done in the TE prior to this TRI operation call. |
| **Effect** | The SA can send the message to the SUT.  The triSend operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

#### 5.5.3.2 triSendBC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSendBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,   in TriMessageType sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  sendMessage the encoded message to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSendBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of sendMessage has to be done in the TE prior to this TRI operation call. |
| **Effect** | The SA can broadcast the message to the SUT.  The triSendBC operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

#### 5.5.3.3 triSendMC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSendMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,   in TriAddressListType SUTaddresses,   in TriMessageType sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  sendMessage the encoded message to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSendMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of sendMessage has to be done in the TE prior to this TRI operation call. |
| **Effect** | The SA can multicast the message to the SUT.  The triSendMC operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

#### 5.5.3.4 triEnqueueMsg (SA → TE)

|  |  |
| --- | --- |
| **Signature** | void triEnqueueMsg(in TriPortIdType tsiPortId,  in TriAddressType SUTaddress, in TriComponentIdType componentId,  in TriMessageType receivedMessage) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the message is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  receivedMessage the encoded received message |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation is called by the SA after it has received a message from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or has been referenced in the previous triExecuteTestCase statement.  In the invocation of a triEnqueueMsg operation receivedMessage shall contain an encoded value. |
| **Effect** | This operation shall pass the message to the TE indicating the component componentId to which the TSI port tsiPortId is mapped.  The decoding of receivedMessage has to be done in the TE. |

### 5.5.4 Procedure based communication operations

#### 5.5.4.1 triCall (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triCall(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCall operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *in* and *inout* procedure parameters contain encoded values.  The procedure parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can initiate the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCall operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCall operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

#### 5.5.4.2 triCallBC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triCallBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,   in TriSignatureIdType signatureId,   in TriParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCallBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *in* and *inout* procedure parameters contain encoded values.  The procedure parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can initiate and broadcast the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCallBC operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCallBC operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

#### 5.5.4.3 triCallMC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triCallMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCallMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *in* and *inout* procedure parameters contain encoded values.  The procedure parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can initiate and multicast the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCallMC operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCallMC operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

#### 5.5.4.4 triReply (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triReply(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriAddressType SUTaddress, in TriSignatureIdType signatureId, in TriParameterListType parameterList, in TriParameterType returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) encoded return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReply operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *out* and *inout* procedure parameters and the return value contain encoded values.  The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can issue the reply to a procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReply operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

#### 5.5.4.5 triReplyBC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triReplyBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriSignatureIdType signatureId, in TriParameterListType parameterList, in TriParameterType returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) encoded return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReplyBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *out* and *inout* procedure parameters and the return value contain encoded values.  The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can broadcast the reply to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReplyBC operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

#### 5.5.4.6 triReplyMC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triReplyMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriAddressListType SUTaddresses, in TriSignatureIdType signatureId, in TriParameterListType parameterList, in TriParameterType returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) encoded return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReplyMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  All *out* and *inout* procedure parameters and the return value contain encoded values.  The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template. Their encoding has to be done in the TE prior to this TRI operation call.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can multicast the reply to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReplyMC operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

#### 5.5.4.7 triRaise (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triRaise(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriAddressType SUTaddress, in TriSignatureIdType signatureId, in TriExceptionType exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the encoded exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaise operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of the exception has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can raise an exception to a procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaise operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

#### 5.5.4.8 triRaiseBC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triRaiseBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriSignatureIdType signatureId,  in TriExceptionType exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the encoded exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaiseBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of the exception has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can raise and broadcast an exception to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaiseBC operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

#### 5.5.4.9 triRaiseMC (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triRaiseMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriSignatureIdType signatureId,  in TriExceptionType exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the encoded exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaiseMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.  The encoding of the exception has to be done in the TE prior to this TRI operation call. |
| **Effect** | On invocation of this operation the SA can raise and multicast an exception to a procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaiseMC operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

#### 5.5.4.10 triEnqueueCall (SA → TE)

|  |  |
| --- | --- |
| **Signature** | void triEnqueueCall(in TriPortIdType tsiPortId,  in TriAddressType SUTaddress, in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the procedure call is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration. Description of data passed as parameters to the operation from the calling entity to the called entity |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a procedure call from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement.  In the invocation of a triEnqueueCall operation all *in* and *inout* procedure parameters contain encoded values. |
| **Effect** | The TE can enqueue this procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped. The decoding of procedure parameters has to be done in the TE.  The TE shall indicate no error in case the value of any *out* parameter is different from null. |

#### 5.5.4.11 triEnqueueReply (SA → TE)

|  |  |
| --- | --- |
| **Signature** | void triEnqueueReply(in TriPortIdType tsiPortId,  in TriAddressType SUTaddress, in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList, in TriParameterType returnValue) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the reply is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call  parameterList a list of encoded parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) encoded return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a reply from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement.  In the invocation of a triEnqueueReply operation all *out* and *inout* procedure parameters and the return value contain encoded values.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be used for the return value. |
| **Effect** | The TE can enqueue this reply to the procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped. The decoding of the procedure parameters has to be done within the TE. The TE shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

#### 5.5.4.12 triEnqueueException (SA → TE)

|  |  |
| --- | --- |
| **Signature** | void triEnqueueException(in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriComponentIdType componentId, in TriSignatureIdType signatureId,  in TriExceptionType exc) |
| **In Parameters** | tsiPortId identifier for the test system interface port via which the exception is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the encoded exception |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a reply from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement.  In the invocation of a triEnqueueException operation exception shall contain an encoded value. |
| **Effect** | The TE can enqueue this exception for the procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped.  The decoding of the exception has to be done within the TE. |

### 5.5.5 Miscellaneous operations

#### 5.5.5.1 triSUTActionInformal (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSUTActionInformal(in string description) |
| **In Parameters** | description an informal description of an action to be taken on the SUT |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSUTactionInformal operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 SUT action operation, which only contains a single character string literal as an argument. |
| **Effect** | On invocation of this operation the SA shall initiate the described actions to be taken on the SUT, e.g. turn on, initialize, or send a message to the SUT.  The triSUTActionInformal operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. Notice that the return value of this TRI operation does not make any statement about the success or failure of the actions to be taken on the SUT. |

#### 5.5.5.2 triSUTActionParam (TE → SA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triSUTActionParam(in TriParameterListType parameterList) |
| **In Parameters** | params encoded parameters of an action to be taken on the SUT |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSUTactionParam operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 SUT action operation, which either contains multiple arguments or a single argument that is not a character string literal. |
| **Effect** | On invocation of this operation the SA shall initiate the described actions to be taken on the SUT, e.g. turn on, initialize, or send a message to the SUT.  The triSUTActionParam operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. Notice that the return value of this TRI operation does not make any statement about the success or failure of the actions to be taken on the SUT. |

## 5.6 Platform interface operations

### 5.6.1 triPAReset (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triPAReset() |
| **In Parameters** | n.a. |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triPAReset operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation can be called by the TE at any time to reset the PA. |
| **Effect** | The PA shall reset all timing activities which it is currently performing, e.g. stop all running timers, discard any pending timeouts of expired timers.  The triPAReset operation returns *TRI\_OK* in case the operation has been performed successfully, *TRI\_Error* otherwise. |

### 5.6.2 Timer operations

#### 5.6.2.1 triStartTimer (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triStartTimer( in TriTimerIdType timerId,  in TriTimerDurationType timerDuration) |
| **In Parameters** | timerId identifier of the timer instance  timerDuration duration of the timer in seconds |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triStartTimer operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when a timer needs to be started. |
| **Effect** | On invocation of this operation the PA shall start the indicated timer with the indicated duration. The timer runs from the value zero (0.0) up to the maximum specified by timerDuration. Should the timer indicated by timerId already be running it is to be restarted. When the timer expires the PA will call the triTimeout() operation with timerId.  The triStartTimer operation returns *TRI\_OK* if the timer has been started successfully, *TRI\_Error* otherwise. |

#### 5.6.2.2 triStopTimer (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triStopTimer(in TriTimerIdType timerId) |
| **In Parameters** | timerId identifier of the timer instance |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triStopTimer operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when a timer is to be stopped. |
| **Effect** | On invocation of this operation the PA shall use the timerId to stop the indicated timer instance. The stopping of an inactive timer, i.e. a timer which has not been started or has already expired, should have no effect.  The triStopTimer operation returns ***TRI\_OK*** if the operation has been performed successfully, ***TRI\_Error*** otherwise. Notice that stopping an inactive timer is a valid operation. In this case ***TRI\_OK***shall be returned. |

#### 5.6.2.3 triReadTimer (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triReadTimer( in TriTimerIdType timerId,  out TriTimerDurationType elapsedTime) |
| **In Parameters** | timerId identifier of the timer instance |
| **Out Parameters** | elapsedTime value of the time elapsed since the timer has been started in seconds |
| **Return Value** | The return status of the triReadTimer operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation may be called by the TE when a TTCN‑3 read timer operation is to be executed on the indicated timer. |
| **Effect** | On invocation of this operation the PA shall use the timerId to access the time that elapsed since this timer was started. The return value elapsedTime shall be provided in seconds. The reading of an inactive timer, i.e. a timer which has not been started or already expired, shall return an elapsed time value of zero.  The triReadTimer operation returns ***TRI\_OK*** if the operation has been performed successfully, ***TRI\_Error*** otherwise. |

#### 5.6.2.4 triTimerRunning (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triTimerRunning(in TriTimerIdType timerId,  out boolean running) |
| **In Parameters** | timerId identifier of the timer instance |
| **Out Parameters** | running status of the timer |
| **Return Value** | The return status of the triTimerRunning operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation may be called by the TE when a TTCN‑3 running timer operation is to be executed on the indicated timer. |
| **Effect** | On invocation of this operation the PA shall use the timerId to access the status of the timer. The operation sets running to the boolean value true if and only if the timer is currently running.  The triTimerRunning operation returns ***TRI\_OK*** if the status of the timer has been successfully determined, ***TRI\_Error*** otherwise. |

#### 5.6.2.5 triTimeout (PA → TE)

|  |  |
| --- | --- |
| **Signature** | void triTimeout(in TriTimerIdType timerId) |
| **In Parameters** | timerId identifier of the timer instance |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation is called by the PA after a timer, which has previously been started using the triStartTimer operation, has expired, i.e. it has reached its maximum duration value. |
| **Effect** | The timeout with the timerId can be added to the timeout list in the TE. The implementation of this operation in the TE has to be done in such a manner that it addresses the different TTCN‑3 semantics for timers defined in ETSI ES 201 873‑4 [3]. |

### 5.6.3 Miscellaneous operations

#### 5.6.3.1 triExternalFunction (TE → PA)

|  |  |
| --- | --- |
| **Signature** | TriStatusType triExternalFunction(  in TriFunctionIdType functionId,  inout TriParameterListType parameterList, out TriParameterType returnValue) |
| **In Parameters** | functionId identifier of the external function |
| **Out Parameters** | returnValue (optional) encoded return value |
| **InOutParameters** | parameterList a list of encoded parameters for the indicated function. The parameters in parameterList are ordered as they appear in the TTCN‑3 function declaration. |
| **Return Value** | The return status of the triExternalFunction operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a function which is defined to be TTCN‑3 external (i.e. all non‑external functions are implemented within the TE).  In the invocation of a triExternalFunction operation by the TE all *in* and *inout* function parameters contain encoded values. No error shall be indicated by the PA in case the value of any *out* parameter is non‑null. |
| **Effect** | For each external function specified in the TTCN‑3 ATS the PA shall implement the behaviour. On invocation of this operation the PA shall invoke the function indicated by the identifier functionId. It shall access the specified *in* and *inout* function parameters in parameterList, evaluate the external function using the values of these parameters, and compute values for *inout* and *out* parameters in parameterList. The operation shall then return encoded values for all *inout* and *out* function parameters and the encoded return value of the external function.  If no return type has been defined for this external function in the TTCN‑3 ATS, the distinct value null shall be used for the latter.  The triExternalFunction operation returns ***TRI\_OK*** if the PA completes the evaluation of the external function successfully, ***TRI\_Error*** otherwise.  Note that whereas all other TRI operations are considered to be non‑blocking, the triExternalFunction operation is considered to be *blocking.* That means that the operation shall not return before the indicated external function has been fully evaluated. External functions have to be implemented carefully as they could cause deadlock of test component execution or even the entire test system implementation. |

#### 5.6.3.2 triSelf (PA → TE)

|  |  |
| --- | --- |
| **Signature** | TriComponentId triSelf() |
| **In Parameters** | n.a. |
| **Out Parameters** | n.a. |
| **Return Value** | The component id of the calling component. |
| **Constraints** | This operation can be called by the PA during the execution of triExternalFunction. |
| **Effect** | The TriComponentId identifying the component which issued the external function call is returned. |

#### 5.6.3.3 triRnd (PA → TE)

|  |  |
| --- | --- |
| **Signature** | TriMessage triRnd(in TriComponentIdType componentId, in TriMessage seed) |
| **In Parameters** | componentId identifier of the component for which to generate the random number |
|  | seed the encoded seed to be used for generation of the random number or null |
| **Out Parameters** | n.a. |
| **Return Value** | The encoded generated float random number. |
| **Constraints** | This operation is called by the PA to generate a random number in the context of an external function. |
| **Effect** | A random number is generated in the scope of the component identified by the given componentId using the given seed (if any) according to the specification of the predefined rnd function defined in ETSI ES 201 873‑1 [2]. |

# 6 JavaTM language mapping

## 6.1 Introduction

This clause introduces the TRI JavaTM language mapping. For efficiency reasons a dedicated language mapping is introduced instead of using the OMG IDL [4] to JavaTM language [5].

The JavaTM language mapping for the TTCN‑3 Runtime Interface defines how the IDL definitions described in clause 5 are mapped to the JavaTM language. The language mapping is independent of the used Java version as only basic JavaTM language constructs are used.

## 6.2 Names and scopes

### 6.2.1 Names

Although there are no conflicts between identifiers used in the IDL definition and the JavaTM language some naming translation rules are applied to the IDL identifiers:

* Java parameter identifiers shall start with a lower case letter, and subsequent part building the parameter identifier start with a capital letter. For example the IDL parameter identifier **SUTaddress** maps to sutAddress in Java.
* Java interfaces or class identifiers are omitting the trailing Type used in the IDL definition. For example the IDL type **TriPortIdType** maps to TriPortId in Java.

The resulting mapping conforms to the standard Java coding conventions.

### 6.2.2 Scopes

The IDL module **triInterface** is mapped to the JavaTM package org.etsi.ttcn3.tri. All IDL type declarations within this module are mapped to Java classes or interface declarations within this package.

## 6.3 Type mapping

### 6.3.1 Basic type mapping

#### 6.3.1.0 IDL type mapping

Table 3 gives an overview on how the used basic IDL types are mapped to the Java types.

Table 3: Basic type mappings

|  |  |
| --- | --- |
| IDL Type | Java Type |
| boolean | org.etsi.ttcn.tri.TriBoolean |
| string | java.lang.String |

Other IDL basic types are not used within the IDL definition.

#### 6.3.1.1 Boolean

The IDL **boolean** type is mapped to the interface org.etsi.ttcn.tri.TriBoolean, so that objects implementing this interface can act as holder objects.

The following interface is defined for org.etsi.ttcn.tri.TriBoolean:

// TriBoolean

package org.etsi.ttcn.tri;

public interface TriBoolean {

public void setBooleanValue(boolean value);

public boolean getBooleanValue();

}

**Methods:**

* setBooleanValue  
  Sets this TriBoolean to the boolean value value.
* getBooleanValue  
  Returns the boolean value represented by this TriBoolean.

#### 6.3.1.2 String

The IDL **string** type is mapped to the java.lang.String class without range checking or bounds for characters in the string. All possible strings defined in TTCN‑3 can be converted to java.lang.String.

### 6.3.2 Structured type mapping

#### 6.3.2.0 Mapping rules

The TRI IDL description defines user‑defined types as native types. In the JavaTM language mapping, these types are mapped to Java interfaces. The interfaces define methods and attributes being available for objects implementing this interface.

#### 6.3.2.1 TriPortIdType

**TriPortIdType** is mapped to the following interface:

// TRI IDL TriPortIdType

package org.etsi.ttcn.tri;

public interface TriPortId {

public String getPortName();

public String getPortTypeName();

public TriComponentId getComponent();

public boolean isArray();

public int getPortIndex();

}

**Methods:**

* getPortName  
  Returns the port name as defined in the TTCN‑3 specification.
* getPortTypeName  
  Returns the port type name as defined in the TTCN‑3 specification.
* getComponent  
  Returns the component identifier that this TriPortId belongs to as defined in the TTCN‑3 specification.
* isArray  
  Returns true if this port is part of a port array, false otherwise.
* getPortIndex  
  Returns the port index if this port is part of a port array starting at zero. If the port is not part of a port array, then ‑1 is returned.

#### 6.3.2.2 TriPortIdListType

**TriPortIdListType** is mapped to the following interface:

// TRI IDL TriPortIdListType

package org.etsi.ttcn.tri;

public interface TriPortIdList {

public int size();

public boolean isEmpty();

public java.util.Enumeration getPortIds();

public TriPortId get(int index);

}

**Methods:**

* size  
  Returns the number of ports in this list.
* isEmpty  
  Returns true if this list contains no ports.
* getPortIds  
  Returns an Enumeration over the ports in the list. The enumeration provides the ports in the same order as they appear in the list.
* get  
  Returns the TriPortId at the specified position.

#### 6.3.2.3 TriComponentIdType

**TriComponentIdType** is mapped to the following interface:

// TRI IDL TriComponentIdType

package org.etsi.ttcn.tri;

public interface TriComponentId {

public String getComponentId();

public String getComponentName();

public String getComponentTypeName();

public TriPortIdList getPortList();

public boolean equals(TriComponentId component);

}

**Methods:**

* getComponentId  
  Returns a representation of this unique component identifier.
* getComponentName  
  Returns the component name as defined in the TTCN‑3 specification. If no name is provided, an empty string is returned.
* getComponentTypeName  
  Returns the component type name as defined in the TTCN‑3 specification.
* getPortList  
  Returns the component's port list as defined in the TTCN‑3 specification.
* equals  
  Compares component with this TriComponentId for equality. Returns true if and only if both components have the same representation of this unique component identifier, false otherwise.

#### 6.3.2.4 TriComponentIdListType

**TriComponentIdListType** is mapped to the following interface:

// TRI IDL TriComponentIdListType

package org.etsi.ttcn.tri;

public interface TriComponentIdListType {

public int size();

public boolean isEmpty();

public java.util.Enumeration getComponents();

public TriComponentId get(int index);

public void clear();

public void add(TriComponentId comp);

}

**Methods:**

* size  
  Returns the number of components in this list.
* isEmpty  
  Returns true if this list contains no components.
* getComponents  
  Returns an Enumeration over the components in the list. The enumeration provides the components in the same order as they appear in the list.
* get  
  Returns the TriComponentId at the specified position.
* clear  
  Removes all components from this TriComponentIdList.
* add  
  Adds comp to the end of this TriComponentIdList.

#### 6.3.2.5 TriMessageType

**TriMessageType** is mapped to the following interface:

// TRI IDL TriMessageType

package org.etsi.ttcn.tri;

public interface TriMessage {

public byte[] getEncodedMessage();

public void setEncodedMessage(byte[] message);

public int getNumberOfBits();

public void setNumberOfBits(int amount);

public boolean equals(TriMessage message);

}

**Methods:**

* getEncodedMessage  
  Returns the message encoded according the coding rules defined in the TTCN‑3 specification.
* setEncodedMessage  
  Sets the encoded message representation of this TriMessage to message.
* getNumberOfBits  
  Returns the amount of bits of the message.
* setNumberOfBits  
  Sets the amount of bits in the message.
* equals  
  Compares message with this TriMessage for equality. Returns true if and only if both messages have the same encoded representation, false otherwise.

#### 6.3.2.6 TriAddressType

**TriAddressType** is mapped to the following interface:

// TRI IDL TriAddressType

package org.etsi.ttcn.tri;

public interface TriAddress {

public byte[] getEncodedAddress();

public void setEncodedAddress(byte[] address);

public int getNumberOfBits();

public void setNumberOfBits(int amount);

public boolean equals(TriAddress address);

}

**Methods:**

* getEncodedAddress  
  Returns the encoded address.
* setEncodedAddress  
  Sets the encoded address of this TriAddress to address.
* getNumberOfBits  
  Returns the amount of bits of the address.
* setNumberOfBits  
  Sets the amount of bits in the address.
* equals  
  Compares address with this TriAddress for equality. Returns true if and only if both addresses have the same encoded representation, false otherwise.

#### 6.3.2.7 TriAddressListType

**TriAddressListType** is mapped to the following interface:

// TRI IDL TriAddressListType

package org.etsi.ttcn.tri;

public interface TriAddressListType {

public int size();

public boolean isEmpty();

public java.util.Enumeration getAddresses();

public TriAddress get(int index);

public void clear();

public void add(TriAddress addr);

}

**Methods:**

* size  
  Returns the number of components in this list.
* isEmpty  
  Returns true if this list contains no components.
* getAddresses  
  Returns an Enumeration over the components in the list. The enumeration provides the addresses in the same order as they appear in the list.
* get  
  Returns the TriAddress at the specified position.
* clear  
  Removes all addresses from this TriAddressList.
* add  
  Adds addr to the end of this TriAddressList.

#### 6.3.2.8 TriSignatureIdType

**TriSignatureIdType** is mapped to the following interface:

// TRI IDL TriSignatureIdType

package org.etsi.ttcn.tri;

public interface TriSignatureId {

public String getSignatureName();

public void setSignatureName(String sigName);

public boolean equals(TriSignatureId sig);

}

**Methods:**

* getSignatureName  
  Returns the signature identifier as defined in the TTCN‑3 specification.
* setSignatureName  
  Sets the signature identifier of this TriSignatureId to sigName.
* equals  
  Compares sig with this TriSignatureId for equality. Returns true if and only if both signatures have the same signature identifier, false otherwise.

#### 6.3.2.9 TriParameterType

**TriParameterType** is mapped to the following interface:

// TRI IDL TriParameterType

package org.etsi.ttcn.tri;

public interface TriParameter {

public String getParameterName();

public void setParameterName(String name);

public int getNumberOfBits();

public void setNumberOfBits(int amount);

public int getParameterPassingMode();

public void setParameterPassingMode(TriParameterPassingMode mode);

public byte[] getEncodedParameter();

public void setEncodedParameter(byte[] parameter);

}

**Methods:**

* getParameterName  
  Returns the parameter name as defined in the TTCN‑3 specification.
* setParameterName  
  Sets the name of this TriParameter parameter to name.
* getNumberOfBits  
  Returns the amount of bits of the parameter.
* setNumberOfBits  
  Sets the amount of bits in the parameter.
* getParameterPassingMode  
  Returns the parameter passing mode of this parameter.
* setParameterPassingMode  
  Sets the parameter mode of this TriParameter parameter to mode.
* getEncodedParameter  
  Returns the encoded parameter representation of this TriParameter, or the null object if the parameter contains the distinct value null (see also clause 5.5.4).
* setEncodedParameter  
  Sets the encoded parameter representation of this TriParameter to parameter. If the distinct value null shall be set to indicate that this parameter holds no value, the Java null shall be passed as parameter (see also clause 5.5.4).

#### 6.3.2.10 TriParameterPassingModeType

**TriParameterPassingModeType** is mapped to the following interface:

// TRI IDL TriParameterPassingModeType

package org.etsi.ttcn.tri;

public interface TriParameterPassingMode {

public final static int TRI\_IN = 0;

public final static int TRI\_INOUT = 1;

public final static int TRI\_OUT = 2;

}

**Methods:**

* TRI\_IN  
  Will be used to indicate that a TriParameter is an in parameter.
* TRI\_INOUT  
  Will be used to indicate that a TriParameter is an inout parameter.
* TRI\_OUT  
  Will be used to indicate that a TriParameter is an out parameter.

#### 6.3.2.11 TriParameterListType

**TriParameterListType** is mapped to the following interface:

// TRI IDL TriParameterListType

package org.etsi.ttcn.tri;

public interface TriParameterList {

public int size();

public boolean isEmpty();

public java.util.Enumeration getParameters();

public TriParameter get(int index);

public void clear();

public void add(TriParameter parameter);

}

**Methods:**

* size  
  Returns the number of parameters in this list.
* isEmpty  
  Returns true if this list contains no parameters.
* getParameters  
  Returns an Enumeration over the parameters in the list. The enumeration provides the parameters in the same order as they appear in the list.
* get  
  Returns the TriParameter at the specified position.
* clear  
  Removes all parameters from this TriParameterList.
* add  
  Adds parameter to the end of this TriParameterList.

#### 6.3.2.12 TriExceptionType

**TriExceptionType** is mapped to the following interface:

// TRI IDL TriExceptionType

package org.etsi.ttcn.tri;

public interface TriException {

public byte[] getEncodedException();

public void setEncodedException(byte[] message);

public int getNumberOfBits();

public void setNumberOfBits(int amount);

public boolean equals(TriException exc);

}

**Methods:**

* getEncodedException  
  Returns the exception encoded according to the coding rules defined in the TTCN‑3 specification.
* setEncodedException  
  Sets the encoded exception representation of this TriException to exc.
* getNumberOfBits  
  Returns the amount of bits of the exception.
* setNumberOfBits  
  Sets the amount of bits in the exception.
* equals  
  Compares exc with this TriException for equality. Returns true if and only if both exceptions have the same encoded representation, false otherwise.

#### 6.3.2.13 TriTimerIdType

**TriTimerIdType** is mapped to the following interface:

// TRI IDL TriTimerIdType

package org.etsi.ttcn.tri;

public interface TriTimerId {

public String getTimerName();

public boolean equals(TriTimerId timer);

}

**Methods:**

* getTimerName  
  Returns the name of this timer identifier as defined in the TTCN‑3 specification. In case of implicit timers the result is implementation dependent (see clause 4.1.2.4).
* equals  
  Compares timer with this TriTimerId for equality. Returns true if and only if both timers identifiers represent the same timer, false otherwise.

#### 6.3.2.14 TriTimerDurationType

**TriTimerDurationType** is mapped to the following interface:

// TRI IDL TriTimerDurationType

package org.etsi.ttcn.tri;

public interface TriTimerDuration {

public double getDuration();

public void setDuration(double duration);

public boolean equals(TriTimerDuration duration);

}

**Methods:**

* getDuration  
  Returns the duration of a timer as double.
* setDuration  
  Sets the duration of this TriTimerDuration to duration.
* equals  
  Compares duration with this TriTimerDuration for equality. Returns true if and only if both have the same duration, false otherwise.

#### 6.3.2.15 TriFunctionIdType

**TriFunctionIdType** is mapped to the following interface:

// TRI IDL TriFunctionIdType

package org.etsi.ttcn.tri;

public interface TriFunctionId {

public String toString();

public String getFunctionName();

public boolean equals(TriFunctionId fun);

}

**Methods:**

* toString  
  Returns the string representation of the function as defined in TTCN‑3 specification.
* getFunctionName  
  Returns the function identifier as defined in the TTCN‑3 specification.
* equals  
  Compares fun with this TriFunctionId for equality. Returns true if and only if both functions have the same function identifier, false otherwise.

#### 6.3.2.16 TriTestCaseIdType

**TriTestCaseIdType** is mapped to the following interface:

// TRI IDL TriTestCaseIdType

package org.etsi.ttcn.tri;

public interface TriTestCaseId {

public String toString();

public String getTestCaseName();

public boolean equals(TriTestCaseId tc);

}

**Methods:**

* toString  
  Returns the string representation of the test case as defined in TTCN‑3 specification.
* getTestCaseName  
  Returns the test case identifier as defined in the TTCN‑3 specification.
* equals  
  Compares tc with this TriTestCaseId for equality. Returns true if and only if both test cases have the same test case identifier, false otherwise.

#### 6.3.2.17 TriActionTemplateType

The content of this clause is obsolete.

#### 6.3.2.18 TriStatusType

**TriStatusType** is mapped to the following interface:

// TriStatusType

package org.etsi.ttcn.tri;

public interface TriStatus {

public final static int TRI\_OK = 0;

public final static int TRI\_ERROR = ‑1;

public String toString();

public int getStatus();

public void setStatus(int status);

public boolean equals(TriStatus status);

}

**Methods:**

* toString  
  Returns the string representation of the status.
* getStatus  
  Returns the status of this TriStatus.
* setStatus  
  Sets the status of this TriStatus.
* equals  
  Compares status with this TriStatus for equality. Returns true if and only if they have the same status, false otherwise.

## 6.4 Constants

Within this JavaTM language mapping constants have been specified. All constants are defined public final static and are accessible from every object from every package. The constants defined within this clause are not defined with the IDL clause. Instead they result from the specification of the TRI IDL types marked as native.

The following constants can be used to determine the parameter passing mode of TTCN‑3 parameters (see also clause 6.3.2.8):

* org.etsi.ttcn.tri.TriParameterPassingMode.TRI\_IN;
* org.etsi.ttcn.tri.TriParameterPassingMode.TRI\_INOUT;
* org.etsi.ttcn.tri.TriParameterPassingMode.TRI\_OUT.

The values of instances of these constants shall reflect the parameter passing mode defined in the TTCN‑3 procedure signatures.

For the distinct parameter value null, the encoded parameter value shall be set to Java null.

The following constants shall be used to indicate the local success of a method (see also clause 6.3.2.18):

* org.etsi.ttcn.tri.TriStatus.TRI\_OK;
* org.etsi.ttcn.tri.TriStatus.TRI\_ERROR.

## 6.5 Mapping of interfaces

### 6.5.0 Basic rules

The TRI IDL definition defines two interfaces, the **triCommunication** and the **triPlatform** interface. As the operations are defined for different directions within this interface, i.e. some operations can only be called by the TTCN‑3 Executable (TE) on the System Adaptor (SA) while others can only be called by the SA on the TE. This is reflected by dividing the TRI IDL interfaces in two sub interfaces, each suffixed by the called entity.

Table 4: Sub Interfaces

|  |  |  |  |
| --- | --- | --- | --- |
| Calling/Called | TE | SA | PA |
| TE | ‑ | TriCommunicationSA | triPlatformPA |
| SA | TriCommunicationTE | ‑ | ‑ |
| PA | TriPlatformTE | ‑ | ‑ |

All methods defined in these interfaces should behave as defined in clause 5.

### 6.5.1 Out and InOut Parameter Passing Mode

The following IDL types are used in out or inout parameter passing mode:

* TriParameter.
* TriParameterList.
* TriBoolean.
* TriTimerDuration.

In case they are used in out or inout parameter passing mode objects of the respective class will be passed with the method call. The called entity can then access methods to set the return values.

### 6.5.2 triCommunication - Interface

#### 6.5.2.0 Introduction

The **triCommunication** interface is divided into two sub interfaces, the triCommunicationSA interface, defining calls from the TE to the SA and the triCommunicationTE interface, defining calls from the SA to the TE.

#### 6.5.2.1 triCommunicationSA

The triCommunicationSA interface is mapped to the following interface:

// TriCommunication

// TE ‑> SA

package org.etsi.ttcn.tri;

public interface TriCommunicationSA {

// Reset Operation

// Ref: TRI‑Definition 5.5.1

TriStatus triSAReset();

// Connection handling operations

// Ref: TRI‑Definition 5.5.2.1

public TriStatus triExecuteTestCase(TriTestCaseId

testCaseId,TriPortIdList tsiPorts);

// Ref: TRI‑Definition 5.5.2.2

public TriStatus triMap(TriPortId compPortId, TriPortId tsiPortId);

// Ref: TRI‑Definition 5.5.2.3

public TriStatus triMapParam(TriPortId compPortId, TriPortId tsiPortId,

TriParameterList paramList);

// Ref: TRI‑Definition 5.5.2.4

public TriStatus triUnmap(TriPortId compPortId, TriPortId tsiPortId);

// Ref: TRI‑Definition 5.5.2.5

public TriStatus triUnmapParam(TriPortId compPortId, TriPortId tsiPortId,

TriParameterList paramList);

// Ref: TRI‑Definition 5.5.2.6

public TriStatus triEndTestCase();

// Message based communication operations

// Ref: TRI‑Definition 5.5.3.1

public TriStatus triSend(TriComponentId componentId, TriPortId tsiPortId,

TriAddress sutAddress, TriMessage sendMessage);

// Ref: TRI‑Definition 5.5.3.2

public TriStatus triSendBC(TriComponentId componentId, TriPortId tsiPortId,

TriMessage sendMessage);

// Ref: TRI‑Definition 5.5.3.3

public TriStatus triSendMC(TriComponentId componentId, TriPortId tsiPortId,

TriAddressList sutAddresses, TriMessage sendMessage);

// Procedure based communication operations

// Ref: TRI‑Definition 5.5.4.1

public TriStatus triCall(TriComponentId componentId,

TriPortId tsiPortId, TriAddress sutAddress,

TriSignatureId signatureId, TriParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.2

public TriStatus triCallBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId, TriParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.3

public TriStatus triCallMC(TriComponentId componentId,

TriPortId tsiPortId, TriAddressList sutAddresses,

TriSignatureId signatureId, TriParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.4

public TriStatus triReply(TriComponentId componentId,

TriPortId tsiPortId, TriAddress sutAddress,

TriSignatureId signatureId, TriParameterList parameterList,

TriParameter returnValue);

// Ref: TRI‑Definition 5.5.4.5

public TriStatus triReplyBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId, TriParameterList parameterList,

TriParameter returnValue);

// Ref: TRI‑Definition 5.5.4.6

public TriStatus triReplyMC(TriComponentId componentId,

TriPortId tsiPortId, TriAddressList sutAddresses,

TriSignatureId signatureId, TriParameterList parameterList,

TriParameter returnValue);

// Ref: TRI‑Definition 5.5.4.7

public TriStatus triRaise(TriComponentId componentId, TriPortId tsiPortId,

TriAddress sutAddress,

TriSignatureId signatureId,

TriException exc);

// Ref: TRI‑Definition 5.5.4.8

public TriStatus triRaiseBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId,

TriException exc);

// Ref: TRI‑Definition 5.5.4.9

public TriStatus triRaiseMC(TriComponentId componentId, TriPortId tsiPortId,

TriAddressList sutAddresses,

TriSignatureId signatureId,

TriException exc);

// Miscellaneous operations

// Ref: TRI‑Definition 5.5.5.1

public TriStatus triSutActionInformal(String description);

// Ref: TRI‑Definition 5.5.5.2

public TriStatus triSutActionParam(TriParameterList parameterList);

}

#### 6.5.2.2 triCommunicationTE

The triCommunicationTE interface is mapped to the following interface:

// TriCommunication

// SA ‑> TE

package org.etsi.ttcn.tri;

public interface TriCommunicationTE {

// Message based communication operations

// Ref: TRI‑Definition 5.5.3.4

public void triEnqueueMsg(TriPortId tsiPortId,

TriAddress sutAddress, TriComponentId componentId,

TriMessage receivedMessage);

// Procedure based communication operations

// Ref: TRI‑Definition 5.5.4.10

public void triEnqueueCall(TriPortId tsiPortId,

TriAddress sutAddress, TriComponentId componentId,

TriSignatureId signatureId, TriParameterList parameterList );

// Ref: TRI‑Definition 5.5.4.11

public void triEnqueueReply(TriPortId tsiPortId, TriAddress sutAddress,

TriComponentId componentId, TriSignatureId signatureId,

TriParameterList parameterList, TriParameter returnValue);

// Ref: TRI‑Definition 5.5.4.12

public void triEnqueueException(TriPortId tsiPortId,

TriAddress sutAddress, TriComponentId componentId,

TriSignatureId signatureId, TriException exc);

// Error handling

// Ref: TRI‑Definition 5.2.1

public void triSAErrorReq (String message);

}

### 6.5.3 triPlatform - Interface

#### 6.5.3.0 Introduction

The **triPlatform** interface is divided in two sub interfaces, the triPlatformPA interface, defining calls from the TE to the PA and the triPlatformTE interface, defining calls from the PA to the TE.

#### 6.5.3.1 TriPlatformPA

The triPlatformPA interface is mapped to the following interface:

// TriPlatform

// TE ‑> PA

package org.etsi.ttcn.tri;

public interface TriPlatformPA {

// Ref: TRI‑Definition 5.6.1

public TriStatus triPAReset();

// Timer handling operations

// Ref: TRI‑Definition 5.6.2.1

public TriStatus triStartTimer(TriTimerId timerId,

TriTimerDuration timerDuration);

// Ref: TRI‑Definition 5.6.2.2

public TriStatus triStopTimer(TriTimerId timerId);

// Ref: TRI‑Definition 5.6.2.3

public TriStatus triReadTimer(TriTimerId timerId,

TriTimerDuration elapsedTime);

// Ref: TRI‑Definition 5.6.2.4

public TriStatus triTimerRunning(TriTimerId timerId,

TriBoolean running);

// Miscellaneous operations

// Ref: TRI‑Definition 5.6.3.1

public TriStatus triExternalFunction(TriFunctionId functionId,

TriParameterList parameterList, TriParameter returnValue);

}

#### 6.5.3.2 TriPlatformTE

The triPlatformTE interface is mapped to the following Java interface:

// TriPlatform

// PA ‑> TE

package org.etsi.ttcn.tri;

public interface TriPlatformTE {

// Ref: TRI‑Definition 5.6.2.5

public void triTimeout(TriTimerId timerId);

// Error handling

// Ref: TRI‑Definition 5.2.2

public void triPAErrorReq (String message);

// Ref: TRI-Definition 5.6.3.2

public TriCompnentId triSelf();

// Ref: TRI-Definition 5.6.3.3

public TriMessage triRnd(TriComponentId componentId, TriMessage seed);

}

## 6.6 Optional parameters

Clause 5.4 defines that a reserved value shall be used to indicate the absence of an optional parameter. For the Java language mapping the Java null value shall be used to indicate the absence of an optional value. For example if in the triSend operation the address parameter shall be omitted the operation invocation shall be: triSend(componentId, tsiPortId, null, sendMessage).

## 6.7 TRI initialization

All methods are non‑static, i.e. operations can only be called on objects. As the present document does not define concrete implementation strategies of TE, SA and PA the mechanism how the TE, the SA, or the PA get to know the handles on the respective objects is out of scope of the present document.

Tool vendors shall provide methods to the developers of SA and PA to register the TE, SA and PA to their respective communication partner.

# 7 ANSI C language mapping

## 7.1 Introduction

This clause defines the TRI ANSI‑C language [6] mapping for the abstract data types specified in clause 5.3. For basic IDL types, the mapping conforms to OMG recommendations.

## 7.2 Names and scopes

### 7.2.0 Naming rules

C parameter identifiers shall start with a lower case letter, and subsequent part building the parameter identifier start with a capital letter. For example the IDL parameter SUTaddress maps to sutAddress in C.

Abstract data type identifiers in C are omitting the trailing Type used in the IDL definition. For example the IDL type TriPortIdType maps to TriPortId in C.

Older C specifications have restricted the identifier uniqueness to the most significant 8 characters. Nevertheless, the recent ANSI‑C specifications have moved this limitation to the 31 most significant characters. Aside from this issue, no naming or scope conflicts have been identified in this mapping.

### 7.2.1 Abstract type mapping

| TRI ADT | ANSI C Representation | Notes and comments |
| --- | --- | --- |
| TriAddress | BinaryString |  |
| TriAddressList | typedef struct TriAddressList  {  TriAddress\*\* addrList;  long int length;  } TriAddressList; | See note 1. |
| TriComponentId | typedef struct TriComponentId  {  BinaryString compInst;  String compName;  QualifiedName compType;  } TriComponentId; | See note 2. |
| TriComponentIdList | typedef struct TriComponentIdList  {  TriComponentId\*\* compIdList;  long int length;  } TriComponentIdList; | See note 3. |
| TriException | BinaryString |  |
| TriFunctionId | QualifiedName |  |
| TriMessage | BinaryString |  |
| TriParameterList | typedef struct TriParameterList  {  TriParameter\*\* parList;  long int length;  } TriParameterList; | See note 4. |
| TriParameter | typedef struct TriParameter  {  BinaryString par;  TriParameterPassingMode mode;  } TriParameter; |  |
| TriParameterPassingMode | typedef enum  {  TRI\_IN = 0,  TRI\_INOUT = 1,  TRI\_OUT = 2  } TriParameterPassingMode; | See note 5. |
| TriPortIdList | typedef struct TriPortIdList  {  TriPortId\*\* portIdList;  long int length;  } TriPortIdList; | See note 6. |
| TriPortId | typedef struct TriPortId  {  TriComponentId compInst;  char\* portName;  long int portIndex;  QualifiedName portType;  void\* aux;  } TriPortId; | See notes 7, 8 and 9. |
| TriSignatureId | QualifiedName |  |
| TriStatus | long int  #define TRI\_ERROR ‑1  #define TRI\_OK 0 | See note 10. |
| TriTestCaseId | QualifiedName |  |
| TriTimerDuration | Double |  |
| TriTimerId | BinaryString | See note 11. |
| NOTE 1: No special values mark the end of addrList[]. The length field shall be used to traverse this array properly.  NOTE 2: compInst is for component instance.  NOTE 3: No special values mark the end of compIdList[]. The length field shall be used to traverse this array properly.  NOTE 4: No special values mark the end of parList. The length field shall be used to traverse this array properly.  NOTE 5: The values of instances of this type shall reflect the parameter passing mode defined in the corresponding TTCN‑3 procedure signatures.  NOTE 6: No special values mark the end of portIdList[]. The length field shall be used to traverse this array properly.  NOTE 7: compInst is for component instance.  NOTE 8: For a singular (non‑array) declaration, the portIndex value should be ‑1.  NOTE 9: The aux field is for future extensibility of TRI functionality.  NOTE 10: All negative values are reserved for future extension of TRI functionality.  NOTE 11: Pending ETSI statement on timer and snapshot semantics may influence future representation! | | |

### 7.2.2 ANSI C type definitions

|  |  |  |
| --- | --- | --- |
| C ADT | Type definition | Notes and comments |
| BinaryString | typedef struct BinaryString  {  unsigned char\* data;  long int bits;  void\* aux;  } BinaryString; | See notes 1, 2 and 3. |
| QualifiedName | typedef struct QualifiedName  {  char\* moduleName;  char\* objectName;  void\* aux;  } QualifiedName; | See notes 4 and 5. |
| NOTE 1: data is a non‑null‑terminated string.  NOTE 2: bits is the number of bits used in data. bits value -1 is used to denote omitted value.  NOTE 3: The aux field is for future extensibility of TRI functionality.  NOTE 4: The moduleName and objectName fields are the TTCN‑3 identifiers literally.  NOTE 5: The aux field is for future extensibility of TRI functionality. | | |

### 7.2.3 IDL type mapping

|  |  |  |
| --- | --- | --- |
| IDL type | ANSI C Representation | Notes and comments |
| Boolean | unsigned char | From OMG IDL to C++ mapping |
| String | char\* | From OMG IDL to C++ mapping |

### 7.2.4 TRI operation mapping

| IDL Representation | ANSI C Representation |
| --- | --- |
| TriStatusType triSAReset() | TriStatus triSAReset() |
| TriStatusType triExecuteTestCase  (in TriTestCaseIdType testCaseId,  in TriPortIdListType tsiPortList) | TriStatus triExecuteTestCase  (const TriTestCaseId\* testCaseId,  const TriPortIdList\* tsiPortList) |
| TriStatusType triMap  (in TriPortIdType compPortId,  in TriPortIdType tsiPortId) | TriStatus triMap  (const TriPortId\* compPortId,  const TriPortId\* tsiPortId) |
| TriStatusType triMapParam  (in TriPortIdType compPortId,  in TriPortIdType tsiPortId,  in TriParameterListType paramList) | TriStatus triMapParam  (const TriPortId\* compPortId,  const TriPortId\* tsiPortId,  const TriParameterList\* paramList) |
| TriStatusType triUnmap  (in TriPortIdType compPortId,  in TriPortIdType tsiPortId) | TriStatus triUnmap  (const TriPortId\* compPortId,  const TriPortId\* tsiPortId) |
| TriStatusType triUnmapParam  (in TriPortIdType compPortId,  in TriPortIdType tsiPortId,  in TriParameterListType paramList) | TriStatus triUnmapParam  (const TriPortId\* compPortId,  const TriPortId\* tsiPortId,  const TriParameterList\* paramList) |
| TriStatusType triEndTestCase() | TriStatus triEndTestCase() |
| TriStatusType triSend  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriMessageType sendMessage) | TriStatus triSend  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriMessage\* sendMessage) |
| TriStatusType triSendBC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriMessageType sendMessage) | TriStatus triSendBC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriMessage\* sendMessage) |
| TriStatusType triSendMC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriMessageType sendMessage) | TriStatus triSendMC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddressList\* sutAddresses,  const TriMessage\* sendMessage) |
| void triEnqueueMsg  (in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriComponentIdType componentId,  in TriMessageType receivedMessage) | void triEnqueueMsg  (const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriComponentId\* componentId,  const TriMessage\* receivedMessage) |
| TriStatusType triCall  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) | TriStatus triCall  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList) |
| TriStatusType triCallBC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) | TriStatus triCallBC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList) |
| TriStatusType triCallMC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) | TriStatus triCallMC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddressList\* sutAddresses,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList) |
| TriStatusType triReply  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList,  in TriParameterType returnValue) | TriStatus triReply  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList,  const TriParameter\* returnValue) |
| TriStatusType triReplyBC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList,  in TriParameterType returnValue) | TriStatus triReplyBC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList,  const TriParameter\* returnValue) |
| TriStatusType triReplyMC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList,  in TriParameterType returnValue) | TriStatus triReplyMC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddressList\* sutAddresses,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList,  const TriParameter\* returnValue) |
| TriStatusType triRaise  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriSignatureIdType signatureId,  in TriExceptionType exc) | TriStatus triRaise  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriSignatureId\* signatureId,  const TriException\* exception) |
| TriStatusType triRaiseBC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriSignatureIdType signatureId,  in TriExceptionType exc) | TriStatus triRaiseBC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriSignatureId\* signatureId,  const TriException\* exception) |
| TriStatusType triRaiseMC  (in TriComponentIdType componentId,  in TriPortIdType tsiPortId,  in TriAddressListType SUTaddresses,  in TriSignatureIdType signatureId,  in TriExceptionType exc) | TriStatus triRaiseMC  (const TriComponentId\* componentId,  const TriPortId\* tsiPortId,  const TriAddressList\* sutAddresses,  const TriSignatureId\* signatureId,  const TriException\* exception) |
| void triEnqueueCall  (in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriComponentId componentId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList) | void triEnqueueCall  (const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriComponentId\* componentId,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList) |
| void triEnqueueReply  (in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TriParameterListType parameterList,  in TriParameterType returnValue) | void triEnqueueReply  (const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriComponentId\* componentId,  const TriSignatureId\* signatureId,  const TriParameterList\* parameterList,  const TriParameter\* returnValue) |
| void triEnqueueException  (in TriPortIdType tsiPortId,  in TriAddressType SUTaddress,  in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TriExceptionType exc) | void triEnqueueException  (const TriPortId\* tsiPortId,  const TriAddress\* sutAddress,  const TriComponentId\* componentId,  const TriSignatureId\* signatureId,  const TriException\* exception) |
| TriStatusType triSUTActionInformal  (in string description) | TriStatus triSUTActionInformal  (const char\* description) |
| TriStatusType triSUTActionParam  (in TriParameterListType parameterList) | TriStatus triSUTActionParam  (const TriParameterList\* parameterList) |
| TriStatusType triPAReset() | TriStatus triPAReset() |
| TriStatusType triStartTimer  (in TriTimerIdType timerId,  in TriTimerDurationType timerDuration) | TriStatus triStartTimer  (const TriTimerId\* timerId,  TriTimerDuration timerDuration) |
| TriStatusType triStopTimer  (in TriTimerIdType timerId) | TriStatus triStopTimer  (const TriTimerId\* timerId) |
| TriStatusType triReadTimer  (in TriTimerIdType timerId,  out TriTimerDurationType elapsedTime) | TriStatus triReadTimer  (const TriTimerId\* timerId,  TriTimerDuration\* elapsedTime) |
| TriStatusType triTimerRunning  (in TriTimerIdType timerId,  out boolean running) | TriStatus triTimerRunning  (const TriTimerId\* timerId,  unsigned char\* running) |
| void triTimeout  (in TriTimerIdType timerId) | void triTimeout  (const TriTimerId\* timerId) |
| TriStatusType triExternalFunction  (in TriFunctionIdType functionId,  inout TriParameterListType parameterList,  out TriParameterType returnValue) | TriStatus triExternalFunction  (const TriFunctionId\* functionId,  TriParameterList\* parameterList,  TriParameter\* returnValue) |
| TriComponentId triSelf() | TriComponentId triSelf() |
| TriMessage triRnd  (in TriComponentId self,  in TriMessage seed) | TriMessage triRnd  (const TriComponentId\* componentId,  const TriMessage\* seed) |
| void triPAErrorReq(in string message) | void triPAErrorReq(const char\* message) |
| void triSAErrorReq(in string message) | void triSAErrorReq(const char\* message) |

## 7.3 Memory management

The content of this clause is obsolete.

# 8 C++ language mapping

## 8.1 Introduction

This clause introduces the TRI C++ language [7] mapping for the definitions given in clause 5.

## 8.2 Names and scopes

The namespace ORG\_ETSI\_TTCN3\_TRI has been defined for the TRI C++ mapping, in order to avoid conflicts with the different names used, for example, in the C mapping.

C++ class identifiers are omitting the trailing "Type" at the end of the abstract definitions, e.g. the type TriMessageType is mapped to TriMessage in C++.

## 8.3 Memory management

A general policy for memory management is not defined in this mapping. However, parameters are passed as pointers (or references) where possible, and a clone method has been added to the definition of every interface. The clone method can be used by the receiving entity to make a local copy where needed.

## 8.4 Void

## 8.5 Type mapping

### 8.5.0 Basic rules

This clause introduces the TRI C++ language mapping for the abstract types defined in clause 5.3. The following concepts have been used:

* Pure classes have been used, following the concept of an interface.
* Basic data types have both set and get methods, so that they can be handled in a general way.
* The Standard Template Library (STL) has been used as it is a standardized way of using container classes, and iterators, such as lists. All classes define the operator "<" for easy insertion in STL containers.
* C++ types have been encapsulated under abstract definitions, like Tfloat or Tinteger.

### 8.5.1 Encapsulated C++ types

The following types have been defined in order to keep the definitions of data types and operations as general as possible:

* Boolean type definition: typedef bool Tboolean.
* Integer type definition: typedef long int Tinteger.
* Size type definition: typedef unsigned long int Tsize.
* Float type definition: typedef double Tfloat.
* Byte type definition: typedef unsigned char Tbyte.
* String type definition: typedef std::string Tstring.

### 8.5.2 Abstract data types

#### 8.5.2.1 QualifiedName

This class defines a qualified TTCN-3 identifier: moduleName and objectName. It is mapped to the following pure virtual class:

class QualifiedName {

public:

~QualifiedName ();

const Tstring & getModuleName () const = 0;

void setModuleName (const Tstring &mName) = 0;

const Tstring & getObjectName () const = 0;

void setObjectName (const Tstring &oName) = 0;

Tboolean equals (const QualifiedName &qn) const = 0;

QualifiedName \* cloneQualifiedName () const = 0;

Tboolean operator< (const QualifiedName &qn) const = 0;

}

**Methods:**

* ~QualifiedName

Destructor.

* getModuleName

Gets the module name as string value.

* setModuleName

Set the module name from string parameter.

* getObjectName

Gets the object name as string value.

* setObjectName

Set the object name from string parameter.

* operator==

Returns true if both objects are equal.

* cloneQualifiedName

Returns a copy of the QualifiedName.

* operator<

Operator < overload.

#### 8.5.2.2 TriAddress

A value of type TriAddress indicates a source or destination address within the SUT. The TriAddress class contains a C++ template: TAddress. It is mapped to the following pure virtual class:

class TriAddress {

public:

virtual ~TriAddress ();

virtual const Tbyte \*getEncodedData()const=0;

virtual void setEncodedData(const Tbyte \*str, Tsize bitLen)=0;

virtual Tsize getBitsDataLen()const=0;

virtual Tboolean operator== (const TriAddress &add) const =0;

virtual TriAddress \* cloneAddress () const =0;

virtual Tboolean operator< (const TriAddress &add) const =0;

}

**Methods:**

* ~TriAddress

Destructor.

* getEncodedData

Gets the encoded address.

* setEncodedData

Sets the encoded address.

* getBitsDataLen

Gets address length.

* operator==

Returns true if both TriAddress objects are equal.

* cloneAddress

Returns a copy of the TriAddress.

* operator<

Operator < overload.

#### 8.5.2.3 TriAddressList

The value of this type is a list of TriAddress elements. This abstract type is used for multicast communication in TRI. It is mapped to the following pure virtual class:

class TriAddressList {

public:

virtual ~TriAddressList ();

virtual Tsize size () const =0;

virtual Tboolean isEmpty () const =0;

virtual const TriAddress & get (Tsize index) const =0;

virtual void clear ()=0;

virtual void add (const TriAddress &elem)=0;

virtual Tboolean operator== (const TriAddressList &addl) const =0;

virtual TriAddressList \* cloneAddressList () const =0;

virtual Tboolean operator< (const TriAddressList &addl) const =0;

}

**Methods:**

* ~TriAddressList

Destructor.

* size

Returns the number of addresses in the list.

* isEmpty

Returns true if address list is empty.

* get

Gets TriAddress element at specified position from the address list.

* clear

Removes all TriAddress elements from the list.

* add

Adds a TriAddress element to the list.

* operator==

Returns true if both TriAddressList objects are equal.

* cloneAddressList

Returns a copy of the TriAddressList.

* operator<

Operator < overload.

#### 8.5.2.4 TriComponentId

A value of type TriComponentId includes an identifier, a name and the component type. This abstract type is mainly used to resolve TRI communication operations on TSI ports that have mappings to many test component ports. It is mapped to the following pure virtual class:

class TriComponentId {

public:

virtual ~TriComponentId ();

virtual const QualifiedName & getComponentTypeName () const =0;

virtual void setComponentTypeName (const QualifiedName &tName)=0;

virtual const Tstring & getComponentName () const =0;

virtual void setComponentName (const Tstring &sName)=0;

virtual const Tinteger & getComponentId () const =0;

virtual void setComponentId (const Tinteger &id)=0;

virtual Tboolean operator== (const TriComponentId &cmp) const =0;

virtual TriComponentId \* cloneComponentId () const =0;

virtual Tboolean operator< (const TriComponentId &cmp) const =0;

}

**Methods:**

* ~TriComponentId

Destructor.

* getComponentTypeName

Returns a const reference to the component type name.

* setComponentTypeName

Set the component type name.

* getComponentName

Gets the component name.

* setComponentName

Set the component name.

* getComponentId

Returns the component identifier.

* setComponentId

Set the component identifier.

* operator==

Returns true if both TriComponentId objects are equal.

* cloneComponentId

Returns a copy of the TriComponentId.

* operator<

Operator < overload.

#### 8.5.2.5 TriComponentIdList

This abstract type defines a list of TriComponentId elements. It is mapped to the following pure virtual class:

class TriComponentIdList {

public:

virtual ~TriComponentIdList ();

virtual Tsize size () const =0;

virtual Tboolean isEmpty () const =0;

virtual const TriComponentId & get (Tsize index)const=0;

virtual void clear ()=0;

virtual void add (const TriComponentId &comp)=0;

virtual Tboolean operator== (const TriComponentIdList &cmpl) const =0;

virtual TriComponentIdList \* cloneComponentIdList () const =0;

virtual Tboolean operator< (const TriComponentIdList &cmpl) const =0;

}

**Methods:**

* ~TriComponentIdList

Destructor.

* size

Returns the number of components in the list.

* isEmpty

Returns true if this list contains no components.

* get

Returns the component at the specified position.

* clear

Removes all the components from this list.

* add

Adds a component to the end of this list.

* operator==

Returns true if both TriComponentIdList are equal.

* cloneComponentIdList

Returns a copy of the TriComponentIdList.

* operator<

Operator < overload.

#### 8.5.2.6 TriException

A value of type TriException is an encoded type and value of an exception that either is to be sent to the SUT or has been received from the SUT. This abstract type is used in procedure based TRI communication operations. It is mapped to the following pure virtual class:

class TriException {

public:

virtual ~TriException ();

virtual const Tbyte \*getData()const=0;

virtual void setData(const Tbyte \*str, Tsize bitLen)=0;

virtual Tsize getBitsDataLen()const=0;

virtual Tboolean operator== (const TriException &exc)const=0;

virtual TriException \* cloneException () const =0;

virtual Tboolean operator< (const TriException &exc) const =0;

}

**Methods:**

* ~TriException

Destructor.

* getData

Gets binary string data (array of characters).

* setData

Set the binary string data (array of characters).

* getBitsDataLen

Gets data length.

* operator==

Returns true if both TriException objects are equal.

* cloneException

Returns a copy of the TriException.

* operator<

Operator < overload.

#### 8.5.2.7 TriFunctionId

A value of type TriFunctionId is the name of a function as specified in the TTCN-3 ATS. It is a derived class from QualifiedName, mapped to the following pure virtual class:

class TriFunctionId : public QualifiedName {

public:

virtual ~TriFunctionId ();

virtual Tboolean operator== (const TriFunctionId &fid) const =0;

virtual TriFunctionId \* cloneFunctionId () const =0;

virtual Tboolean operator< (const TriFunctionId &fid) const =0;

}

**Methods:**

* ~TriFunctionId

Destructor.

* operator==

Returns true if both TriFunctionId objects are equal.

* cloneFunctionId

Returns a copy of the TriFunctionId.

* operator<

Operator < overload.

#### 8.5.2.8 TriMessage

A value of type TriMessage is encoded test data that either is to be sent to the SUT or has been received from the SUT. It is mapped to following pure virtual class:

class TriMessage {

public:

virtual ~TriMessage ();

virtual const Tbyte \*getData()const=0;

virtual void setData(const Tbyte \*str, Tsize bitLen)=0;

virtual Tsize getBitsDataLen()const=0;

virtual Tboolean operator== (const TriMessage &msg) const =0;

virtual TriMessage \* cloneMessage () const =0;

virtual Tboolean operator< (const TriMessage &msg) const =0;

}

**Methods:**

* ~TriMessage

Destructor.

* getData

Gets binary string data (array of characters).

* setData

Set the binary string data (array of characters).

* getBitsDataLen

Gets data length.

* operator==

Returns true if both TriMessage objects are equal.

* cloneMessage

Returns a copy of the TriMessage.

* operator<

Operator < overload.

#### 8.5.2.9 TriParameter

A value of type TriParameter includes an encoded parameter and a value of TriParameterPassingMode to represent the passing mode specified for the parameter in the TTCN-3 ATS. It is mapped to the following pure virtual class:

class TriParameter {

public:

virtual ~TriParameter ();

virtual const Tstring & getParameterName () const =0;

virtual void setParameterName (const Tstring &name)=0;

virtual const TriParameterPassingMode & getParameterPassingMode () const =0;

virtual void setParameterPassingMode (const TriParameterPassingMode &mode)=0;

virtual const Tbyte \*getEncodedParameter()const=0;

virtual void setEncodedParameter(const Tbyte \*str, Tsize bitLen)=0;

virtual Tsize getBitsDataLen()const=0;

virtual Tboolean operator== (const TriParameter &par) const =0;

virtual TriParameter \* cloneParameter () const =0;

virtual Tboolean operator< (const TriParameter &par) const =0;

}

**Methods:**

* ~TriParameter

Destructor.

* getParameterName

Returns the parameter name as defined in the TTCN-3 specification.

* setParameterName

Set the parameter name.

* getParameterPassingMode

Returns the parameter passing mode of this parameter.

* setParameterPassingMode

Set the parameter passing mode.

* getEncodedParameter

Gets the encoded parameter.

* setEncodedParameter

Sets the encoded parameter.

* getBitsDataLen

Gets parameter length.

* operator==

Returns true if both TriParameter objects are equal.

* cloneParameter

Returns a copy of the TriParameter.

* operator<

Operator < overload.

#### 8.5.2.10 TriParameterList

A value of type TriParameterList is a list of TriParameterType. This abstract type is used in procedure based TRI communication operations and for external function calls. It is mapped to the following pure virtual class:

class TriParameterList {

public:

virtual ~TriParameterList ();

virtual Tsize size () const =0;

virtual Tboolean isEmpty () const =0;

virtual const TriParameter & get (Tsize index) const =0;

virtual void clear ()=0;

virtual void add (const TriParameter &parameter)=0;

virtual Tboolean operator== (const TriParameterList &pml) const =0;

virtual TriParameterList \* cloneParameterList () const =0;

virtual Tboolean operator< (const TriParameterList &pml) const =0;

}

**Methods:**

* ~TriParameterList

Destructor.

* size

Returns the number of parameters in this list.

* isEmpty

Returns true if this list contains no parameters.

* get

Returns the TriParameter at the specified position.

* clear

Removes all parameters from this TriParameterList.

* add

Adds parameter to the end of this TriParameterList.

* operator==

Returns true if both TriParameterList objects are equal.

* cloneParameterList

Returns a copy of the TriParameterList.

* operator<

Operator < overload.

#### 8.5.2.11 TriParameterPassingMode

Defines the parameter passing mode. It is mapped to an enumeration:

typedef enum

{

IN = 0,

OUT = 1,

INOUT = 2

} TriParameterPassingMode;

#### 8.5.2.12 TriPortId

A value of type TriPortId includes a value of type TriComponentIdType to represent the component to which the port belongs, a port index (if present), and the port name as specified in the TTCN-3 ATS. The TriPortId type is mainly required to pass information about the TSI and connections to the TSI from the TE to the SA. It is mapped to the following pure virtual class:

class TriPortId {

public:

virtual ~TriPortId (void);

virtual const Tstring & getPortName () const =0;

virtual void setPortName (const Tstring &pName)=0;

virtual const TriComponentId & getComponent () const =0;

virtual void setComponent (const TriComponentId &comp)=0;

virtual Tsize getPortIndex () const =0;

virtual void setPortIndex (Tsize index)=0;

virtual const QualifiedName & getPortType () const =0;

virtual void setPortType (const QualifiedName &pType)=0;

virtual Tboolean isArray () const =0;

virtual Tboolean operator== (const TriPortId &prt) const =0;

virtual TriPortId \* clonePortId () const =0;

virtual Tboolean operator< (const TriPortId &prt) const =0;

}

**Methods:**

* ~TriPortId

Destructor.

* getPortName

Returns the port name.

* setPortName

Set the port name.

* getComponent

Returns the component identifier that this TRI port belongs to.

* setComponent

Set the component identifier that this port belongs to.

* getPortIndex

Gets the port index (0..N). Returns -1 if it is not part of an array.

* setPortIndex

Set the port index.

* getPortType

Gets the port type.

* setPortType

Set the port type.

* isArray

Returns true if port is defined as part of an array.

* operator==

Returns true if both TriPortId objects are equal.

* clonePortId

Returns a copy of the TriPortId.

* operator<

Operator < overload.

#### 8.5.2.13 TriPortIdList

The value of this type is a list of TriPortIdType elements. It is mapped to the following pure virtual class:

class TriPortIdList {

public:

virtual ~TriPortIdList ();

virtual Tsize size () const =0;

virtual bool isEmpty () const =0;

virtual const TriPortId & get (Tsize index) const =0;

virtual void clear ()=0;

virtual void add (const TriPortId &elem)=0;

virtual Tboolean operator== (const TriPortIdList &prtl) const =0;

virtual TriPortIdList \* clonePortIdList () const =0;

virtual Tboolean operator< (const TriPortIdList &prtl) const =0;

}

**Methods:**

* ~TriPortIdList

Destructor.

* size

Returns the number of ports in this list.

* isEmpty

Returns true if port list is empty.

* get

Gets TriPortIdType element at position index from the port list.

* clear

Removes all TriPortIdType elements from the list.

* add

Adds a TriPortIdType element to the list.

* operator==

Returns true if both TriPortIdList objects are equal.

* clonePortIdList

Returns a copy of the TriPortIdList.

* operator<

Operator < overload.

#### 8.5.2.14 TriSignatureId

A value of type TriSignatureIdType is the name of a procedure signature as specified in the TTCN-3 ATS. It is a derived class from QualifiedName, mapped to the following pure virtual class:

class TriSignatureId : public QualifiedName {

public:

virtual ~TriSignatureId ();

virtual Tboolean operator== (const TriSignatureId &sid) const =0;

virtual TriSignatureId \* cloneSignatureId () const =0;

virtual Tboolean operator< (const TriSignatureId &sid) const =0;

}

**Methods:**

* ~TriSignatureId

Destructor.

* operator==

Returns true if both TriSignatureId objects are equal.

* cloneSignatureId

Returns a copy of the TriSignatureId.

* operator<

Operator < overload.

#### 8.5.2.15 TriStatus

Defines TRI status as an enumeration:

typedef enum

{

TRI\_OK = 0,

TRI\_ERROR = -1

} TriStatus;

#### 8.5.2.16 TriTestCaseId

A value of type TriTestCaseId is the name of a test case as specified in the TTCN-3 ATS. It is a derived class from QualifiedName, mapped to the following pure virtual class:

class TriTestCaseId : public QualifiedName {

public:

virtual ~TriTestCaseId ();

virtual Tboolean operator== (const TriTestCaseId &tcid) const =0;

virtual TriTestCaseId \* cloneTestCaseId () const =0;

virtual Tboolean operator< (const TriTestCaseId &tcid) const =0;

}

**Methods:**

* ~TriTestCaseId

Destructor.

* operator==

Returns true if both TriTestCaseId objects are equal.

* cloneTestCaseId

Returns a copy of the TriTestCaseId.

* operator<

Operator < overload.

#### 8.5.2.17 TriTimerDuration

A value of type TriTimerDuration specifies the duration for a timer in seconds. It is mapped to the following pure virtual class:

class TriTimerDuration {

public:

virtual ~TriTimerDuration ();

virtual Tfloat getDuration () const =0;

virtual void setDuration (Tfloat duration)=0;

virtual Tboolean operator== (const TriTimerDuration &timd) const =0;

virtual TriTimerDuration \* cloneTimerDuration () const =0;

virtual Tboolean operator< (const TriTimerDuration &timd) const =0;

}

**Methods:**

* ~TriTimerDuration

Destructor.

* getDuration

Gets the timer duration time.

* setDuration

Set the timer duration time from "duration" value.

* operator==

Returns true if both TriTimerDuration objects are equal.

* cloneTimerDuration

Returns a copy of the TriTimerDuration.

* operator<

Operator < overload.

#### 8.5.2.18 TriTimerId

A value of type TriTimerId specifies an identifier for a timer. This type is required for all TRI timer operations. It is mapped to the following pure virtual class:

class TriTimerId {

public:

virtual ~TriTimerId ();

virtual const Tstring & getTimerName () const =0;

virtual void setTimerName (const Tstring &tName)=0;

virtual const Tinteger getTId() const =0;

virtual Tboolean operator== (const TriTimerId &tmid) const =0;

virtual TriTimerId \* cloneTimerId () const =0;

virtual Tboolean operator< (const TriTimerId &tmid) const =0;

}

**Methods:**

* ~TriTimerId

Destructor.

* getTimerName

Returns the timer id name (string value).

* setTimerName

Sets the timer id name.

* getTId

Returns the timer identification as integer.

* operator==

Returns true if both TriTimerId objects are equal.

* cloneTimerId

Returns a copy of the TriTimerId.

* operator<

Operator < overload.

## 8.6 Mapping of interfaces

### 8.6.1 TriCommunicationSA

This interface consists of operations that are necessary to implement the communication of the TTCN-3 ETS with the SUT. It is mapped to the following pure virtual class:

class TriCommunicationSA {

public:

//Destructor.

virtual ~TriCommunicationSA ();

//To reset the System Adaptor

virtual TriStatus triSAReset ()=0;

//To execute a test case.

virtual TriStatus triExecuteTestCase (const TriTestCaseId \*testCaseId, const TriPortIdList \*tsiPortList)=0;

//To establish a dynamic connection between two ports.

virtual TriStatus triMap (const TriPortId \*comPortId, const TriPortId \*tsiPortId)=0;

//To establish a dynamic connection between two ports including configuration parameters.

virtual TriStatus triMapParam (const TriPortId \*comPortId, const TriPortId \*tsiPortId,

const TriParameterList \*paramList)=0;

//To close a dynamic connection to the SUT for the referenced TSI port.

virtual TriStatus triUnmap (const TriPortId \*comPortId, const TriPortId \*tsiPortId)=0;

//To close a dynamic connection to the SUT for the referenced TSI port

//including configuration parameters.

virtual TriStatus triUnmapParam (const TriPortId \*comPortId, const TriPortId \*tsiPortId,

const TriParameterList \*paramList)=0;

//To end a test case.

virtual TriStatus triEndTestCase ()=0;

//Send operation on a component which has been mapped to a TSI port.

virtual TriStatus triSend (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddress \*SUTaddress, const TriMessage \*sendMessage)=0;

//Send (broadcast) operation on a component which has been mapped to a TSI port.

virtual TriStatus triSendBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriMessage \*sendMessage)=0;

//Send (multicast) operation on a component which has been mapped to a TSI port.

virtual TriStatus triSendMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddressList \*SUTaddresses, const TriMessage \*sendMessage)=0;

//Initiate the procedure call.

virtual TriStatus triCall (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddress \*sutAddress, const TriSignatureId \*signatureId, const TriParameterList \*parameterList)=0;

//Initiate and broadcast the procedure call.

virtual TriStatus triCallBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TriParameterList \*parameterList)=0;

//Initiate and multicast the procedure call.

virtual TriStatus triCallMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddressList \*sutAddresses, const TriSignatureId \*signatureId, const TriParameterList \*parameterList)=0;

//Issue the reply to a procedure call.

virtual TriStatus triReply (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddress \*sutAddress, const TriSignatureId \*signatureId, const TriParameterList \* parameterList, const TriParameter \*returnValue)=0;

//Broadcast the reply to a procedure call.

virtual TriStatus triReplyBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TriParameterList \*parameterList, const TriParameter \*returnValue)=0;

//Multicast the reply to a procedure call.

virtual TriStatus triReplyMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddressList \*sutAddresses, const TriSignatureId \*signatureId, const TriParameterList \*parameterList, const TriParameter \*returnValue)=0;

//Raise an exception to a procedure call.

virtual TriStatus triRaise (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddress \*sutAddress, const TriSignatureId \*signatureId, const TriException \*exc)=0;

//Raise an broadcast an exception to a procedure call.

virtual TriStatus triRaiseBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TriException \*exc)=0;

//Raise an multicast an exception to a procedure call.

virtual TriStatus triRaiseMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriAddressList \*sutAddresses, const TriSignatureId \*signatureId, const TriException \*exc)=0;

//Initiate the described actions to be taken on the SUT.

virtual TriStatus triSUTactionInformal (const Tstring \*description)=0;

//Initiate the described actions to be taken on the SUT with parameters.

virtual TriStatus triSUTactionParam (const TriParameterList \*parameterList)=0;

}

### 8.6.2 TriCommunicationTE

This interface consists of operations that are necessary to implement the communication of the SUT with the TTCN-3 ETS. It is mapped to the following pure virtual class:

class TriCommunicationTE {

public:

//Destructor.

virtual ~TriCommunicationTE ();

//Called by SA after it has received a message from the SUT.

virtual void triEnqueueMsg (const TriPortId \*tsiPortId, const TriAddress \*SUTaddress, const TriComponentId \*componentId, const TriMessage \*receivedMessage)=0;

//Called by SA after it has received a procedure call from the SUT.

virtual void triEnqueueCall (const TriPortId \*tsiPortId, const TriAddress \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const TriParameterList \*parameterList)=0;

//Called by SA after it has received a reply from the SUT.

virtual void triEnqueueReply (const TriPortId \*tsiPortId, const TriAddress \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const TriParameterList \*parameterList, const TriParameter \*returnValue)=0;

//Called by SA after it has received an exception from the SUT.

virtual void triEnqueueException (const TriPortId \*tsiPortId, const TriAddress \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const TriException \*exc)=0;

//Called by SA in unrecoverable error situations.

virtual void triSAError (const Tstring &message)=0;

}

### 8.6.3 TriPlatformPA

This interface consists of operations that are necessary to implement the communication of the TTCN-3 ETS with the platform, in which the testcase is running. It is mapped to the following pure virtual class:

class TriPlatformPA {

public:

//Destructor.

virtual ~TriPlatformPA ();

//Reset all timing activities which It is currently performing.

virtual TriStatus triPAReset ()=0;

//Start the indicated timer with the indicated duration.

virtual TriStatus triStartTimer (const TriTimerId \*timerId, const TriTimerDuration \*timerDuration)=0;

//Stop the indicated timer.

virtual TriStatus triStopTimer (const TriTimerId \*timerId)=0;

//Use the timerId to access the time that elapsed since this timer was started.

virtual TriStatus triReadTimer (const TriTimerId \*timerId, TriTimerDuration \*elapsedTime)=0;

//Use the timerId to access the status of the timer.

virtual TriStatus triTimerRunning (const TriTimerId \*timerId, Tboolean \* running)=0;

//For each external function specified in the TTCN-3 ATS implement the behaviour.

virtual TriStatus triExternalFunction (const TriFunctionId \*functionId, TriParameterList \*parameterList, TriParameter \*returnValue)=0;

}

### 8.6.4 TriPlatformTE

This interface consists of operations that are necessary to implement the communication of the platform, in which the testcase is running, with the TTCN-3 ETS. It is mapped to the following pure virtual class:

class TriPlatformTE {

public:

//Destructor.

virtual ~TriPlatformTE ();

//Notify the timeout of the timer.

virtual void triTimeout (const TriTimerId \*timerId)=0;

//Called by PA in unrecoverable error situations.

virtual void triPAError (const Tstring &message)=0;

//Called by PA inside external function

virtual TriComponentId \*triSelf ()=0;

//Generate random number.

virtual TriMessage\* triRnd (const TriComponentId \*componentId, const TriMessage \*seed)=0;

}

# 9 C# language mapping

## 9.1 Introduction

The C# mapping for the TTCN-3 Runtime Interface defines how the IDL definitions described in clause 5 are mapped to C# [8].

## 9.2 Names and scopes

### 9.2.1 Names

Although there are no conflicts between identifiers used in the IDL definition and C# some naming translation rules are applied to the IDL identifiers.

C# parameter identifiers shall start with a lower case letter and subsequent part building the parameter identifier start with a capital letter.

EXAMPLE 1: The IDL parameter identifier **SUTaddress** maps to sutAddress in C#.

C# interfaces are omitting the trailing Type used in the IDL definition. In addition to that, the capital letter "I" is added to the beginning of interface names.

EXAMPLE 2: The IDl type **TriPortIdType** maps to ITriPortId in C#.

The resulting mapping conforms to the standard C# coding conventions.

### 9.2.2 Scopes

The IDL module triInterface is mapped to the namespace Etsi.Ttcn3.Tri. All IDL type declarations within this module are mapped to C# interface declarations within this namespace. The associated assembly file is Etsi.Ttcn3.Tri.dll.

## 9.3 Null value mapping

The distinct value null specified in the IDL definition is equal to null in C#.

## 9.4 Type mapping

### 9.4.1 Basic type mapping

#### 9.4.1.0 IDL type mapping

Table 5 gives an overview on how the used basic IDL types are mapped to the C# types.

Table 5: Basic type mappings

| IDL Type | C# Type/Interface |
| --- | --- |
| boolean | Etsi.Ttcn3.Tri.ITriBoolean |
| string | string |

Other IDL basic types are not used within the IDL definition.

#### 9.4.1.1 Boolean

The IDL boolean type is mapped to the interface Etsi.Ttcn3.Tri.ITriBoolean, so that objects implementing this interface can act as holder objects.

The following interface is defined for Etsi.Ttcn3.Tri.ItriBoolean:

public interface ITriBoolean {  
 bool BooleanValue { get; set; }  
}

**Members:**

* BooleanValue  
  Gets or sets the boolean value associated with the object.

#### 9.4.1.2 String

The IDL string type is mapped to the System.String class without range checking or bounds for characters in the string. All possible strings defined in TTCN-3 can be converted to System.String.

### 9.4.2 Structured type mapping

#### 9.4.2.0 Mapping rules

The TRI IDL description defines user-defined types as native types. In the C# mapping, these types are mapped to C# interfaces. The interfaces define methods and properties being available for classes implementing this interface.

#### 9.4.2.1 IQualifiedName

**IQualifiedName** interface represents a TTCN-3 identifier. Although it is not specified in the TRI IDL description, it is used as parent type of several other C# interfaces which are present in the IDL description. It is also common type of TRI properties containing TTCN-3 type references. The interface is defined as follows:

public interface IQualifiedName {  
 string ModuleName { get; }  
 string BaseName { get; }  
 bool Equals(IQualifiedName name);  
}

**Members:**

* ModuleName  
  Returns the name of the module where the identifier is defined.
* BaseName  
  Returns the name of the identifier.
* Equals  
  Compares a qualified name with this IQualifiedName for equality. Returns true if and only if the module and base name of both instances are equal, false otherwise.

#### 9.4.2.2 TriPortIdType

**TriPortIdType** is mapped to the following interface:

public interface ITriPortId {  
 string PortName { get; }  
 ITriComponentId Component { get; }  
 bool IsArray { get; }  
 int PortIndex { get; }  
 IQualifiedName PortTypeName { get; }  
}

**Members:**

* PortName  
  Returns the port name as defined in the TTCN-3 specification.
* PortTypeName  
  Returns the port type name as defined in the TTCN-3 specification.
* Component  
  Returns the component identifier that this ITriPortId belongs to as defined in the TTCN-3 specification.
* IsArray  
  Returns true if this port is part of a port array, false otherwise.
* PortIndex  
  Returns the port index if this port is part of a port array starting at zero. If the port is not part of a port array, then -1 is returned.

#### 9.4.2.3 TriPortIdListType

**TriPortIdListType** is mapped to the following interface:

public interface ITriPortIdList   
 : System.Collections.IEnumerable {  
 int Size { get; }  
 bool IsEmpty { get; }  
 ITriPortId this[int index] { get; }  
}

**Members:**

* Size  
  Returns the number of ports in this list.
* IsEmpty  
  Returns true if this list contains no ports.
* getEnumerator  
  Inherited from IEnumerable. Returns an enumerator for this object and allows to use the list in a foreach loop.
* Indexing operator  
  Returns a ITriPortId instance at the specified position. IndexOutOfRangeException is thrown if the index is less than zero or greater or equal to the list size.

#### 9.4.2.4 TriComponentIdType

**TriComponentIdType** is mapped to the following interface:

public interface ITriComponentId {  
 string ComponentId { get; }  
 string ComponentName { get; }  
 IQualifiedName ComponentTypeName { get; }  
 bool Equals(ITriComponentId comp);  
}

**Members:**

* ComponentId  
  Returns a representation of this unique component identifier.
* ComponentName  
  Returns the component name as defined in the TTCN-3 specification. If no name is provided, null is returned.
* ComponentTypeName  
  Returns the component type name as defined in the TTCN-3 specification.
* Equals  
  Compares component with this TriComponentId for equality. Returns true if and only if both components have the same representation of this unique component identifier, false otherwise.

#### 9.4.2.5 TriComponentIdListType

**TriComponentIdListType** is mapped to the following interface:

public interface ITriComponentIdList: System.Collections.IEnumerable {  
 int Size { get; }  
 bool IsEmpty { get; }  
 ITriComponentId this[int index] { get; }  
 void Clear();  
 void Add(ITriComponentId comp);  
}

**Members:**

* Size  
  Returns the number of components in this list.
* IsEmpty  
  Returns true if this list contains no components.
* getEnumerator  
  Inherited from IEnumerable. Returns an enumerator for this object and allows to use the list in a foreach loop.
* Indexing operator  
  Returns a ITriComponentId instance at the specified position. IndexOutOfRangeException is thrown if the index is less than zero or greater or equal to the list size.
* Clear  
  Removes all components from the list.
* Add  
  Adds a component to the end of the list.

#### 9.4.2.6 TriMessageType

**TriMessageType** is mapped to the following interface:

public interface ITriMessage {  
 byte [] EncodedMessage { get; set; }  
 int NumberOfBits { get; }  
 void SetEncodedMessage(byte[] data, int numberOfBits);  
 bool Equals(ITriMessage msg);  
}

**Members:**

* EncodedMessage  
  Gets or sets the message encoded according the coding rules defined in the TTCN-3 specification. In case the message is set, the property assignment call produces the same result as calling the SetEncodedMessage method with the second parameter equal to byte array length \* 8.
* NumberOfBits  
  Returns the amount of bits of the message.
* SetEncodedMessage  
  Sets the encoded message representation of this TriMessage to message. The number of bits has to be less or equal to data.Length \* 8.
* Equals  
  Compares a message with this TriMessage for equality. Returns true if and only if both messages have  
  the same encoded representation, false otherwise.

#### 9.4.2.7 TriAddressType

**TriAddressType** is mapped to the following interface:

public interface ITriAddress {  
 byte [] EncodedAddress { get; set; }  
 bool Equals(ITriAddress addr);  
 void SetEncodedAddress(byte[] data, int numberOfBits);  
 int NumberOfBits { get; }  
}

**Methods:**

* EncodedAddress  
  Gets or sets the encoded address.
* Equals  
  Compares an address with this ITriAddress for equality. Returns true if and only if both addresses have the same encoded representation, false otherwise.
* SetEncodedAddress  
  Sets the encoded address value of this ITriAddress together with the number of valid bits. The number of bits shall be less or equal to data.Length \* 8.
* NumberOfBits  
  Returns the amount of bits of the encoded address.

#### 9.4.2.8 TriAddressListType

**TriAddressListType** is mapped to the following interface:

public interface ITriAddressList: System.Collections.IEnumerable {  
 int Size { get; }  
 bool IsEmpty { get; }  
 ITriAddress this[int index] { get; }  
 void Clear();  
 void Add(ITriAddress addr);  
}

**Members:**

* Size  
  Returns the number of addresses in this list.
* IsEmpty  
  Returns true if this list contains no addresses.
* getEnumerator  
  Inherited from IEnumerable. Returns an enumerator for this object and allows to use the list in a foreach loop.
* Indexing operator  
  Returns a ITriAddress instance at the specified position. IndexOutOfRangeException is thrown if the index is less than zero or greater or equal to the list size.
* Clear  
  Removes all addresses from the list.
* Add  
  Adds an address to the end of the list.

#### 9.4.2.9 TriSignatureIdType

**TriSignatureIdType** C# mapping is derived from the IQualifiedName interface:

public interface ITriSignatureId : IQualifiedName {}

#### 9.4.2.10 TriParameterPassingModeType

**TriParameterPassingModeType** is mapped to the following enumeration:

public enum TriParameterPassingMode {   
 TriIn = 0,   
 TriInOut = 1,   
 TriOut =2   
}

#### 9.4.2.11 TriParameterType

**TriParameterType** is mapped to the following interface:

public interface ITriParameter {  
 string ParameterName { get; set; }  
 TriParameterPassingMode ParameterPassingMode { get; set; }  
 byte [] EncodedParameter { get; set; }  
 void SetEncodedParameter(byte[] data, int numberOfBits);  
 int NumberOfBits { get; }  
}

**Members:**

* ParameterName  
  Gets or sets the parameter name.
* ParameterPassingMode  
  Gets or sets the parameter passing mode of this parameter.
* EncodedParameter  
  Gets or sets the encoded representation of this TriParameter, or the null object if the parameter contains the distinct value null (see also clause 5.5.4). The null value is used to indicate that this parameter holds no value.
* SetEncodedParameter  
  Sets the encoded parameter value of this ITriParameter together with the number of valid bits. The number of bits shall be less or equal to data.Length \* 8.
* NumberOfBits  
  Returns the amount of bits of the encoded parameter.

#### 9.4.2.12 TriParameterListType

**TriParameterListType** is mapped to the following interface:

public interface ITriParameterList: System.Collections.IEnumerable {  
 int Size { get; }  
 bool IsEmpty { get; }  
 ITriParameterId this[int index] { get; }  
 void Clear();  
 void Add(ITriParameter comp);  
}

**Members:**

* Size  
  Returns the number of parameters in this list.
* IsEmpty  
  Returns true if this list contains no parameters.
* getEnumerator  
  Inherited from IEnumerable. Returns an enumerator for this object and allows to use the list in a foreach loop.
* Indexing operator  
  Returns a ITriParameter instance at the specified position. IndexOutOfRangeException is thrown if the index is less than zero or greater or equal to the list size.
* Clear  
  Removes all parameters from the list.
* Add  
  Adds a parameter to the end of the list.

#### 9.4.2.13 TriExceptionType

**TriExceptionType** is mapped to the following interface:

public interface ITriException {  
 byte [] EncodedException { get; set; }  
 bool Equals(ITriException exception);  
 void SetEncodedException(byte[] data, int numberOfBits);  
 int NumberOfBits { get; }  
}

**Methods:**

* EncodedException  
  Gets or sets the encoded exception.
* Equals  
  Compares an exception with this ITriException for equality. Returns true if and only if both exceptions have the same encoded representation, false otherwise.
* SetEncodedException  
  Sets the encoded exception value of this ITriException together with the number of valid bits. The number of bits shall be less or equal to data.Length \* 8.
* NumberOfBits  
  Returns the amount of bits in the encoded exception.

#### 9.4.2.14 TriTimerIdType

**TriTimerIdType** is mapped to the following interface:

public interface ITriTimerId {  
 string TimerName { get; }  
 bool Equals(ITriTimerId timer);  
}

**Members:**

* TimerName  
  Returns the name of this timer identifier as defined in the TTCN-3 specification. In case of implicit timers the result is implementation dependent (see clause 4.1.2.4).
* Equals  
  Compares timer with this TriTimerId for equality. Returns true if and only if both timers identifiers represent the same timer, false otherwise.

#### 9.4.2.15 TriTimerDurationType

**TriTimerDurationType** is mapped to the following interface:

public interface ITriTimerDuration {  
 double Duration { get; set; }  
 bool Equals(ITriTimerDuration duration);  
}

**Members:**

* Duration  
  Gets or sets the duration of a timer.
* Equals  
  Compares duration with this TriTimerDuration for equality. Returns true if and only if both have the same duration, false otherwise.

#### 9.4.2.16 TriFunctionIdType

**TriFunctionIdType** C# mapping is derived from the IQualifiedName interface:

public interface ITriFunctionId : IQualifiedName {}

#### 9.4.2.17 TriTestCaseIdType

**TriTestCaseIdType** C# mapping is derived from the IQualifiedName interface:

public interface ITriTestCaseId : IQualifiedName {}

#### 9.4.2.18 TriStatusType

**TriStatusType** is mapped to the following enumeration:

public enum TriStatus {   
 TriOk = 0,   
 TriError = -1   
}

## 9.5 Mapping of interfaces

### 9.5.0 Basic rules

The TRI IDL definition defines two interfaces, the triCommunication and the triPlatform interface. As the operations are defined for different directions within this interface, i.e. some operations can only be called by the TTCN-3 Executable (TE) on the System Adaptor (SA) while others can only be called by the SA on the TE. This is reflected by dividing the TRI IDL interfaces in two sub interfaces, each suffixed by the called entity.

Table 6: TRI sub-interfaces

| Calling/Called | TE | SA | pA |
| --- | --- | --- | --- |
| TE | - | ITriCommunicationSA | ITriPlatformPA |
| SA | ITriCommunicationTE | - | - |
| PA | ITriPlatformTE | - | - |

All methods defined in these interfaces should behave as defined in clause 5.

### 9.5.1 Out and inout parameter passing mode

The following C# interfaces are used in out or inout parameter passing mode:

* ITriParameter
* ITriParameterList
* ITriBoolean
* ITriTimerDuration

In case they are used in out or inout parameter passing mode, instances of the respective interfaces will be passed with the method call. The called entity can then access methods and properties of the passed instances to set the return values.

### 9.5.2 triCommunication interface

#### 9.5.2.0 Introduction

The **triCommunication** interface is divided into two C# sub-interfaces, the ITriCommunicationSA interface, defining calls from the TE to the SA and the ITriCommunicationTE interface, defining calls from the SA to the TE.

#### 9.5.2.1 ITriCommunicationSA

The **ITriCommunicationSA** interface is defined as follows:

public interface ITriCommunicationSA {  
 // Reset operation  
 // Ref: TRI-Definition clause 5.5.1  
 TriStatus TriSAReset();  
 // Connection handling operations  
 // Ref: TRI-Definition clause 5.5.2.1  
 triStatus TriExecuteTestCase(iTriTestCaseId testCaseId,  
 ITriPortIdList portIdList);  
 // Ref: TRI-Definition clause 5.5.2.2  
 TriStatus TriMap(ITriPortId compPortId, ITriPortId tsiPortId);  
 // Ref: TRI-Definition clause 5.5.2.3  
 TriStatus TriMapparam(ITriPortId compPortId, ITriPortId tsiPortId,

ITriParameterList paramList);  
 // Ref: TRI-Definition clause 5.5.2.4  
 TriStatus TriUnmap(ITriPortId compPortId, ITriPortId tsiPortId);  
 // Ref: TRI-Definition clause 5.5.2.5  
 TriStatus TriUnmapparam(ITriPortId compPortId, ITriPortId tsiPortId,

ITriParameterList paramList);  
 // Ref: TRI-Definition clause 5.5.2.6  
 TriStatus TriEndTestCase();  
  
 // Message based communication operations  
 // Ref: TRI-Definition clause 5.5.3.1  
 TriStatus TriSend(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddress address, ITriMessage sentMessage);  
 // Ref: TRI-Definition clause 5.5.3.2  
 TriStatus TriSendBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriMessage sentMessage);  
 // Ref: TRI-Definition clause 5.5.3.3  
 TriStatus TriSendMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddressList addresses, ITriMessage sentMessage);  
  
 // Procedure based communication operations  
 // Ref: TRI-Definition clause 5.5.4.1  
 TriStatus TriCall(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddress sutAddress, ITriSignatureId signatureId,  
 ITriParameterList parameterList);  
 // Ref: TRI-Definition clause 5.5.4.2  
 TriStatus TriCallBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITriParameterList parameterList);  
 // Ref: TRI-Definition clause 5.5.4.3  
 TriStatus TriCallMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddressList sutAddresses, ITriSignatureId signatureId,  
 ITriParameterList parameterList);  
 // Ref: TRI-Definition clause 5.5.4.4  
 TriStatus TriReply(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddress sutAddress, ITriSignatureId signatureId,  
 ITriParameterList parameterList, ITriParameter returnValue);  
 // Ref: TRI-Definition clause 5.5.4.5  
 TriStatus TriReplyBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITriParameterList parameterList,  
 ITriParameter returnValue);  
 // Ref: TRI-Definition clause 5.5.4.6  
 TriStatus TriReplyMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddressList sutAddresses, ITriSignatureId signatureId,  
 ITriParameterList parameterList, ITriParameter returnValue);  
 // Ref: TRI-Definition clause 5.5.4.7  
 TriStatus TriRaise(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddress sutAddress, ITriSignatureId signatureId,  
 ITriException exc);  
 // Ref: TRI-Definition clause 5.5.4.8  
 TriStatus TriRaiseBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITriException exc);  
 // Ref: TRI-Definition clause 5.5.4.9  
 TriStatus TriRaiseMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriAddressList sutAddresses, ITriSignatureId signatureId,  
 ITriException exc);  
  
 // Miscellaneous operations  
 // Ref: TRI-Definition clause 5.5.5.1  
 TriStatus TriSutActionInformal(string description);  
 // Miscellaneous operations  
 // Ref: TRI-Definition clause 5.5.5.2  
 TriStatus TriSutActionParam(ITriParameterList parameterList);  
}

#### 9.5.2.2 ITriCommunicationTE

The **ITriCommunicationTE** interface is defined as follows:

public interface ITriCommunicationTE {  
 // Message based communication operations  
 // Ref: TRI-Definition clause 5.5.3.4  
 void EnqueueMessage(ITriPortId tsiPortId, ITriAddress sutAddress,  
 ITriComponentId componentId, ITriMessage msg);  
  
 // Procedure based communication operations  
 // Ref: TRI-Definition clause 5.5.4.10  
 void EnqueueCall(ITriPortId tsiPortId, ITriAddress sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 ITriParameterList parameterList);  
 // Ref: TRI-Definition clause 5.5.4.10  
 void EnqueueReply(ITriPortId tsiPortId, ITriAddress sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 ITriParameterList parameterList, ITriParameter returnValue);  
 // Ref: TRI-Definition clause 5.5.4.11  
 void EnqueueException(ITriPortId tsiPortId, ITriAddress sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 ITriException exc);  
 // Ref: TRI Definition clause 5.2.1

void TriSAErrorReq(string message);

}

#### 9.5.2.3 ITriPlatformPA

The **ITriPlatformPA** interface is defined as follows:

public interface ITriPlatformPA {  
 // Ref: TRI-Definition clause 5.6.1  
 TriStatus TriPAReset();  
  
 // Timer handling operations  
 // Ref: TRI-Definition clause 5.6.2.1  
 TriStatus TriStartTimer(ITriTimerId timerId, ITriTimerDuration duration);  
 // Ref: TRI-Definition clause 5.6.2.2  
 TriStatus TriStopTimer(ITriTimerId timerId);  
 // Ref: TRI-Definition clause 5.6.2.3  
 TriStatus TriReadtimer(ITriTimerId timerId,  
 ITriTimerDuration elapsedTime);  
 // Ref: TRI-Definition clause 5.6.2.4  
 TriStatus TriTimerrunning(ITriTimerId timerId, ITriBoolean running);  
  
 // Miscellaneous operations  
 // Ref: TRI-Definition clause 5.6.3.1  
 TriStatus TriExternalFunction(ItriFunctionId functionId,   
 ITriparameterList parameterList, ITriParameter returnValue);  
}

#### 9.5.2.4 ITriPlatformTE

The **ITriPlatformTE** interface is defined as follows:

public interface ITriPlatformTE {  
 // Ref: TRI-Definition clause 5.6.2.5  
 void TriTimeout(ITriTimerId timerId);  
 // Ref: TRI Definition clause 5.2.2

void TriPAErrorReq(string message);

// Ref: TRI Definition clause 5.6.3.2

ITriComponentId TriSelf();

// Ref: TRI Definition clause 5.6.3.3

ITriMessage TriRnd(ITriComponentId componentId, ITriMessage seed);

}

## 9.6 Optional parameters

Clause 5.4 defines that a reserved value shall be used to indicate the absence of an optional parameter. For the C# language mapping the distinct value null shall be used to indicate the absence of an optional value. For example if in the triSend operation the address parameter shall be omitted the operation invocation shall be TriSend(componentId, tsiPortId, null, sendMessage).

Annex A (normative):  
IDL Summary

This clause summarizes the IDL definition of TRI operations as defined in clause 5.

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Interface definition for the TTCN‑3 Runtime Interface

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

module triInterface

{

//

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Types

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

//

// Connection

native TriPortIdType;

typedef sequence<TriPortIdType> TriPortIdListType;

native TriComponentIdType;

typedef sequence<TriComponentIdType> TriComponentIdListType;

// Communication

native TriMessageType;

native TriAddressType;

typedef sequence<TriAddressType> TriAddressListType;

native TriSignatureIdType;

native TriParameterType;

typedef sequence<TriParameterType> TriParameterListType;

native TriExceptionType;

// Timing

native TriTimerIdType;

native TriTimerDurationType;

// Miscellaneous

native TriFunctionIdType;

native TriTestCaseIdType;

native TriStatusType;

//

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Interfaces

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

//

//

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// The communication interface (Ref: TRI‑Definition: clauses 5.5 and 5.2)

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

//

interface triCommunication

{

// Reset operation

// Ref: TRI‑Definition clause 5.5.1

TriStatusType triSAReset();

// Connection handling operations

// Ref: TRI‑Definition clause 5.5.2.1

TriStatusType triExecuteTestCase(in TriTestCaseIdType testCaseId,

in TriPortIdListType tsiPortList);

// Ref: TRI‑Definition clause 5.5.2.2

TriStatusType triMap(in TriPortIdType compPortId, in TriPortIdType tsiPortId);

// Ref: TRI‑Definition clause 5.5.2.3

TriStatusType triMapParam(in TriPortIdType compPortId, in TriPortIdType tsiPortId, in TriParameterListType paramList);

// Ref: TRI‑Definition clause 5.5.2.4

TriStatusType triUnmap(in TriPortIdType compPortId, in TriPortIdType tsiPortId);

// Ref: TRI‑Definition clause 5.5.2.5

TriStatusType triUnmapParam(in TriPortIdType compPortId, in TriPortIdType tsiPortId, in TriParameterListType paramList);

// Ref: TRI‑Definition clause 5.5.2.6

TriStatusType triEndTestCase();

// Message based communication operations

// Ref: TRI‑Definition clause 5.5.3.1

TriStatusType triSend(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressType SUTaddress, in TriMessageType sendMessage);

// Ref: TRI‑Definition clause 5.5.3.2

TriStatusType triSendBC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriMessageType sendMessage);

// Ref: TRI‑Definition clause 5.5.3.3

TriStatusType triSendMC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressListType SUTaddresses, in TriMessageType sendMessage);

// Ref: TRI‑Definition clause 5.5.3.4

void triEnqueueMsg(in TriPortIdType tsiPortId , in TriAddressType SUTaddress,

in TriComponentIdType componentId, in TriMessageType receivedMessage);

// Procedure based communication operations

// Ref: TRI‑Definition clause 5.5.4.1

TriStatusType triCall(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressType SUTaddress, in TriSignatureIdType signatureId,

in TriParameterListType parameterList);

// Ref: TRI‑Definition clause 5.5.4.2

TriStatusType triCallBC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriSignatureIdType signatureId,

in TriParameterListType parameterList);

// Ref: TRI‑Definition clause 5.5.4.3

TriStatusType triCallMC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressListType SUTaddresses, in TriSignatureIdType signatureId,

in TriParameterListType parameterList);

// Ref: TRI‑Definition clause 5.5.4.4

TriStatusType triReply(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressType SUTaddress, in TriSignatureIdType signatureId,

in TriParameterListType parameterList, in TriParameterType returnValue );

// Ref: TRI‑Definition clause 5.5.4.5

TriStatusType triReplyBC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriSignatureIdType signatureId,

in TriParameterListType parameterList, in TriParameterType returnValue );

// Ref: TRI‑Definition clause 5.5.4.6

TriStatusType triReplyMC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressListType SUTaddresses, in TriSignatureIdType signatureId,

in TriParameterListType parameterList, in TriParameterType returnValue );

// Ref: TRI‑Definition clause 5.5.4.7

TriStatusType triRaise(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressType SUTaddress, in TriSignatureIdType signatureId,

in TriExceptionType exc);

// Ref: TRI‑Definition clause 5.5.4.8

TriStatusType triRaiseBC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriSignatureIdType signatureId,

in TriExceptionType exc);

// Ref: TRI‑Definition clause 5.5.4.9

TriStatusType triRaiseMC(in TriComponentIdType componentId, in TriPortIdType tsiPortId,

in TriAddressListType SUTaddresses, in TriSignatureIdType signatureId,

in TriExceptionType exc);

// Ref: TRI‑Definition clause 5.5.4.10

void triEnqueueCall(in TriPortIdType tsiPortId, in TriAddressType SUTaddress,

in TriComponentIdType componentId, in TriSignatureIdType signatureId,

in TriParameterListType parameterList );

// Ref: TRI‑Definition clause 5.5.4.11

void triEnqueueReply(in TriPortIdType tsiPortId, in TriAddressType SUTaddress,

in TriComponentIdType componentId, in TriSignatureIdType signatureId,

in TriParameterListType parameterList, in TriParameterType returnValue );

// Ref: TRI‑Definition clause 5.5.4.12

void triEnqueueException(in TriPortIdType tsiPortId, in TriAddressType SUTaddress,

in TriComponentIdType componentId, in TriSignatureIdType signatureId,

in TriExceptionType exc);

// Miscellaneous operations

// Ref: TRI‑Definition clause 5.5.5.1

TriStatusType triSUTactionInformal(in string description);

// Ref: TRI‑Definition clause 5.5.5.2

TriStatusType triSUTactionParam(in TriParameterListType parameterList);

// Error Handling

// Ref: TRI Definition clause 5.2.1

void triSAErrorReq(in string message);

};

//

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// The platform interface (Ref: TRI‑Definition: clauses 5.6 and 5.2)

// \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

//

interface triPlatform

{

// Reset Operation

// Ref: TRI‑Definition clause 5.6.1

TriStatusType triPAReset();

// Timer handling operations

// Ref: TRI‑Definition clause 5.6.2.1

TriStatusType triStartTimer(in TriTimerIdType timerId,

in TriTimerDurationType timerDuration);

// Ref: TRI‑Definition clause 5.6.2.2

TriStatusType triStopTimer(in TriTimerIdType timerId);

// Ref: TRI‑Definition clause 5.6.2.3

TriStatusType triReadTimer(in TriTimerIdType timerId,

out TriTimerDurationType elapsedTime);

// Ref: TRI‑Definition clause 5.6.2.4

TriStatusType triTimerRunning(in TriTimerIdType timerId, out boolean running);

// Ref: TRI‑Definition clause 5.6.2.5

void triTimeout(in TriTimerIdType timerId);

// Miscellaneous operations

// Ref: TRI‑Definition clause 5.6.3.1

TriStatusType triExternalFunction(in TriFunctionIdType functionId,

inout TriParameterListType parameterList,

out TriParameterType returnValue);

// Ref: TRI‑Definition clause 5.6.3.2

TriComponentIdType triSelf();

// Ref: TRI‑Definition clause 5.6.3.3

TriMessage triRnd(in TriComponentIdType componentId,

in TriMessage seed);

// Error Handling

// Ref: TRI Definition clause 5.2.2

void triPAErrorReq(in string message);

};

};

Annex B (informative):  
Use scenarios

# B.0 Introduction

This annex contains use scenarios that should help users of the TRI and tool vendors providing the TRI understand the semantics of the operations defined within the present document.

Three scenarios are defined in terms of Message Sequence Charts (MSC). A scenario consists of a TTCN‑3 code fragment that uses TTCN‑3 communication functions to the SUT as well as timer handling functions. The MSC shows the interactions between the TE, SA and PA entities together with the SUT.

Please note that the TTCN‑3 fragments are not complete, as the main objective of the fragments is the usage of dynamic behaviour. All of the presented scenarios use a common preamble sequence of TRI operations shown in figure B.1.

Notice that the MSCs presented in this clause use message pairs to model each TRI operation. The MSC message triMap followed by triMapOK denotes, for example, that the TRI operation triMap has been invoked by the TE and it returns successfully from the SA. TRI operation calls are shown using abstract types and values, and are intended to serve only for illustration purposes. The concrete representation of these parameters in a particular target language is defined in the respective language mappings.



Figure B.1: Common MSC Preamble

# B.1 First scenario

## B.1.0 Use case

The first scenario shows some TTCN‑3 timer operations, i.e. start and timer running, message based communication operations, i.e. send and receive, as well as connection handling operations, i.e. map and unmap.

## B.1.1 TTCN‑3 fragment

module triScenario1

{

external function MyFunction();

type port PortTypeMsg message { inout integer }

type component MyComponent {

port PortTypeMsg MyPort;

timer MyTimer

}

type component MyTSI {

port PortTypeMsg PCO1;

}

testcase scenario1() runs on MyComponent system MyTSI

{

MyPort.clear;

MyPort.start;

MyTimer.start(2);

map(MyComponent: MyPort, system: PCO1);

MyPort.send (integer : 5);

if (MyTimer.running)

{

MyPort.receive(integer:7);

}

else

{

MyFunction();

}

unmap(MyComponent: MyPort, system:PCO1);

MyPort.stop;

}

control {

execute( scenario1() );

}

}

## B.1.2 Message sequence chart



Figure B.2: Use Scenario 1

# B.2 Second scenario

## B.2.0 Use case

The second example shows a similar scenario which also uses timed procedure based communication operations which are initiated by the test component MyComponent. In this example MyComponent is assumed to run as the MTC.

## B.2.1 TTCN‑3 fragment

module triScenario2

{

signature MyProc ( in float par1, inout float par2)

exception(MyExceptionType);

type record MyExceptionType { FieldType1 par1, FieldType2 par2 }

type port PortTypeProc procedure { out MyProc }

type component MyComponent {

port PortTypeProc MyPort;

timer MyTimer = 7

}

testcase scenario2() runs on MyComponent

{

var float MyVar;

MyPort.clear;

MyPort.start;

MyTimer.start;

MyVar := MyTimer.read;

if (MyVar>5.0) {

MyPort.call (MyProc:{MyVar, 5.7}, 5);

alt {

[] MyPort.getreply(MyProc:{‑,MyVar\*5}) {}

[] MyPort.catch (MyProc, MyExceptionType:\* ) {}

[] MyPort.catch (timeout) {}

}

}

MyTimer.stop;

MyPort.stop;

}

control {

execute( scenario2() );

}

}

## B.2.2 Message sequence chart



Figure B.3: Use Scenario 2

# B.3 Third scenario

## B.3.0 Use case

Use scenario 3 shows the reception of a procedure call as well as a reply and raising of an exception based on this received call. Again MyComponent is assumed to run as the MTC. FieldType1, FieldType2, p1, and p2 are assumed to be defined elsewhere.

## B.3.1 TTCN‑3 fragment

module triScenario3

{

signature MyProc ( in float par1, inout float par2)

exception(MyExceptionType);

type record MyExceptionType { FieldType1 par1, FieldType2 par2 }

type port PortTypeProc procedure { in MyProc }

type component MyComponent {

port PortTypeProc MyPort;

timer MyTimer = 3

}

testcase scenario3(integer x) runs on MyComponent

{

MyPort.start;

MyTimer.start;

alt

{

[] MyPort.getcall(MyProc:{5.0, 6.0})

{

MyTimer.stop;

}

[x>5] MyTimer.timeout

{

MyPort.reply(MyProc:{‑, 30.0});

}

[x<=5] MyTimer.timeout

{

MyPort.raise(MyProc, MyExceptionType:{p1, p2} );

}

}

MyPort.stop;

}

control {

execute( scenario3(4) );

}

}

## B.3.2 Message sequence chart



Figure B.4: Use Scenario 3

Annex C (informative):  
Bibliography

* INTOOL CGI/NPL038 (V2.2): "Generic Compiler/Interpreter interface; GCI Interface Specification", Infrastructural Tools, December 1996.

# History

|  |  |  |
| --- | --- | --- |
| **Document history** | | |
| V1.1.1 | February 2003 | Publication |
| V3.1.1 | June 2005 | Publication |
| V3.2.1 | February 2007 | Publication |
| V3.3.1 | April 2008 | Publication |
| V4.1.1 | June 2009 | Publication |
| V4.2.1 | July 2010 | Publication |
| V4.3.1 | June 2011 | Publication |
| V4.4.1 | April 2012 | Publication |
| V4.5.1 | April 2013 | Publication |
| V4.6.1 | June 2014 | Publication |
| V4.7.1 | June 2015 | Publication |
| V4.8.1 | March 2017 | Membership Approval Procedure MV 20170509: 2017-03-10 to 2017-05-09 |
| V4.8.1 | May 2017 | Publication |