/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.3, multidimensional index redirect in any from port.trigger statement
 ** @verdict  pass accept, ttcn3verdict:pass
 *****************************************************************/

// The following requirements are tested:
// It is also possible to store the index of a port in a single-dimensional port array
// at which the operation was successful to a variable of type integer or, in case of
// multi-dimensional port arrays the index of the successful port to an integer array
// or record of integer variable. When checking the port array for matching messages,
// the port indices to be checked are iterated from lowest to highest. If the port
// array is multi-dimensional, then the ports are iterated over from innermost to
// outermost array dimension from lowest to highest index for each dimension, e.g.
// [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will
// cause the operation to be successful even if other ports in the array would also
// meet the criteria.

module Sem_220203_TriggerOperation_021 {

	type port P message {
		inout integer;
	}

    type component GeneralComp
	{
		port P p [2][3];
        port P altP;
	}

    type record of integer RoI;

    testcase TC_Sem_220203_TriggerOperation_021() runs on GeneralComp {
        var RoI v_index;
        p[0][2].send(10);
        altP.send(1);
        alt {
            [] any from p.trigger(integer:?) -> @index value v_index {
                if (v_index == { 0, 2 }) { setverdict(pass); }
                else { setverdict(fail, "v_index: ", v_index); }
            }
            [] any port.receive { setverdict(fail); }
        }
    }

    control {
        execute(TC_Sem_220203_TriggerOperation_021(), 5.0);
    }
}