/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.2, redirect assignment of message fields
 ** @verdict  pass accept, ttcn3verdict:pass
 *****************************************************************/

// The following requirements are tested:
// As a special case the field reference can be absent to indicate that the whole
// message shall be stored in a variable.

module Sem_220202_ReceiveOperation_010 {
	type record R
    {
        integer field1[2],
        charstring field2
    }

	type port P message {
		inout R;
	}

    type component GeneralComp
	{
		port P p;
	}

    testcase TC_Sem_220202_ReceiveOperation_010() runs on GeneralComp {
        var integer v_int;
        var charstring v_str;
        var R v_rec;
        p.send(R:{ field1 := { 1, 2 }, field2 := "abc" });
        alt {
            [] p.receive(R:?) -> value ( v_int := field1[1], v_rec, v_str := field2) {
                if (v_int == 2 and v_str == "abc" and v_rec == { field1 := { 1, 2 }, field2 := "abc" }) { setverdict (pass); }
                else { setverdict(fail); }
            }
            [] p.receive { setverdict(fail); }
        }
    }

    control {
        execute(TC_Sem_220202_ReceiveOperation_010(), 5.0);
    }
}