/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.2, insufficient element value range of variable in index redirection
 ** @verdict  pass reject
 *****************************************************************/

// The following requirements are tested:
// If the index redirection is used for multi-dimensional port arrays, the size of the
// integer array or record of integer type shall exactly be the same as the dimension of
// the respective array, and its type shall allow storing the highest index (from all
// dimensions) of the array.

module NegSem_220202_ReceiveOperation_021 {
	type integer RestrInt(0..2);
    type port P message {
		inout integer;
	}

    type component GeneralComp {
		port P p[4][2][3];
	}

    testcase TC_NegSem_220202_ReceiveOperation_021() runs on GeneralComp {
        var RestrInt v_indices[3];
        p[3][1][2].send(100);
        any from p.receive(integer:?) -> @index value v_indices;
        setverdict(pass);
    }

    control {
        execute(TC_NegSem_220202_ReceiveOperation_021(), 5.0);
    }
}