/***************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:20.5.2, control block timer as a parameter of activated altstep
 ** @verdict  pass accept, ttcn3verdict:pass
 ***************************************************/

// The following requirement is tested:
// For altsteps activated in module control or in functions or altsteps invoked
// directly or indirectly from module control, all timer instances in the actual
// parameter list shall be declared in the highest scope of the module control
// part (see clause 26.2). Timers from lower scopes of the module control part
// (i.e. from the nested statement blocks) are not allowed to occur in the actual
// parameter list.

module Sem_200502_the_activate_operation_005 {

	type port P message {
		inout integer;
	}

	type component GeneralComp {
		port P p;
	}

	altstep a(timer t_tmr) {
		[] t_tmr.timeout { log ("Timeout in default"); }
	}

	testcase TC_Sem_200502_the_activate_operation_005() runs on GeneralComp {
        setverdict(pass);
	}

	control{
        timer t_tmr := 1.0, t_tmr2;
        t_tmr.start;
        activate(a(t_tmr));
        alt {
            [] t_tmr2.timeout { }
        }
		execute(TC_Sem_200502_the_activate_operation_005());
	}
}
