/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.3, trying to store address with trigger operation on connected port
 ** @verdict  pass reject
 *****************************************************************/

// The following requirements are tested:
// Type mismatch at storing the received value or parts of the received value and storing
// the sender shall cause an error.

module NegSem_220203_TriggerOperation_013 {

	type port P message {
		inout integer;
        address integer;
	}

    type component GeneralComp
	{
		port P p;
	}

    testcase TC_NegSem_220203_TriggerOperation_013() runs on GeneralComp system GeneralComp {
        var P.address v_addr;
        connect(self:p, self:p);
        p.send(10);
        p.trigger -> sender v_addr;
        setverdict(pass);
    }

    control {
        execute(TC_NegSem_220203_TriggerOperation_013(), 5.0);
    }
}