/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.2, fuzzy variable in sender redirect
 ** @verdict  pass accept, ttcn3verdict:pass
 *****************************************************************/

// The following requirements are tested:
// If a variable referenced in the value, sender or @index clause is a lazy or fuzzy
// variable, the expression assigned to this variable is equal to the result produced
// by the receive operation i.e. later evaluation of the lazy or fuzzy variable does not
// lead to repeated invocation of the receive operation.

module Sem_220202_ReceiveOperation_028 {
    type integer address;

	type port P message {
		inout integer;
	}

    type component GeneralComp {
		port P p;
	}

    testcase TC_Sem_220202_ReceiveOperation_028() runs on GeneralComp {
        var @fuzzy address v_addr;
        p.send(1) to 1;
        p.send(2) to 2;
        p.send(3) to 3;
        p.receive(integer:?) -> sender v_addr;
        if (v_addr == 1) { // evaluation of @lazy (receive shall not be called again)
            alt {
                [] p.receive(integer:2) { setverdict(pass); }
                [] p.receive { setverdict(fail); }
            }
        } else {
            setverdict(fail);
        }
    }

    control {
        execute(TC_Sem_220202_ReceiveOperation_028(), 5.0);
    }
}