ETSI ES 202 789 V1.5.2 (2021-12)

Methods for Testing and Specification (MTS);

The Testing and Test Control Notation version 3;

TTCN-3 Language Extensions: Extended TRI

**ETSI Standard**

Reference

RES/MTS-202789ed151

Keywords

interface, testing, TTCN-3

***ETSI***

650 Route des Lucioles

F-06921 Sophia Antipolis Cedex - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Siret N° 348 623 562 00017 - NAF 742 C

Association à but non lucratif enregistrée à la

Sous-Préfecture de Grasse (06) N° 7803/88

***Important notice***

The present document can be downloaded from:  
<http://www.etsi.org/standards-search>

The present document may be made available in electronic versions and/or in print. The content of any electronic and/or print versions of the present document shall not be modified without the prior written authorization of ETSI. In case of any existing or perceived difference in contents between such versions and/or in print, the prevailing version of an ETSI deliverable is the one made publicly available in PDF format at [www.etsi.org/deliver](http://www.etsi.org/deliver).

Users of the present document should be aware that the document may be subject to revision or change of status. Information on the current status of this and other ETSI documents is available at <https://portal.etsi.org/TB/ETSIDeliverableStatus.aspx>

If you find errors in the present document, please send your comment to one of the following services:  
<https://portal.etsi.org/People/CommiteeSupportStaff.aspx>

***Copyright Notification***

No part may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm except as authorized by written permission of ETSI.  
The content of the PDF version shall not be modified without the written authorization of ETSI.  
The copyright and the foregoing restriction extend to reproduction in all media.

© ETSI 2020.

All rights reserved.

**DECT™**, **PLUGTESTS™**, **UMTS™** and the ETSI logo are trademarks of ETSI registered for the benefit of its Members.  
**3GPP™**and **LTE™** are trademarks of ETSI registered for the benefit of its Members and  
of the 3GPP Organizational Partners.  
**oneM2M™** logo is a trademark of ETSI registered for the benefit of its Members and  
of the oneM2M Partners.  
**GSM®** and the GSM logo are trademarks registered and owned by the GSM Association.

Contents

Intellectual Property Rights 4

Foreword 4

Modal verbs terminology 4

1 Scope 5

2 References 5

2.1 Normative references 5

2.2 Informative references 6

3 Definition of terms, symbols and abbreviations 6

3.1 Terms 6

3.2 Symbols 6

3.3 Abbreviations 7

4 Package conformance and compatibility 7

5 Package concepts for the core language 7

6 Package semantics 7

7 TRI extensions for the package 8

7.0 Introduction 8

7.1 Changes to clause 5.2 of ETSI ES 201 873-5, Error handling 8

7.2 Changes to clause 5.5.2 of ETSI ES 201 873-5, Connection handling operations 9

7.3 Changes to clause 5.5.3 of ETSI ES 201 873-5, Message based communication operations 9

7.4 Addition to clause 5.5.3 of ETSI ES 201 873-5, Message based communication operations 11

7.5 Changes to clause 5.5.4 of ETSI ES 201 873-5, Procedure based communication operations 11

7.5A Changes to clause 5.5.5 of ETSI ES 201 873-5, Miscellaneous operations 17

7.5B Addition to clause 5.5.5 of ETSI ES 201 873-5, Miscellaneous operations 18

7.6 Changes to clause 5.6.3 of ETSI ES 201 873-5, Miscellaneous operations 18

7.7 Changes to clause 6 of ETSI ES 201 873-5, Java language mapping 19

7.8 Changes to clause 7 of ETSI ES 201 873-5, C language mapping 22

7.9 Changes to clause 8 of ETSI ES 201 873-5, C++ language mapping 24

7.10 Changes to clause 9 of ETSI ES 201 873-5, C# language mapping 27

8 TCI extensions for the package 28

Annex A (informative): Bibliography 29

History 30

# Intellectual Property Rights

Essential patents

IPRs essential or potentially essential to normative deliverables may have been declared to ETSI. The information pertaining to these essential IPRs, if any, is publicly available for **ETSI members and non-members**, and can be found in ETSI SR 000 314: *"Intellectual Property Rights (IPRs); Essential, or potentially Essential, IPRs notified to ETSI in respect of ETSI standards"*, which is available from the ETSI Secretariat. Latest updates are available on the ETSI Web server (<https://ipr.etsi.org/>).

Pursuant to the ETSI IPR Policy, no investigation, including IPR searches, has been carried out by ETSI. No guarantee can be given as to the existence of other IPRs not referenced in ETSI SR 000 314 (or the updates on the ETSI Web server) which are, or may be, or may become, essential to the present document.

Trademarks

The present document may include trademarks and/or tradenames which are asserted and/or registered by their owners. ETSI claims no ownership of these except for any which are indicated as being the property of ETSI, and conveys no right to use or reproduce any trademark and/or tradename. Mention of those trademarks in the present document does not constitute an endorsement by ETSI of products, services or organizations associated with those trademarks.

# Foreword

This ETSI Standard (ES) has been produced by ETSI Technical Committee Methods for Testing and Specification (MTS).

**The use of strike through (deleted text) highlights the differences between base document and extended documents.**

The present document relates to the multi-part standard ETSI ES 201 873 covering the Testing and Test Control Notation version 3, as identified in ETSI ES 201 873-1 [1].

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the [ETSI Drafting Rules](https://portal.etsi.org/Services/editHelp!/Howtostart/ETSIDraftingRules.aspx) (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in ETSI deliverables except when used in direct citation.

# 1 Scope

The present document defines the Extended TRI package of TTCN‑3. TTCN‑3 can be used for the specification of all types of reactive system tests over a variety of communication ports. Typical areas of application are protocol testing (including mobile and Internet protocols), service testing (including supplementary services), module testing, testing of CORBA based platforms, APIs, etc. TTCN‑3 is not restricted to conformance testing and can be used for many other kinds of testing including interoperability, robustness, regression, system and integration testing. The specification of test suites for physical layer protocols is outside the scope of the present document.

TTCN‑3 packages are intended to define additional TTCN-3 concepts, which are not mandatory as concepts in the TTCN-3 core language or in its interfaces TRI and TCI, but which are optional as part of a package which is suited for dedicated applications and/or usages of TTCN-3.

This package defines a more efficient handling of software values by a version of TRI, that does not use binary encoded messages for the communication with the SUT, but uses the values as they are; meaning e.g. that software objects or serialized data can be passed directly between the SUT and the TE.

While the design of TTCN‑3 package has taken into account the consistency of a combined usage of the core language with a number of packages, the concrete usages of and guidelines for this package in combination with other packages is outside the scope of the present document.

# 2 References

## 2.1 Normative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

Referenced documents which are not found to be publicly available in the expected location might be found at <https://docbox.etsi.org/Reference>.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are necessary for the application of the present document.

[1] ETSI ES 201 873-1: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN-3 Core Language".

[2] ETSI ES 201 873-4: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 4: TTCN-3 Operational Semantics".

[3] ETSI ES 201 873-5: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 5: TTCN-3 Runtime Interface (TRI)".

[4] ETSI ES 201 873-6: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 6: TTCN-3 Control Interface (TCI)".

[5] Recommendation ITU-T X.290: "OSI conformance testing methodology and framework for protocol Recommendations for ITU-T applications - General concepts".

NOTE: The corresponding ISO/IEC standard is ISO/IEC 9646-1: "Information technology -- Open Systems Interconnection -- Conformance testing methodology and framework -- Part 1: General concepts".

## 2.2 Informative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, ETSI cannot guarantee their long term validity.

The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.

[i.1] Void.

[i.2] Void.

[i.3] ETSI ES 201 873-7: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 7: Using ASN.1 with TTCN-3".

[i.4] ETSI ES 201 873-8: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 8: The IDL to TTCN-3 Mapping".

[i.5] ETSI ES 201 873-9: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 9: Using XML schema with TTCN-3".

[i.6] ETSI ES 201 873-10: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 10: TTCN-3 Documentation Comment Specification".

[i.7] ETSI ES 202 781: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Configuration and Deployment Support".

[i.8] ETSI ES 202 784: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Advanced Parameterization".

[i.9] ETSI ES 202 785: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Behaviour Types".

[i.10] ETSI ES 202 782: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: TTCN-3 Performance and Real Time Testing".

[i.11] ETSI ES 202 786: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Support of interfaces with continuous signals".

# 3 Definition of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in ETSI ES 201 873-1 [1], ETSI ES 201 873‑4 [2], ETSI ES 201 873-5 [3], ETSI ES 201 873-6 [4] and Recommendation ITU-T X.290 [5] apply.

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in ETSI ES 201 873-1 [1], ETSI ES 201 873‑4 [2], ETSI ES 201 873-5 [3], ETSI ES 201 873-6 [4], Recommendation ITU-T X.290 [5] and the following apply:

XTRI eXtended TRI

# 4 Package conformance and compatibility

The package has no package tag as the choice to use TRI and/or XTRI affects the test adaptor only, but not the test specifications in TTCN-3.

For an implementation claiming to conform to this package version, all features specified in the present document shall be implemented consistently with the requirements given in the present document, ETSI ES 201 873-1 [1] and ETSI ES 201 873-4 [2].

The package presented in the present document is compatible to:

ETSI ES 201 873-1 [1] (V4.5.1)

ETSI ES 201 873-4 [2] (V4.4.1)

ETSI ES 201 873-6 [4] (V4.5.1)

ETSI ES 201 873-7 [i.3] (V4.5.1)

ETSI ES 201 873-8 [i.4] (V4.5.1)

ETSI ES 201 873-9 [i.5] (V4.5.1)

ETSI ES 201 873-10 [i.6] (V4.5.1)

If later versions of those parts are available and should be used instead, the compatibility of the package defined in the present document has to be checked individually.

The package defined in the present document is also compatible to:

ETSI ES 202 784 [i.8] (V1.3.1)

ETSI ES 202 781 [i.7] (V1.2.1)

ETSI ES 202 782 [i.10] (V1.2.1)

ETSI ES 202 785 [i.9] (V1.3.1)

ETSI ES 202 786 [i.11] (V1.2.1)

and can be used together with those packages.

If later versions of those packages are available and should be used instead, the compatibility to the package defined in the present document has to be checked individually.

# 5 Package concepts for the core language

Not applicable.

# 6 Package semantics

Not applicable.

# 7 TRI extensions for the package

## 7.0 Introduction

Historically, TTCN has been used to test communication protocols which typically use encoded messages. This has been reflected in the TRI SA and TCI CD design of TTCN-3 by encoding and decoding messages to and from bitstrings. However, TTCN-3 also supports signature-based communication for which the transformation of objects into bitstrings and vice versa is cumbersome. Furthermore, some protocols use also structured messages for which the bitstring encoding is not helpful.

Therefore, an alternative API is being defined in this extension package of TTCN-3 along which TTCN-3 values can be directly passed to/from the SUT. It is defined by redefining the operations in TRI SA and PA as follows.

## 7.1 Changes to clause 5.2 of ETSI ES 201 873-5, Error handling

The SA or PA can in addition provide notifications about unrecoverable error situations by use of the operations xtriSAErrorReq and xtriPAErrorReq, respectively.

5.2.1 triSAErrorReq 🡪 xtriSAErrorReq

|  |  |
| --- | --- |
| **Signature** | void xtriSAErrorReq(in string message, in any cause) |
| **In Parameters** | message A string value, i.e. the error phrase describing the problem.  cause (Optional) cause of the problem. |
| **Return Value** | void |
| **Constraint** | Shall be called whenever an error situation has occurred in the SA with the exception of errors occurring when processing SA calls initiated by the TE. These errors are reported in the operation return. The optional cause parameter can be used to provide information in addition to the error phrase in message. |
| **Effect** | The TE will be notified about an unrecoverable error situation within the SA and may forward the error indication to the test management. |

5.2.2 triPAErrorReq 🡪 xtriPAErrorReq

|  |  |
| --- | --- |
| **Signature** | void xtriPAErrorReq(in string message, in any cause) |
| **In Parameters** | message A string value, i.e. the error phrase describing the problem.  cause (Optional) cause of the problem. |
| **Return Value** | Void |
| **Constraint** | Shall be called whenever an error situation has occurred in the PA with the exception of errors occurring when processing PA calls initiated by the TE. These errors are reported in the operation return. The optional cause parameter can be used to provide information in addition to the error phrase in message. |
| **Effect** | The TE will be notified about an unrecoverable error situation within the PA and may forward the error indication to the test management. |

## 7.2 Changes to clause 5.5.2 of ETSI ES 201 873-5, Connection handling operations

5.5.2.3 triMapParam 🡪 xtriMapParam

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriMap(in TriPortIdType compPortId,  in TriPortIdType tsiPortId,  in TciParameterListType paramList) |
| **In Parameters** | compPortId identifier of the test component port to be mapped tsiPortId identifier of the test system interface port to be mapped  paramList parameters of the parameterized map |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triMap operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 map operation. |
| **Effect** | The SA can establish a dynamic connection to the SUT for the referenced TSI port. The triMap operation returns ***TRI\_Error*** in case a connection could not be established successfully, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connection needs to be established by the test system. |

5.5.2.5 triUnmapParam 🡪 xtriUnmapParam

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriUnmap(in TriPortIdType compPortId, in TriPortIdType tsiPortId, in TciParameterListType paramList) |
| **In Parameters** | compPortId identifier of the test component port to be unmapped tsiPortId identifier of the test system interface port to be unmapped  paramList parameters of the parameterized map |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triUnmap operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes any TTCN‑3 unmap operation. |
| **Effect** | The SA shall close a dynamic connection to the SUT for the referenced TSI port.  The triUnmap operation returns ***TRI\_Error*** in case a connection could not be closed successfully or no such connection has been established previously, ***TRI\_OK*** otherwise. The operation should return ***TRI\_OK*** in case no dynamic connections have to be closed by the test system. |

## 7.3 Changes to clause 5.5.3 of ETSI ES 201 873-5, Message based communication operations

5.5.3.1 triSend 🡪 xtriSend

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriSend(in TriComponentIdType componentId, in TriPortIdType tsiPortId, in Value SUTaddress, in Value sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  SUTaddress (optional) destination address value within the SUT  sendMessage the value to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSend operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | The SA can send the message to the SUT.  The triSend operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

5.5.3.2 triSendBC 🡪 xtriSendBC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriSendBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in Value sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  sendMessage the value to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSendBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | The SA can broadcast the message to the SUT.  The triSendBC operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

5.5.3.3 triSendMC 🡪 xtriSendMC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriSendMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TciValueList SUTaddresses, in Value sendMessage) |
| **In Parameters** | componentId identifier of the sending test component  tsiPortId identifier of the test system interface port via which the message is sent to the SUT Adaptor  SUTaddresses destination address values within the SUT  sendMessage the values to be sent |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triSendMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast send operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 send operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | The SA can multicast the message to the SUT.  The triSendMC operation returns ***TRI\_OK*** in case it has been completed successfully. Otherwise ***TRI\_Error*** shall be returned. Notice that the return value ***TRI\_OK*** does not imply that the SUT has received sendMessage. |

5.5.3.4 triEnqueueMsg 🡪 xtriEnqueueMsg

|  |  |
| --- | --- |
| **Signature** | void xtriEnqueueMsg(in TriPortIdType tsiPortId, in any SUTaddress, in TriComponentIdType componentId, in any receivedMessage) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the message is enqueued by the SUT Adaptor  SUTaddress (optional) source address value within the SUT  componentId identifier of the receiving test component  receivedMessage the received value |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation is called by the SA after it has received a message from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or has been referenced in the previous triExecuteTestCase statement. |
| **Effect** | This operation shall pass the message to the TE indicating the component componentId to which the TSI port tsiPortId is mapped.  The decoding of receivedMessage has to be done in the TE. |

## 7.4 Addition to clause 5.5.3 of ETSI ES 201 873-5, Message based communication operations

In order to interpret unknown values along a type hypothesis, an additional xtriConvert operation is defined. It can be used in all cases where the type of the incoming value is not known. Please note that typically the value type is known in procedure-based communication and sometimes in message-based communication.

5.5.3.5 xtriConvert

|  |  |
| --- | --- |
| **Signature** | Value xtriConvert(in any value, in Type typeHypothesis) |
| **In Parameters** | value the value to be converted  typeHypothesis the type hypothesis |
| **Out Parameters** | n.a. |
| **Return Value** | Returns the converted value, if the value is of a compatible type as the typeHypothesis, else the distinct value null. |
| **Constraints** | This operation shall be called whenever the TE has to convert a value. The TE might convert immediately after reception of the value, or might for performance considerations postpone the conversion until the actual access to the value. |
| **Effect** | This operation converts a value and returns a value according to the type hypothesis if it matches. The typeHypothesis determines whether the value can be converted. If not, the distinct null value shall be returned. |

## 7.5 Changes to clause 5.5.4 of ETSI ES 201 873-5, Procedure based communication operations

5.5.4.1 triCall 🡪 xtriCall

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriCall(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in Value SUTaddress, in TriSignatureIdType signatureId, in TciParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCall operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.The procedure parameters are the parameters specified in the TTCN‑3 signature template. |
| **Effect** | On invocation of this operation the SA can initiate the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCall operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCall operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

5.5.4.2 triCallBC 🡪 xtriCallBC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriCallBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriSignatureIdType signatureId, in TciParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCallBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. The procedure parameters are the parameters specified in the TTCN‑3 signature template. |
| **Effect** | On invocation of this operation the SA can initiate and broadcast the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCallBC operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCallBC operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

5.5.4.3 triCallMC 🡪 xtriCallMC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriCallMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TciValueList SUTaddresses, in TriSignatureIdType signatureId, in TciParameterListType parameterList) |
| **In Parameters** | componentId identifier of the test component issuing the procedure call  tsiPortId identifier of the test system interface port via which the procedure call is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triCallMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast call operation on a component port, which has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 call operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case.The procedure parameters are the parameters specified in the TTCN‑3 signature template. |
| **Effect** | On invocation of this operation the SA can initiate and multicast the procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triCallMC operation shall return without waiting for the return of the issued procedure call (see note). This TRI operation returns *TRI\_OK* on successful initiation of the procedure call, *TRI\_Error* otherwise. No error shall be indicated by the SA in case the value of any *out* parameter is non‑null. Notice that the return value of this TRI operation does not make any statement about the success or failure of the procedure call. Note that an optional timeout value, which can be specified in the TTCN‑3 ATS for a call operation, is *not* included in the triCallMC operation signature. The TE is responsible to address this issue by starting a timer for the TTCN‑3 call operation in the PA with a separate TRI operation call, i.e. triStartTimer. |
| NOTE: This might be achieved for example by spawning a new thread or process. This handling of this procedure call is, however, dependent on implementation of the TE. | |

5.5.4.4 triReply 🡪 xtriReply

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriReply(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in Value SUTaddress, in TriSignatureIdType signatureId, in TciParameterListType parameterList, in Value returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReply operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can issue the reply to a procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReply operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

5.5.4.5 triReplyBC 🡪 xtriReplyBC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriReplyBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriSignatureIdType signatureId, in TciParameterListType parameterList, in Value returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReplyBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can broadcast the reply to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReplyBC operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

5.5.4.6 triReplyMC 🡪 xtriReplyMC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriReplyMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TciValueList SUTaddresses, in TriSignatureIdType signatureId, in TciParameterListType parameterList, in Value returnValue) |
| **In Parameters** | componentId identifier of the replying test component  tsiPortId identifier of the test system interface port via which the reply is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triReplyMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast reply operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 reply operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. The parameterList contains procedure call parameters. These parameters are the parameters specified in the TTCN‑3 signature template.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be passed for the return value. |
| **Effect** | On invocation of this operation the SA can multicast the reply to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId. The triReplyMC operation will return ***TRI\_OK*** on successful execution of this operation, ***TRI\_Error*** otherwise. The SA shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

5.5.4.7 triRaise 🡪 xtriRaise

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriRaise(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in Value SUTaddress, in TriSignatureIdType signatureId, in Value exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  SUTaddress (optional) destination address within the SUT  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaise operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 unicast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | On invocation of this operation the SA can raise an exception to a procedure call corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaise operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

5.5.4.8 triRaiseBC 🡪 xtriRaiseBC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriRaiseBC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TriSignatureIdType signatureId, in Value exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaiseBC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 broadcast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | On invocation of this operation the SA can raise and broadcast an exception to procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaiseBC operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

5.5.4.9 triRaiseMC 🡪 xtriRaiseMC

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriRaiseMC(in TriComponentIdType componentId,  in TriPortIdType tsiPortId, in TciValueList SUTaddresses, in TriSignatureIdType signatureId, in Value exc) |
| **In Parameters** | componentId identifier of the test component raising the exception  tsiPortId identifier of the test system interface port via which the exception is sent to the SUT Adaptor  SUTaddresses destination addresses within the SUT  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the exception |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the triRaiseMC operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 multicast raise operation on a component port that has been mapped to a TSI port. This operation is called by the TE for all TTCN‑3 raise operations if no system component has been specified for a test case, i.e. only a MTC test component is created for a test case. |
| **Effect** | On invocation of this operation the SA can raise and multicast an exception to a procedure calls corresponding to the signature identifier signatureId and the TSI port tsiPortId.  The triRaiseMC operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. |

5.5.4.10 triEnqueueCall 🡪 xtriEnqueueCall

|  |  |
| --- | --- |
| **Signature** | void xtriEnqueueCall(in TriPortIdType tsiPortId,  in any SUTaddress, in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TciParameterListType parameterList) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the procedure call is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration. Description of data passed as parameters to the operation from the calling entity to the called entity |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a procedure call from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement. |
| **Effect** | The TE can enqueue this procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped. The decoding of procedure parameters has to be done in the TE.  The TE shall indicate no error in case the value of any *out* parameter is different from null. |

5.5.4.11 triEnqueueReply 🡪 xtriEnqueueReply

|  |  |
| --- | --- |
| **Signature** | void xtriEnqueueReply(in TriPortIdType tsiPortId,  in any SUTaddress, in TriComponentIdType componentId,  in TriSignatureIdType signatureId,  in TciParameterListType parameterList, in Value returnValue) |
| **In Parameters** | tsiPortId identifier of the test system interface port via which the reply is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call  parameterList a list of parameters which are part of the indicated signature. The parameters in parameterList are ordered as they appear in the TTCN‑3 signature declaration  returnValue (optional) return value of the procedure call |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a reply from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement.  If no return type has been defined for the procedure signature in the TTCN‑3 ATS, the distinct value null shall be used for the return value. |
| **Effect** | The TE can enqueue this reply to the procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped. The decoding of the procedure parameters has to be done within the TE. The TE shall indicate no error in case the value of any *in* parameter or an undefined return value is different from null. |

5.5.4.12 triEnqueueException 🡪 xtriEnqueueException

|  |  |
| --- | --- |
| **Signature** | void xtriEnqueueException(in TriPortIdType tsiPortId,  in any SUTaddress,  in TriComponentIdType componentId, in TriSignatureIdType signatureId,  in any exc) |
| **In Parameters** | tsiPortId identifier for the test system interface port via which the exception is enqueued by the SUT Adaptor  SUTaddress (optional) source address within the SUT  componentId identifier of the receiving test component  signatureId identifier of the signature of the procedure call which the exception is associated with  exc the exception |
| **Out Parameters** | n.a. |
| **Return Value** | void |
| **Constraints** | This operation can be called by the SA after it has received a reply from the SUT. It can only be used when tsiPortId has been either previously mapped to a port of componentId or referenced in the previous triExecuteTestCase statement. |
| **Effect** | The TE can enqueue this exception for the procedure call with the signature identifier signatureId at the port of the component componentId to which the TSI port tsiPortId is mapped.  The decoding of the exception has to be done within the TE. |

## 7.5A Changes to clause 5.5.5 of ETSI ES 201 873-5, Miscellaneous operations

5.5.5.2 triSUTActionParam 🡪 xtriSUTActionParam

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriSUTActionParam (  in TciParameterListType parameterList) |
| **In Parameters** | parameterList parameters of an action to be taken on the SUT |
| **Out Parameters** | n.a. |
| **Return Value** | The return status of the xtriSUTActionParam operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a TTCN‑3 SUT action operation, which either contains multiple arguments or a single argument that is not a character string literal. |
| **Effect** | On invocation of this operation the SA shall initiate the described actions to be taken on the SUT, e.g. turn on, initialize, or send a message to the SUT.  The xtriSUTActionParam operation returns *TRI\_OK* on successful execution of the operation, *TRI\_Error* otherwise. Notice that the return value of this TRI operation does not make any statement about the success or failure of the actions to be taken on the SUT. |

## 7.5B Addition to clause 5.5.5 of ETSI ES 201 873-5, Miscellaneous operations

In order to properly log message or procedure communication via TCI TL, an optional xtriDisplay function is used for conversion of not encoded XTRI data structures into a format suitable for TCI TL operations.

5.5.5.3 xtriDisplay

|  |  |
| --- | --- |
| **Signature** | TriMessageType xtriDisplay(in TriComponentIdType componentId, in TriPortIdType tsiPortId, in Value dataToDisplay) |
| **In Parameters** | componentId identifier of the sending or receiving test component  tsiPortId identifier of the test system interface port via which the message was sent to the SUT adaptor or received from it  dataToDisplay data to be logged |
| **Out Parameters** | n.a. |
| **Return Value** | Data in the format suitable for TCI logging or null if no logging format is available. |
| **Constraints** | This optional TRI operation is called by the TE when it logs message or procedure communication and a TCI TL operation requires data in its encoded form (TriMessageType for messages; TriParameterListType, TriParameterType and TriExceptionType for procedures; TriAddressType for addresses). |
| **Effect** | The operation converts the supplied value to a TRI data structure and returns it. The converted structure typically contains the data in a form that can be used in the logs for increased readability. The conversion might be context-specific, depending on the provided component and TSI port participating in the logged communication operation. If the conversion is not supported, the distinct null value shall be returned. |

## 7.6 Changes to clause 5.6.3 of ETSI ES 201 873-5, Miscellaneous operations

5.6.3.1 triExternalFunction 🡪 xtriExternalFunction

|  |  |
| --- | --- |
| **Signature** | TriStatusType xtriExternalFunction(  in TriFunctionIdType functionId, inout TciParameterListType parameterList, out Value returnValue) |
| **In Parameters** | functionId identifier of the external function |
| **Out Parameters** | returnValue (optional) encoded return value |
| **InOutParameters** | parameterList a list of ~~encoded~~ parameters for the indicated function. The parameters in parameterList are ordered as they appear in the TTCN‑3 function declaration. |
| **Return Value** | The return status of the triExternalFunction operation. The return status indicates the local success (***TRI\_OK***) or failure (***TRI\_Error***) of the operation. |
| **Constraints** | This operation is called by the TE when it executes a function which is defined to be TTCN‑3 external (i.e. all non‑external functions are implemented within the TE).  No error shall be indicated by the PA in case the value of any *out* parameter is non‑null. |
| **Effect** | For each external function specified in the TTCN‑3 ATS the PA shall implement the behaviour. On invocation of this operation the PA shall invoke the function indicated by the identifier functionId. It shall access the specified *in* and *inout* function parameters in parameterList, evaluate the external function using the values of these parameters, and compute values for *inout* and *out* parameters in parameterList. The operation shall then return values for all *inout* and *out* function parameters and the return value of the external function.  If no return type has been defined for this external function in the TTCN‑3 ATS, the distinct value null shall be used for the latter.  The triExternalFunction operation returns ***TRI\_OK*** if the PA completes the evaluation of the external function successfully, ***TRI\_Error*** otherwise.  Note that whereas all other TRI operations are considered to be non‑blocking, the triExternalFunction operation is considered to be *blocking.* That means that the operation shall not return before the indicated external function has been fully evaluated. External functions have to be implemented carefully as they could cause deadlock of test component execution or even the entire test system implementation. |

5.6.3.3 triRnd 🡪 xtriRnd

|  |  |
| --- | --- |
| **Signature** | FloatValue xtriRnd(in TriComponentIdType componentId, in FloatValue seed) |
| **In Parameters** | componentId identifier of the component for which to generate the random number |
|  | seed the seed to be used for generation of the random number or null |
| **Out Parameters** | n.a. |
| **Return Value** | The generated float random number. |
| **Constraints** | This operation is called by the PA to generate a random number in the context of an external function. |
| **Effect** | A random number is generated in the scope of the component identified by the given component Id using the given seed (if any) according to the specification of the predefined rnd function defined in ETSI ES 201 873‑1 [1]. |

## 7.7 Changes to clause 6 of ETSI ES 201 873-5, Java language mapping

Addition of the following clause in clause 6.3 Type mapping.

6.3.3 Any type mapping

The IDL any type is represented by Java java.lang.Object.

6.5.2.1 Changes to triCommunicationSA

The extension to the triCommunicationSA interface is mapped to the following interface:

// TriCommunication

// TE ‑> SA

package org.etsi.ttcn.xtri;

public interface xTriCommunicationSA {

public TriStatus xtriMapParam(TriPortId compPortId, TriPortId tsiPortId,  
 TciParameterList paramList);

// Ref: TRI‑Definition 5.5.2.3

public TriStatus xtriUnmapParam(TriPortId compPortId, TriPortId tsiPortId,  
 TciParameterList paramList);

// Ref: TRI‑Definition 5.5.2.4

// Message based communication operations

// Ref: TRI‑Definition 5.5.3.1

public TriStatus xtriSend(TriComponentId componentId, TriPortId tsiPortId,

Value sutAddress, Value sendMessage);

// Ref: TRI‑Definition 5.5.3.2

public TriStatus xtriSendBC(TriComponentId componentId, TriPortId tsiPortId,

Value sendMessage);

// Ref: TRI‑Definition 5.5.3.3

public TriStatus xtriSendMC(TriComponentId componentId, TriPortId tsiPortId,

TciValueList sutAddresses, Value sendMessage);

// Procedure based communication operations

// Ref: TRI‑Definition 5.5.4.1

public TriStatus xtriCall(TriComponentId componentId,

TriPortId tsiPortId, Value sutAddress,

TriSignatureId signatureId, TciParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.2

public TriStatus xtriCallBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId, TciParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.3

public TriStatus xtriCallMC(TriComponentId componentId,

TriPortId tsiPortId, TciValueList sutAddresses,

TriSignatureId signatureId, TciParameterList parameterList);

// Ref: TRI‑Definition 5.5.4.4

public TriStatus xtriReply(TriComponentId componentId,

TriPortId tsiPortId, Value sutAddress,

TriSignatureId signatureId, TciParameterList parameterList,

Value returnValue);

// Ref: TRI‑Definition 5.5.4.5

public TriStatus xtriReplyBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId, TciParameterList parameterList,

Value returnValue);

// Ref: TRI‑Definition 5.5.4.6

public TriStatus xtriReplyMC(TriComponentId componentId,

TriPortId tsiPortId, TciValueList sutAddresses,

TriSignatureId signatureId, TciParameterList parameterList,

Value returnValue);

// Ref: TRI‑Definition 5.5.4.7

public TriStatus xtriRaise(TriComponentId componentId, TriPortId tsiPortId,

Value sutAddress,

TriSignatureId signatureId,

Value exc);

// Ref: TRI‑Definition 5.5.4.8

public TriStatus xtriRaiseBC(TriComponentId componentId,

TriPortId tsiPortId,

TriSignatureId signatureId,

Value exc);

// Ref: TRI‑Definition 5.5.4.9

public TriStatus xtriRaiseMC(TriComponentId componentId, TriPortId tsiPortId,

TciValueList sutAddresses,

TriSignatureId signatureId,

Value exc);

// Miscellaneous operations

// Ref: TRI‑Definition 5.5.3.5

public Value xtriConvert(Object value, Type typeHypothesis);

// Ref: TRI‑Definition 5.5.5.2

public TriStatus xtriSutActionParam(TciParameterList parameterList);

// Ref: TRI‑Definition 5.5.5.3

public TriMessage xtriDisplay(TriComponentId componentId, TriPortId tsiPortId,

Value dataToDisplay);

}

6.5.2.2 Changes to triCommunicationTE

The extension to the triCommunicationTE interface is mapped to the following interface:

// TriCommunication

// SA ‑> TE

package org.etsi.ttcn.xtri;

public interface xTriCommunicationTE {

// Message based communication operations

// Ref: TRI‑Definition 5.5.3.4

public void xtriEnqueueMsg(TriPortId tsiPortId,

Object sutAddress, TriComponentId componentId,

Object receivedMessage);

// Procedure based communication operations

// Ref: TRI‑Definition 5.5.4.10

public void xtriEnqueueCall(TriPortId tsiPortId,

Object sutAddress, TriComponentId componentId,

TriSignatureId signatureId, TciParameterList parameterList );

// Ref: TRI‑Definition 5.5.4.11

public void xtriEnqueueReply(TriPortId tsiPortId, Object sutAddress,

TriComponentId componentId, TriSignatureId signatureId,

TciParameterList parameterList, Value returnValue);

// Ref: TRI‑Definition 5.5.4.12

public void xtriEnqueueException(TriPortId tsiPortId,

Object sutAddress, TriComponentId componentId,

TriSignatureId signatureId, Object exc);

// Error handling

// Ref: TRI‑Definition 5.2.1

public void xtriSAErrorReq (String message, Object cause);

}

6.5.3.1 Changes to TriPlatformPA

The extension to the triPlatformPA interface is mapped to the following interface:

// TriPlatform

// TE ‑> PA

package org.etsi.ttcn.xtri;

public interface xTriPlatformPA {

// Ref: TRI‑Definition 5.6.3.1

public TriStatus xtriExternalFunction(TriFunctionId functionId,

TciParameterList parameterList, Value returnValue);

}

6.5.3.2 Changes to TriPlatformTE

The extension to the triPlatformTE interface is mapped to the following interface:

// TriPlatform

// PA ‑> TE

package org.etsi.ttcn.xtri;

public interface xTriPlatformTE {

// Error handling

// Ref: TRI‑Definition 5.2.2

public void xtriPAErrorReq (String message, Object cause);

// Ref: TRI-Definition 5.6.3.3

public FloatValue xtriRnd(TriComponentId componentId, FloatValue seed);}

## 7.8 Changes to clause 7 of ETSI ES 201 873-5, C language mapping

7.2.1 Changes to Abstract type mapping

| TRI ADT | ANSI C Representation | Notes and comments |
| --- | --- | --- |
| any | typedef enum {   e\_char = 1, // character   e\_unsigned\_char = 2, // unsigned char   e\_signed\_char = 3, // signed char    e\_short = 4, // short signed integer   e\_short\_int = 5, // short signed integer   e\_signed\_short = 6, // short signed integer   e\_signed\_short\_int = 7, // short signed integer  e\_unsigned\_short = 8, // unsigned short  e\_unsigned\_short\_int = 9, // unsigned short integer    e\_int = 10, // integer    e\_signed\_int = 11, // signed integer  e\_unsigned = 12, // unsigned   e\_unsigned\_int = 13, // unsigned integer    e\_long = 14, // long integer    e\_long\_int = 15, // long integer    e\_signed\_long = 16, // signed long integer    e\_signed\_long\_int = 17, // signed long integer  e\_unsigned\_long = 18, // unsigned long integer  e\_unsigned\_long\_int = 19, // unsigned long integer    e\_long\_long = 20, // long long integer    e\_long\_long\_int = 21, // long long integer    e\_signed\_long\_long = 22, // signed long long integer    e\_signed\_long\_long\_int = 23, // signed long long integer    e\_unsigned\_long\_long = 24, // unsigned long long integer    e\_unsigned\_long\_long\_int = 25,// unsigned long long integer    e\_float = 26, // float   e\_double = 27, // double   e\_long\_double = 28, // long double    e\_ptr = 29, // void \*    e\_char\_string = 30, // char \*   e\_wchar\_string = 31 // wchar\_t \*  } type\_kind;  typedef void \*value;  typedef struct {   type\_kind tag;   value val; } Object; |  |

7.2.4 Changes to TRI operation mapping

TriStatus xtriMapParam

(const TriPortId\* compPortId,

const TriPortId\* tsiPortId,

const TciParameterListType\* parameterList)

TriStatus xtriUnmapParam

(const TriPortId\* compPortId,

const TriPortId\* tsiPortId,

const TciParameterListType\* parameterList)

TriStatus xtriSend

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const Value\* sutAddress,

const Value\* sendMessage)

TriStatus xtriSendBC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const Value\* sendMessage)

TriStatus xtriSendMC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TciValueList\* sutAddresses,

const Value\* sendMessage)

void xtriEnqueueMsg

(const TriPortId\* tsiPortId,

const Object\* sutAddress,

const TriComponentId\* componentId,

const Object\* receivedMessage)

TriStatus xtriCall

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const Value\* sutAddress,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList)

TriStatus xtriCallBC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList)

TriStatus xtriCallMC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TciValueList\* sutAddresses,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList)

TriStatus xtriReply

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const Value\* sutAddress,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList,

const Value\* returnValue)

TriStatus xtriReplyBC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList,

const Value\* returnValue)

TriStatus xtriReplyMC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TciValueList\* sutAddresses,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList,

const Value\* returnValue)

TriStatus xtriRaise

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const Value\* sutAddress,

const TriSignatureId\* signatureId,

const Value\* exception)

TriStatus xtriRaiseBC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TriSignatureId\* signatureId,

const Value\* exception)

TriStatus xtriRaiseMC

(const TriComponentId\* componentId,

const TriPortId\* tsiPortId,

const TciValueList\* sutAddresses,

const TriSignatureId\* signatureId,

const Value\* exception)

TriStatus xtriSutActionParam

(const TciParameterListType\* parameterList)

void xtriEnqueueCall

(const TriPortId\* tsiPortId,

const Object\* sutAddress,

const TriComponentId\* componentId,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList)

void xtriEnqueueReply

(const TriPortId\* tsiPortId,

const Object\* sutAddress,

const TriComponentId\* componentId,

const TriSignatureId\* signatureId,

const TciParameterListType\* parameterList,

const Value\* returnValue)

void xtriEnqueueException

(const TriPortId\* tsiPortId,

const Object\* sutAddress,

const TriComponentId\* componentId,

const TriSignatureId\* signatureId,

const Object\* exception)

TriStatus xtriExternalFunction

(const TriFunctionId\* functionId,

TciParameterListType\* parameterList,

Value\* returnValue)

Value xtriConvert

(const Object\* value,

const Type\* typeHypothesis)

TFloat xtriRnd(TriComponentId \*componentId, TFloat\* seed)

void xtriPAErrorReq

(const char\* message,

const Object\* cause)

void xtriSAErrorReq

(const char\* message,

const Object\* cause)

TriMessage \* xtriDisplay(TriComponentId \* componentId, TriPortId \* tsiPortId,

Value dataToDisplay)

## 7.9 Changes to clause 8 of ETSI ES 201 873-5, C++ language mapping

Addition of the following clause in clause 8.5 Type mapping.

8.5.3 Any type mapping

The IDL any type is represented by struct type of type tag and value:

typedef enum {  
  e\_char = 1, // character  
  e\_unsigned\_char = 2, // unsigned char  
  e\_signed\_char = 3, // signed char

  e\_short = 4, // short signed integer  
  e\_short\_int = 5, // short signed integer  
  e\_signed\_short = 6, // short signed integer  
  e\_signed\_short\_int = 7, // short signed integer

e\_unsigned\_short = 8, // unsigned short  
 e\_unsigned\_short\_int = 9, // unsigned short integer

  e\_int = 10, // integer

  e\_signed\_int = 11, // signed integer

e\_unsigned = 12, // unsigned   
 e\_unsigned\_int = 13, // unsigned integer

  e\_long = 14, // long integer

  e\_long\_int = 15, // long integer

  e\_signed\_long = 16, // signed long integer

  e\_signed\_long\_int = 17, // signed long integer

e\_unsigned\_long = 18, // unsigned long integer  
 e\_unsigned\_long\_int = 19, // unsigned long integer

  e\_long\_long = 20, // long long integer

  e\_long\_long\_int = 21, // long long integer

  e\_signed\_long\_long = 22, // signed long long integer

  e\_signed\_long\_long\_int = 23, // signed long long integer

  e\_unsigned\_long\_long = 24, // unsigned long long integer

  e\_unsigned\_long\_long\_int = 25, // unsigned long long integer

  e\_float = 26, // float  
  e\_double = 27, // double  
  e\_long\_double = 28, // long double

  e\_ptr = 29 // void \*

  e\_char\_string = 30, // char \*  
  e\_wchar\_string = 31 // wchar\_t \*

} type\_kind;

typedef void \*value;  
  
typedef struct {  
  type\_kind tag;  
  value val;  
} Object;

8.6.1 Changes to TriCommunicationSA

The extension to the TriCommunicationSA class is mapped to the following class:

class xTriCommunicationSA {

public:

//Destructor.

virtual ~xTriCommunicationSA ();

//To establish a dynamic connection between two ports.

virtual TriStatus xtriMapParam (const TriPortId \*comPortId, const TriPortId \*tsiPortId,   
 TciParameterList \*parameterList)=0;

//To close a dynamic connection to the SUT for the referenced TSI port.

virtual TriStatus xtriUnmapParam (const TriPortId \*comPortId, const TriPortId \*tsiPortId,   
 TciParameterList \*parameterList)=0;

//Send operation on a component which has been mapped to a TSI port.

virtual TriStatus xtriSend (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValue \*SUTaddress, const TciValue \*sendMessage)=0;

//Send (broadcast) operation on a component which has been mapped to a TSI port.

virtual TriStatus xtriSendBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValue \*sendMessage)=0;

//Send (multicast) operation on a component which has been mapped to a TSI port.

virtual TriStatus xtriSendMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValueList \*SUTaddresses, const TciValue \*sendMessage)=0;

//Initiate the procedure call.

virtual TriStatus xtriCall (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValue \*sutAddress, const TriSignatureId \*signatureId, const TciParameterList \*parameterList)=0;

//Initiate and broadcast the procedure call.

virtual TriStatus xtriCallBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TciParameterList \*parameterList)=0;

//Initiate and multicast the procedure call.

virtual TriStatus xtriCallMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValueList \*sutAddresses, const TriSignatureId \*signatureId, const TciParameterList \*parameterList)=0;

//Issue the reply to a procedure call.

virtual TriStatus xtriReply (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValue \*sutAddress, const TriSignatureId \*signatureId, const TciParameterList \* parameterList, const TciValue \*returnValue)=0;

//Broadcast the reply to a procedure call.

virtual TriStatus xtriReplyBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TciParameterList \*parameterList, const TciValue \*returnValue)=0;

//Multicast the reply to a procedure call.

virtual TriStatus xtriReplyMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValueList \*sutAddresses, const TriSignatureId \*signatureId, const TciParameterList \*parameterList, const TciValue \*returnValue)=0;

//Raise an exception to a procedure call.

virtual TriStatus xtriRaise (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValue \*sutAddress, const TriSignatureId \*signatureId, const TciValue \*exc)=0;

//Raise a broadcast an exception to a procedure call.

virtual TriStatus xtriRaiseBC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TriSignatureId \*signatureId, const TciValue \*exc)=0;

//Raise a multicast an exception to a procedure call.

virtual TriStatus xtriRaiseMC (const TriComponentId \*componentId, const TriPortId \*tsiPortId, const TciValueList \*sutAddresses, const TriSignatureId \*signatureId, const TciValue \*exc)=0;

Conversion of received data

virtual TciValue \*xtriConvert(const Object \*value, const TciType \*typeHypothesis)=0;

//Perform an SUT action with parameters

virtual TriStatus xtriSUTActionParam (const TciParameterList \*parameterList)=0;

// Conversion to the logging format

virtual TriMessage \* xtriDisplay(const TriComponentId \* componentId, const TriPortId \* tsiPortId, const TciValue dataToDisplay)=0;

}

8.6.2 Changes to TriCommunicationTE

The extension to the TriCommunicationTE class is mapped to the following class:

class xTriCommunicationTE {

public:

//Destructor.

virtual ~xTriCommunicationTE ();

//Called by SA after it has received a message from the SUT.

virtual void xtriEnqueueMsg (const TriPortId \*tsiPortId, const Object \*SUTaddress, const TriComponentId \*componentId, const Object \*receivedMessage)=0;

//Called by SA after it has received a procedure call from the SUT.

virtual void xtriEnqueueCall (const TriPortId \*tsiPortId, const Object \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const TciParameterList \*parameterList)=0;

//Called by SA after it has received a reply from the SUT.

virtual void xtriEnqueueReply (const TriPortId \*tsiPortId, const Object \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const TciParameterList \*parameterList, const TciValue \*returnValue)=0;

//Called by SA after it has received an exception from the SUT.

virtual void xtriEnqueueException (const TriPortId \*tsiPortId, const Object \*SUTaddress, const TriComponentId \*componentId, const TriSignatureId \*signatureId, const Object \*exc)=0;

// Error handling

virtual void xtriSAErrorReq (const String message, const Object \*cause)=0;

}

8.6.3 Changes to TriPlatformPA

The extension to the TriPlatformPA class is mapped to the following class:

class xTriPlatformPA {

public:

//Destructor.

virtual ~xTriPlatformPA ();

//For each external function specified in the TTCN-3 ATS implement the behaviour.

virtual TriStatus xtriExternalFunction (const TriFunctionId \*functionId, TciParameterList \*parameterList, TciValue \*returnValue)=0;

}

8.6.4 Changes to TriPlatformTE

The extension to the TriPlatformTE class is mapped to the following interface:

class TriPlatformTE {

public:

//Destructor.

virtual ~xTriPlatformTE ();

//Called by PA in unrecoverable error situations.

virtual void xtriPAError (const Tstring &message, const Object \*cause)=0;

//Generate random number.

virtual FloatValue\* xtriRnd (const TriComponentId \*componentId, const FloatValue \*seed)=0;

}

## 7.10 Changes to clause 9 of ETSI ES 201 873-5, C# language mapping

Addition of the following clause in clause 9.4 Type mapping.

9.4.3 Any type mapping

The IDL any type is represented by C# object.

9.5.2.1 Changes to ITriCommunicationSA

The extension to the **ITriCommunicationSA** interface is defined as follows:

public interface IXTriCommunicationSA {  
 // Reset operation  
 // Ref: TRI-Definition 5.5.1  
 TriStatus XTriMapParam(ITriPortId compPortId, ITriPortId tsiPortId,  
 ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.2.3  
 TriStatus XTriUnmapParam(ITriPortId compPortId, ITriPortId tsiPortId,  
 ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.2.4  
  
 // Message based communication operations  
 // Ref: TRI-Definition 5.5.3.1  
 TriStatus XTriSend(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue address, ITciValue sentMessage);  
 // Ref: TRI-Definition 5.5.3.2  
 TriStatus XTriSendBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue sentMessage);  
 // Ref: TRI-Definition 5.5.3.3  
 TriStatus XTriSendMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValueList addresses, ITciValue sentMessage);  
  
 // Procedure based communication operations  
 // Ref: TRI-Definition 5.5.4.1  
 TriStatus XTriCall(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue sutAddress, ITriSignatureId signatureId,  
 ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.4.2  
 TriStatus XTriCallBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.4.3  
 TriStatus XTriCallMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValueList sutAddresses, ITriSignatureId signatureId,  
 ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.4.4  
 TriStatus XTriReply(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue sutAddress, ITriSignatureId signatureId,  
 ITciParameterList parameterList, ITciValue returnValue);  
 // Ref: TRI-Definition 5.5.4.5  
 TriStatus XTriReplyBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITciParameterList parameterList,  
 ITciValue returnValue);  
 // Ref: TRI-Definition 5.5.4.6  
 TriStatus XTriReplyMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValueList sutAddresses, ITriSignatureId signatureId,  
 ITciParameterList parameterList, ITciValue returnValue);  
 // Ref: TRI-Definition 5.5.4.7  
 TriStatus XTriRaise(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue sutAddress, ITriSignatureId signatureId,  
 ITciValue exc);  
 // Ref: TRI-Definition 5.5.4.8  
 TriStatus XTriRaiseBC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITriSignatureId signatureId, ITciValue exc);  
 // Ref: TRI-Definition 5.5.4.9  
 TriStatus XTriRaiseMC(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValueList sutAddresses, ITriSignatureId signatureId,  
 ITciValue exc);  
 // Ref: TRI‑Definition 5.5.3.5

ITciValue XTriConvert(object value, ITciType typeHypothesis);

// Ref: TRI-Definition 5.5.5.2  
 TriStatus XTriSutActionParam(ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.5.3  
 ITriMessage XTriDisplay(ITriComponentId componentId, ITriPortId tsiPortId,  
 ITciValue dataToDisplay);

}

9.5.2.2 Changes to ITriCommunicationTE

The extension to the **ITriCommunicationTE** interface is defined as follows:

public interface IXTriCommunicationTE {  
 // Message based communication operations  
 // Ref: TRI-Definition 5.5.3.4  
 void XTriEnqueueMessage(ITriPortId tsiPortId, object sutAddress,  
 ITriComponentId componentId, object msg);  
  
 // Procedure based communication operations  
 // Ref: TRI-Definition 5.5.4.10  
 void XTriEnqueueCall(ITriPortId tsiPortId, object sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 ITciParameterList parameterList);  
 // Ref: TRI-Definition 5.5.4.10  
 void XTriEnqueueReply(ITriPortId tsiPortId, object sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 ITciParameterList parameterList, ITciValue returnValue);  
 // Ref: TRI-Definition 5.5.4.11  
 void XTriEnqueueException(ITriPortId tsiPortId, object sutAddress,  
 ITriComponentId componentId, ITriSignatureId signatureId,   
 object exc);

// Ref: TRI Definition 5.2.1

void XTriSAErrorReq (string message, object cause);

}

9.5.2.3 Changes to ITriPlatformPA

The extension to the **ITriPlatformPA** interface is defined as follows:

public interface IXTriPlatformPA {  
 // Ref: TRI-Definition 5.6.1 // Miscellaneous operations  
 // Ref: TRI-Definition 5.6.3.1  
 TriStatus XTriExternalFunction(ITriFunctionId functionId,   
 ITciParameterList parameterList, ITciValue returnValue);  
}

9.5.2.4 Changes to ITriPlatformTE

The extension to the **ITriPlatformTE** interface is defined as follows:

public interface ITriPlatformTE {

// Ref: TRI Definition 5.2.2

void XTriPAErrorReq (string message, object cause);

// Ref: TRI Definition clause 5.6.3.3

FloatValue XTriRnd(ITriComponentId componentId, FloatValue seed);

}

# 8 TCI extensions for the package

Not applicable.

Annex A (informative):  
Bibliography

* ETSI ES 201 873-3: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 3: TTCN-3 Graphical presentation Format (GFT)".

# History

|  |  |  |
| --- | --- | --- |
| **Document history** | | |
| V1.1.1 | April 2012 | Publication |
| V1.2.1 | April 2013 | Publication |
| V1.3.1 | June 2014 | Publication |
| V1.4.1 | June 2015 | Publication |
| V1.5.1 | February 2020 | Membership Approval Procedure MV 20200428: 2020-02-28 to 2020-04-28 |
| V1.5.1 | May 2020 | Publication |