/***************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:21.1.2, violation of strong typing rules for PTC ports in unmap operations
 ** @verdict  pass reject
 ***************************************************/

// The following requirements are tested:
// If the type of the component referenced in a connection operation is known (either
// when the component reference is a variable or value returned from a function or the
// type is defined the runs on, mtc or system clause of the calling function), the
// referenced port declaration shall be present in this component type.

module NegSem_210102_disconnect_and_unmap_operations_013 {

	type port P message {
		inout integer;
	}

	type component GeneralComp {
		port P p;
	}

    type component GeneralCompEx extends GeneralComp {
        port P p2;
    }

	testcase TC_NegSem_210102_disconnect_and_unmap_operations_013() runs on GeneralComp system GeneralComp {
        var GeneralCompEx v_ptc := GeneralCompEx.create;
        var GeneralComp v_ptcAlias := v_ptc;
		map(system:p, v_ptc:p2);
        unmap(system:p, v_ptcAlias:p2);// although the actual PTC instance contains the p2 port,
          // it cannot be referenced as the variable v_ptc is of the GeneralComp type and
          // not GeneralCompEx
		setverdict(pass);
	}

	control{
	    execute(TC_NegSem_210102_disconnect_and_unmap_operations_013());
	}
}
