/*****************************************************************
 ** @author   STF 487
 ** @version  0.0.1
 ** @purpose  1:22.2.2, insufficient value range of variable in index redirection
 ** @verdict  pass reject
 *****************************************************************/

// The following requirements are tested:
// If the index redirection is used for single-dimensional port arrays, the type of the
// integer variable shall allow storing the highest index of the respective array.

module NegSem_220202_ReceiveOperation_019 {
    type integer RestrInt(0..2);
	type port P message {
		inout integer;
	}

    type component GeneralComp {
		port P p[10];
	}

    testcase TC_NegSem_220202_ReceiveOperation_019() runs on GeneralComp {
        var RestrInt v_int;
        p[5].send(100);
        any from p.receive(integer:?) -> @index value v_int;
        setverdict(pass);
    }

    control {
        execute(TC_NegSem_220202_ReceiveOperation_019(), 5.0);
    }
}