/***************************************************
 ** @author   STF 433
 ** @version  0.0.1
 ** @purpose  1:24.4, Ensure timer read result is non-negative float
 ** @verdict  pass accept, ttcn3verdict:pass
 ***************************************************/
// #reqname  /Requirements/23 Timer operations/23.4 The Read timer operation/Read returns elapsed time that is non-neg float


module Sem_2304_timer_read_003 {
    type component TComp{
        timer t_aux := 1.0;
        timer t_aux2 := 1.05;
        timer t_timer := 20.0;
    }
    testcase TC_Sem_2304_timer_read_003() runs on TComp{
        var float v_elapsed;

        t_aux2.start;

        t_timer.start;

		// wait for 1 second
        t_aux.start;
		t_aux.timeout;

        v_elapsed:=t_timer.read;
        if (v_elapsed < 1.0){
            setverdict(fail);
        } else {
			setverdict(pass);
        }
        if (t_aux2.running) {
            if (v_elapsed <= 1.05) {
                setverdict(pass);
            } else {
            	setverdict(fail);
            }
        }
    }
    control{

            execute(TC_Sem_2304_timer_read_003())


    }
}
