*** Settings ***
Library           JSONSchemaLibrary    schemas/
Resource          environment/variables.txt    # Generic Parameters
Library           JSONLibrary
Resource          VNFIndicatorsKeywords.robot
Library           REST    ${VNFM_SCHEMA}://${VNFM_HOST}:${VNFM_PORT}    ssl_verify=false

*** Test Cases ***
Get all VNF Indicators
    [Documentation]    Test ID: 7.3.6.1.1
    ...    Test title: Get all VNF Indicators
    ...    Test objective: The objective is to test the retrieval of all the available VNF indicators and perform a JSON schema validation of the collected indicators data structure
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get all VNF indicators
    Check HTTP Response Status Code Is    200
    Check HTTP Response Body Json Schema Is   vnfIndicators
    
Get VNF Indicators with attribute-based filter
    [Documentation]    Test ID: 7.3.6.1.2
    ...    Test title: Get VNF Indicators with attribute-based filter
    ...    Test objective: The objective is to test the retrieval of VNF indicators using attribute-based filter, perform a JSON schema validation of the collected indicators data structure, and verify that the retrieved information matches the issued attribute-based filters 
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get VNF indicators with filter
    Check HTTP Response Status Code Is    200
    Check HTTP Response Body Json Schema Is   vnfIndicators
    Check HTTP Response Body vnfIndicators Matches the requested attribute-based filter

Get VNF Indicators with invalid attribute-based filter
    [Documentation]    Test ID: 7.3.6.1.3
    ...    Test title: Get VNF Indicators with invalid attribute-based filter
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails when using invalid attribute-based filters, and perform the JSON schema validation of the failed operation HTTP response. 
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get VNF indicators with invalid filter
    Check HTTP Response Status Code Is    400
    Check HTTP Response Body Json Schema Is   ProblemDetails

Get all VNF Indicators with malformed authorization token
    [Documentation]    Test ID: 7.3.6.1.4
    ...    Test title: Get all VNF Indicators with malformed authorization token
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails when using malformed authorization token
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: The VNFM requires the usage of access tokens for authorizing the API requests.
    ...    Post-Conditions: none
    Get all VNF indicators with malformed authorization token
    Check HTTP Response Status Code Is    400

Get all VNF Indicators without authorization token
    [Documentation]    Test ID: 7.3.6.1.5
    ...    Test title: Get all VNF Indicators without authorization token
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails when omitting the authorization token
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: The VNF requires the usage of access tokens for authorizing the API requests.
    ...    Post-Conditions: none
    Get all VNF indicators without authorization token
    Check HTTP Response Status Code Is    401

GET all VNF Indicators with expired or revoked authorization token
    [Documentation]    Test ID: 7.3.6.1.6
    ...    Test title: GET all VNF Indicators with expired or revoked authorization token
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails when using expired or revoked authorization token
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: The VNF requires the usage of access tokens for authorizing the API requests.
    ...    Post-Conditions: none
    Get all VNF indicators with expired or revoked authorization token
    Check HTTP Response Status Code Is    401

Get all VNF Indicators with invalid resource endpoint
    [Documentation]    Test ID: 7.3.6.1.7
    ...    Test title: Get all VNF Indicators with invalid resource endpoint
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails when using invalid resource endpoint
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get all VNF indicators with invalid resource endpoint
    Check HTTP Response Status Code Is    404

POST all VNF Indicators - Method not implemented
    [Documentation]    Test ID: 7.3.6.1.8
    ...    Test title: POST all VNF Indicators - Method not implemented
    ...    Test objective: The objective is to test that POST method is not allowed to create new VNF indicators
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM
    ...    Reference: Clause 8.4.2.3.1 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Send POST Request for all VNF indicators
    Check HTTP Response Status Code Is    405

PUT all VNF Indicators - Method not implemented
    [Documentation]    Test ID: 7.3.6.1.9
    ...    Test title: PUT all VNF Indicators - Method not implemented
    ...    Test objective: The objective is to test that PUT method is not allowed to modify VNF indicators
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM
    ...    Reference: Clause 8.4.2.3.3 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Send PUT Request for all VNF indicators
    Check HTTP Response Status Code Is    405

PATCH all VNF Indicators - Method not implemented
     [Documentation]    Test ID: 7.3.6.1.10
    ...    Test title: PATCH all VNF Indicators - Method not implemented
    ...    Test objective: The objective is to test that PATCH method is not allowed to update VNF indicators
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNF
    ...    Reference: Clause 8.4.2.3.4 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Send PATCH Request for all VNF indicators
    Check HTTP Response Status Code Is    405

DELETE all VNF Indicators - Method not implemented
    [Documentation]    Test ID: 7.3.6.1.11
    ...    Test title: DELETE all VNF Indicators - Method not implemented
    ...    Test objective: The objective is to test that DELETE method is not allowed to delete VNF indicators
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNF
    ...    Reference: Clause 8.4.2.3.5 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: The VNF indicators are not deleted by the unsuccessful operation
    Send DELETE Request for all VNF indicators
    Check HTTP Response Status Code Is    405
    Check Postcondition VNF Indicators Exist
    
Get all VNF Indicators as Paged Response
    [Documentation]    Test ID: 7.3.6.1.12
    ...    Test title: Get all VNF Indicators as Paged Response
    ...    Test objective: The objective is to test the retrieval of all the available VNF indicators as Paged Response.
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get all VNF indicators
    Check HTTP Response Status Code Is    200
    Check HTTP Response Header Contain Link

Get VNF Indicators - Bad Request Response too Big
    [Documentation]    Test ID: 7.3.6.1.13
    ...    Test title: Get VNF Indicators - Bad Request Response too Big
    ...    Test objective: The objective is to test that the retrieval of VNF indicators fails because reponse is too big, and perform the JSON schema validation of the failed operation HTTP response. 
    ...    Pre-conditions: A VNF instance is instantiated. One or more measures of VNF indicators are available in the VNFM.
    ...    Reference: Clause 8.4.2.3.2 - ETSI GS NFV-SOL 003 [1] v2.7.1
    ...    Config ID: Config_prod_VNFM
    ...    Applicability: none
    ...    Post-Conditions: none
    Get all VNF indicators
    Check HTTP Response Status Code Is    400
    Check HTTP Response Body Json Schema Is   ProblemDetails