*** Settings ***
Resource    NSLCMOperationKeywords.robot 

*** Test Cases ***
POST Individual VNF Snapshot - Method not implemented
    [Documentation]    Test ID: 5.3.2.27.1
    ...    Test title: POST Individual VNF Snapshot - Method not implemented
    ...    Test objective: The objective is to test that POST method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.1 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: none
    POST individual VNF Snapshot
    Check HTTP Response Status Code Is    405
    
GET Information about an individual VNF Snapshot - SUCCESSFUL
    [Documentation]    Test ID: 5.3.2.27.2
    ...    Test title: GET Information about an individual VNF Snapshot - SUCCESSFUL
    ...    Test objective: The objective is to GET information about an individual VNF Snapshot
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.2 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: none
    GET individual VNF Snapshot
    Check HTTP Response Status Code Is    200
    Check HTTP Response Body Json Schema Is    VnfSnapshotInfo
        
GET Information about an individual VNF Snapshot - NOT FOUND
     [Documentation]    Test ID: 5.3.2.27.3
    ...    Test title: GET Information about an individual VNF Snapshot - NOT FOUND
    ...    Test objective: The objective is to test that the retrieval of individual VNF Snapshot fails when using an invalid resource identifier.
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.2 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: none
    GET Individual VNF Snapshot with Invalid URI
    Check HTTP Response Status Code Is    404
    Check HTTP Response Body Json Schema Is   ProblemDetails

PUT Individual VNF Snapshot - Method not implemented 
     [Documentation]    Test ID: 5.3.2.27.4
    ...    Test title: PUT Individual VNF Snapshot - Method not implemented
    ...    Test objective: The objective is to test that PUT method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.3 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: none
    PUT individual VNF Snapshot
    Check HTTP Response Status Code Is    405

PATCH Individual VNF Snapshot - Method not implemented 
     [Documentation]    Test ID: 5.3.2.27.5
    ...    Test title: PATCH Individual VNF Snapshot - Method not implemented
    ...    Test objective: The objective is to test that PATCH method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.4 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: VNF Snapshot not modified
    PATCH individual VNF Snapshot
    Check HTTP Response Status Code Is    405

DELETE Individual VNF Snapshot
    [Documentation]    Test ID: 5.3.2.27.6
    ...    Test title: DELETE Individual VNF Snapshot
    ...    Test objective: The objective is to delete a VNF Snapshot
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.5 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: none
    ...    Post-Conditions: VNF Snapshot resource is deleted.
    DELETE individual VNF Snapshot
    Check HTTP Response Status Code Is    204
    Check Postcondition VNF Snapshot Resource Is Deleted

DELETE Individual VNF Snapshot - Conflict
     [Documentation]    Test ID: 5.3.2.27.7
    ...    Test title: DELETE Individual VNF Snapshot Conflict
    ...    Test objective: The objective is to verify that The operation cannot be executed currently, due to a conflict with the state of the VNF Snapshot resource.
    ...    Pre-conditions: none
    ...    Reference: Clause 6.4.20.3.5 - ETSI GS NFV-SOL 005 [3] v3.3.1
    ...    Config ID: Config_prod_NFVO
    ...    Applicability: VNF snapshot is in use by some operation such as reverting a VNF instance to a VNF snapshot or creating a VNF snapshot package.
    ...    Post-Conditions: VNF Snapshot resource is not deleted.
    DELETE individual VNF Snapshot - CONFLICT
    Check HTTP Response Status Code Is    409
    Check HTTP Response Body Json Schema Is    ProblemDetails
    Check Postcondition VNF Snapshot Resource Existence