*** Settings ***
Resource    environment/variables.txt 
Resource    VnfLcmOperationKeywords.robot
Library    REST    ${VNFM_SCHEMA}://${VNFM_HOST}:${VNFM_PORT}       ssl_verify=false 
Library    JSONLibrary
Library    JSONSchemaLibrary    schemas/
Documentation    This resource represents VNF lifecycle management operation occurrences. The client can use this resource to query
...    status information about multiple VNF lifecycle management operation occurrences.

*** Test Cases ***
POST VNF LCM operation occurrences - Method not implemented
    [Documentation]    Test ID: 6.3.5.11.1
    ...    Test title: POST VNF LCM operation occurrences - Method not implemented
    ...    Test objective: The objective is to test that POST method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.1 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none 
    Post VNF LCM OP occurrences
    Check HTTP Response Status Code Is    405

GET status information about multiple VNF LCM operation occurrences 
    [Documentation]    Test ID: 6.3.5.11.2
    ...    Test title: GET status information about multiple VNF LCM operation occurrences
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    GET VNF LCM OP occurrences
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs 
    Check HTTP Response Body vnf LCM OpOCCs content against VNF Descriptor
    
GET status information about multiple VNF LCM operation occurrences Bad Request Invalid attribute-based filtering parameters
    [Documentation]    Test ID: 6.3.5.11.3
    ...    Test title: GET status information about multiple VNF LCM operation occurrences Bad Request Invalid attribute-based filtering parameters
    ...    Test objective: The objective is to test that GET method fail retrieving status information about multiple VNF lifecycle management operation occurrences because attribute is invalid.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    GET VNF LCM OP occurrences invalid attribute
    Check HTTP Response Status Code Is    400
    Check HTTP Response Body Json Schema Is    ProblemDetails

GET status information about multiple VNF LCM Operation occurrences Bad Request Invalid attribute selector
    [Documentation]    Test ID: 6.3.5.11.4
    ...    Test title: GET status information about multiple VNF LCM Operation occurrences Bad Request Invalid attribute selector
    ...    Test objective: The objective is to test that GET method fail retrieving status information about multiple VNF lifecycle management operation occurrences because attribute is invalid.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none 
    GET VNF LCM OP occurrences invalid filter
    Check HTTP Response Status Code Is    400
    Check HTTP Response Body Json Schema Is    ProblemDetails

GET status information about multiple VNF LCM Operation occurrences with "all_fields"   
    [Documentation]    Test ID: 6.3.5.11.5
    ...    Test title: GET status information about multiple VNF LCM Operation OCC with "all_fields"
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    Get VNF LCM Operation occurrences with all_fields attribute selector
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs 

GET status information about multiple VNF LCM Operation occurrences with "exlude_default"   
    [Documentation]    Test ID: 6.3.5.11.6
    ...    Test title: GET status information about multiple VNF LCM Operation OCC with "exclude_default"
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    Get VNF LCM Operation occurrences with exclude_default attribute selector
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs 

GET status information about multiple VNF LCM Operation occurrences with "fields"   
    [Documentation]    Test ID: 6.3.5.11.7
    ...    Test title: GET status information about multiple VNF LCM Operation OCC with "fields"
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    Get VNF LCM Operation occurrences with fields attribute selector
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs

GET status information about multiple VNF LCM Operation occurrences with "exclude_fields"   
    [Documentation]    Test ID: 6.3.5.11.8
    ...    Test title: GET status information about multiple VNF LCM Operation OCC with "exclude_fields"
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    Get VNF LCM Operation occurrences with exclude_fields attribute selector
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs    
    
PUT status information about multiple VNF LCM operation occurrences - Method not implemented
     [Documentation]    Test ID: 6.3.5.11.9
    ...    Test title: PUT status information about multiple VNF LCM operation occurrences - Method not implemented
    ...    Test objective: The objective is to test that PUT method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.3 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none 
    PUT VNF LCM OP occurrences
    Check HTTP Response Status Code Is    405

PATCH status information about multiple VNF LCM operation occurrences - Method not implemented
    [Documentation]    Test ID: 6.3.5.11.10
    ...    Test title: PATCH status information about multiple VNF LCM operation occurrences - Method not implemented
    ...    Test objective: The objective is to test that PATCH method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.4 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none
    PATCH VNF LCM OP occurrences
    Check HTTP Response Status Code Is    405

DELETE status information about multiple VNF LCM operation occurrences - Method not implemented
    [Documentation]    Test ID: 6.3.5.11.11
    ...    Test title: DELETE status information about multiple VNF LCM operation occurrences - Method not implemented
    ...    Test objective: The objective is to test that DELETE method is not implemented
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.5 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none
    DELETE VNF LCM OP occurrences
    Check HTTP Response Status Code Is    405
    
GET status information about multiple VNF LCM operation occurances to get Paged Response   
    [Documentation]    Test ID: 6.3.5.11.12
    ...    Test title: GET status information about multiple VNF LCM operation occurances to get Paged Response
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences to get paged response.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    GET VNF LCM OP occurrences
    Check HTTP Response Status Code Is    200
    Check HTTP Response Header Contain Link
    
GET status information about multiple VNF LCM Operation occurrences Bad Request Response too big
    [Documentation]    Test ID: 6.3.5.11.13
    ...    Test title: GET status information about multiple VNF LCM Operation occurrences Bad Request Response too big
    ...    Test objective: The objective is to test that GET method fail retrieving status information about multiple VNF lifecycle management operation occurrences because Response is too big.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none 
    GET VNF LCM OP occurrences
    Check HTTP Response Status Code Is    400
    Check HTTP Response Body Json Schema Is    ProblemDetails
    
GET status information about multiple VNF LCM Operation occurrences with "exlude_default" and "fields" 
    [Documentation]    Test ID: 6.3.5.11.14
    ...    Test title: GET status information about multiple VNF LCM Operation OCC with "exclude_default" and "fields"
    ...    Test objective: The objective is to test that GET method retrieve Query status information about multiple VNF lifecycle management operation occurrences.
    ...    Pre-conditions: none
    ...    Reference: Clause 5.4.12.3.2 - ETSI GS NFV-SOL 002 [2] v3.3.1
    ...    Config ID: Config_prod_VE
    ...    Applicability: none
    ...    Post-Conditions: none   
    Get VNF LCM Operation occurrences with exclude_default and fields attribute selector
    Check HTTP Response Status Code Is    202
    Check HTTP Response Body Json Schema Is    VnfLcmOpOccs 