(Cmd) # get_interface_inventory_script.txt : script for Lightweight NETCONF controlleur lncc.py
(Cmd) # run me using: lncc.py 'run_script set_tx_power_script.txt' quit
(Cmd) set feedback_to_output true
feedback_to_output - was: False
now: True
(Cmd) ne load ne.yaml
Loading complete: 2 new NEs: ['ne1', 'ne2']
(Cmd) # set logging_config logging_config.yaml
(Cmd) connect
2 new connections, 2 total: ['ne1', 'ne2']
(Cmd) netconf get --filter-file interface_type_microwaveCarrierTermination_filter.xml
NETCONF <get> operation completed: 2 NEs, stored in 'get'
(Cmd) netconf close-session
NETCONF <close-session> operation completed: 2 NEs, stored in 'close-session'
(Cmd) table from_xml --xsl-transform get-interface-transform.xsl
New tables 'get' in each NE, build from XML stored in 'get'
(Cmd) table concat
Table 'get' available for group
(Cmd) table to_excel interfaces.xlsx
Wrote Excel file interfaces.xlsx, with 1 tabs: args.tables
