|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
| **Title\*:** | SOL003ed451 Bug008203 statement correction in clause 5.4.3.3.4 | | |
|  |  | | |
| from **Source**\*: | DOCOMO Communications Lab. | | |
| Contact: | Yinan Liu, Yuya Kuno, Bertrand Souville | | |
|  |  | | |
| input for **Committee**\***:** | NFV SOL | | |
|  |  | | |
| Contribution **For\*:** | Decision | **X** |  |
|  | Discussion |  |  |
|  | Information |  |  |
|  |  | | |
| Submission date**\***: | 2023-06-03 | | |
|  |  | | |
| Meeting & Allocation: | **NFVSOL#248-at NFV#42** - | | |
| Relevant WI(s), or deliverable(s): | RGS/NFV-SOL003ed451 | | |
|  | | | |

**Decision requested:** Please approve

**ABSTRACT:** *This contribution is to fix the bug008203 (*[*http://oldforge.etsi.org/mantis/view.php?id=8203*](http://oldforge.etsi.org/mantis/view.php?id=8203)*) to correct the statement in clause 5.4.3.3.4 where the existing "metadata" is missed.*

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CHANGE REQUEST** | | | | | | | |
| **NFV-SOL003** | **Version** | | **4.4.2** | **CR** | **CR(23)194** | **rev** | - |
|  | | | | | | | |
| ***CR Title:*** | SOL003ed451 Bug008203 statement correction in clause 5.4.3.3.4 | | | | | | |
|  | | | | | | | |
| ***Source:*** | DOCOMO Communications Lab. | | | | | | |
|  | | | | | | | |
| ***Work Item Ref:*** | RGS/NFV-SOL003ed451 | | | | ***Date:*** | 03/06/2023 | |
|  | | | | | | | |
| ***Category:*** | F | | | | ***Release:*** | 4 | |
|  | *Use one of the following categories:*  ***F*** *(correction)*  ***A*** *(corresponds to a correction in an earlier release)*  ***B*** *(addition of feature)*  ***C*** *(functional modification of feature)*  ***D*** *(editorial modification)* | | | | | | |
|  | | | | | | | |
| ***Reason for change:*** | | See ETSI bug tracker [*http://oldforge.etsi.org/mantis/view.php?id=8203*](http://oldforge.etsi.org/mantis/view.php?id=8203)*.* | | | | | |
|  | | | | | | | |
| ***Summary of change:*** | |  | | | | | |
|  | | | | | | | |
| ***Clauses affected:*** | | Clause 5.4.3.3.4 | | | | | |
|  | | | | | | | |
| ***Other deliverables***  ***affected:*** | |  | | | | | |
|  | | | | | | | |
| ***Other comments:*** | | \*\*\* Analysis of backward compatibility changes \*\*\*   * Change Type: BWC * Change Type Code: BWC\_OTHER | | | | | |

\*\*\* START OF CHANGES \*\*\*

|  |
| --- |
| **Change #1** |

<…>

The VNFM shall apply the "metadata", "extensions" and "vnfConfigurableProperties" attributes in the "VnfInfoModificationRequest" data structure in the message content to the existing "metadata", "extensions" and "vnfConfigurableProperties" attributes from the "VnfInstance" data structure according to the rules of JSON Merge Patch (see IETF RFC 7396 [5]).

<…>

\*\*\* END OF CHANGES \*\*\*