/*****************************************************************
 ** @author   STF 470
 ** @version  0.0.1
 ** @purpose  1:22.3.2, Verify that any from getcall is not triggered if there hasn't been any call
 ** @verdict  pass accept, ttcn3verdict:pass
 *****************************************************************/
// The following requirements are tested:
// To getcall on any port from a specific port array,  use the any from PortArrayRef syntax where
// PortArrayRef shall be a reference to a  port array identifier.
// The first port which matches all the criteria will cause the operation to be successful even if
// other ports in the array would also meet the criteria.
module Sem_220302_getcall_operation_006 {
	signature S();

	type port P procedure {
		inout S;
	}

	const integer c_portCount := 4;
    type component GeneralComp
	{
		port P p[c_portCount];
	}

	function f() runs on GeneralComp
	{
        alt
		{
        	[] any from p.getcall { setverdict(fail, "The any from getcall operation produced incorrect match"); }
			[else] { setverdict(pass); }
		}
	}

	testcase TC_Sem_220302_getcall_operation_006() runs on GeneralComp system GeneralComp {
        var GeneralComp v_ptc := GeneralComp.create;
		for(var integer i := 0; i < c_portCount; i := i + 1) {
			connect(self:p[i], v_ptc:p[i]);
		}
		v_ptc.start(f());
		v_ptc.done;
    }

    control {
        execute(TC_Sem_220302_getcall_operation_006(), 5.0);
    }
}