/***************************************************
 ** @author   STF 521
 ** @version  0.0.1
 ** @purpose  1:22.3.3, verify that values that are not addresses or components cannot be used in the to clause of the reply operation
 ** @verdict  pass reject
 ***************************************************/

// The following requirements are tested:
// d) All AddressRef items in the to clause shall be of type address, component or of the address
// type bound to the port type (see clause 6.2.9) of the port instance referenced in the reply
// operation.

module NegSem_220303_ReplyOperation_009 {

    signature S();

    type port P procedure {
        inout S;
    }

    type component GeneralComp {
        port P p;
    }

    function f_server() runs on GeneralComp {
		var integer v_addr := 10;
        p.getcall(S:?);
        p.reply(S:{}) to v_addr;
    }

    testcase TC_NegSem_220303_ReplyOperation_009() runs on GeneralComp system GeneralComp {
        var GeneralComp v_ptc := GeneralComp.create("PTC");
        connect(self:p, v_ptc:p);
        v_ptc.start(f_server());
        p.call(S:{}, nowait);
        alt {
			[] p.getreply {}
			[] v_ptc.done {}
		}
        setverdict(pass);
    }

    control{
        execute(TC_NegSem_220303_ReplyOperation_009(), 5.0);
    }

}
